09:48:27.872085 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:27.872164 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: TC_attach_mnc3-BVCI196(27), component type: BSSGP_Emulation.BSSGP_BVC_CT, component name: TC_attach_mnc3-BVCI196. Version: 11.1.0.
09:48:27.872186 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:27.872227 - Connected to MC.
09:48:27.872243 - Initializing variables, timers and ports of component type BSSGP_Emulation.BSSGP_BVC_CT inside testcase TC_attach_mnc3.
09:48:27.873269 - Port BVC was started.
09:48:27.873298 - Port MGMT was started.
09:48:27.873309 - Port GLOBAL was started.
09:48:27.873318 - Port BSSGP_SP was started.
09:48:27.873327 - Port BSSGP_SP_SIG was started.
09:48:27.873337 - Port BSSGP_PROC was started.
09:48:27.873347 - Component type BSSGP_Emulation.BSSGP_BVC_CT was initialized.
09:48:27.873378 - Port BVC has established the connection with SGSN_Test-Gb0-BSSGP0(25):BVC using transport type UNIX.
09:48:27.873670 - Starting function f_bssgp_bvc_main({ bvci := 196, cell_id := { ra_id := { lai := { mcc_mnc := '023042'H, lac := 13135 }, rac := 0 }, cell_id := 20960 }, depth := BSSGP_DECODE_DEPTH_L3 (3), create_cb := refers(BSSGP_Emulation.DefaultCreateCallback) }, false, 96, "TC_attach_mnc3-BVCI196").
09:48:27.874435 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.874851 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:27.874927 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:27.874941 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.874954 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:27.874965 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:27.875009 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:27.875027 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:27.875046 BSSGP_Emulation.ttcnpp:1319 Message with id 1 was extracted from the queue of BVC.
09:48:27.875066 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.884421 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:27.884477 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:27.884520 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.884636 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:27.884652 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:27.884665 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:27.884678 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:27.884696 BSSGP_Emulation.ttcnpp:1319 Message with id 2 was extracted from the queue of BVC.
09:48:27.884716 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.884765 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:27.884798 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:27.884812 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:27.884842 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC succeeded:  matched
09:48:27.884855 BSSGP_Emulation.ttcnpp:1303 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:27.884867 BSSGP_Emulation.ttcnpp:1303 Message with id 3 was extracted from the queue of BVC.
09:48:27.885655 BSSGP_Emulation.ttcnpp:1044 Sent on BVC to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 0, lsp := 196, sdu := '22048200C40781080888200324334F0051E0'O, bssgp := omit }
09:48:27.885752 BSSGP_Emulation.ttcnpp:1045 Start timer g_T2: 60 s
09:48:27.888160 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:27.888313 BSSGP_Emulation.ttcnpp:1071 Matching on port BVC succeeded:  matched
09:48:27.888333 BSSGP_Emulation.ttcnpp:1071 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:27.888347 BSSGP_Emulation.ttcnpp:1071 Message with id 4 was extracted from the queue of BVC.
09:48:27.888368 BSSGP_Emulation.ttcnpp:1072 Stop timer g_T2: 60 s
09:48:27.888384 BSSGP_Emulation.ttcnpp:1398 BVCI(196) State Transition: BVC_S_BLOCKED (2) -> BVC_S_UNBLOCKED (3)
09:48:29.281082 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP is waiting for connection from TC_attach_mnc3(44):BSSGP[0] on UNIX pathname /tmp/ttcn3-portconn-b87bc546.
09:48:29.284930 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP has accepted the connection from TC_attach_mnc3(44):BSSGP[0].
09:48:29.285410 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG is waiting for connection from TC_attach_mnc3(44):BSSGP_SIG[0] on UNIX pathname /tmp/ttcn3-portconn-b86dc550.
09:48:29.285933 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG has accepted the connection from TC_attach_mnc3(44):BSSGP_SIG[0].
09:48:29.287041 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC is waiting for connection from TC_attach_mnc3(44):BSSGP_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-a83fbd36.
09:48:29.287349 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC has accepted the connection from TC_attach_mnc3(44):BSSGP_PROC[0].
09:48:29.314926 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000001001'H, tlli := 'E91C47EA'O } id 1
09:48:29.315427 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC succeeded: { imsi := '262420000001001'H with ? matched, tlli := 'E91C47EA'O with ? matched }
09:48:29.315665 BSSGP_Emulation.ttcnpp:1333 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_mnc3(44): @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000001001'H, tlli := 'E91C47EA'O } id 1
09:48:29.315766 BSSGP_Emulation.ttcnpp:1333 Operation with id 1 was extracted from the queue of BSSGP_PROC.
09:48:29.315920 BSSGP_Emulation.ttcnpp:851 Adding Client=TC_attach_mnc3(44), IMSI='262420000001001'H, TLLI='E91C47EA'O, index=0
09:48:29.316962 BSSGP_Emulation.ttcnpp:1335 Replied on BSSGP_PROC to TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_register_client : { }
09:48:29.335231 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_mnc3(44) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O } } } id 1
09:48:29.335528 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:29.335588 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_mnc3(44): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O } } } id 1
09:48:29.335645 BSSGP_Emulation.ttcnpp:1218 Message with id 1 was extracted from the queue of BSSGP_SP.
09:48:29.335966 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00EA201C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O, bssgp := omit }
09:48:29.345826 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:29.346782 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:29.347001 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.347333 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:29.347530 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.347723 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:29.347855 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:29.347996 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:29.348081 BSSGP_Emulation.ttcnpp:1154 Message with id 5 was extracted from the queue of BVC.
09:48:29.353184 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_mnc3(44) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:48:29.356347 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_mnc3(44) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000100001CA2F61'O } } } id 2
09:48:29.356884 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:29.357004 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_mnc3(44): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000100001CA2F61'O } } } id 2
09:48:29.357106 BSSGP_Emulation.ttcnpp:1218 Message with id 2 was extracted from the queue of BSSGP_SP.
09:48:29.357350 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9101C0040816084A99990000100001CA2F61'O, bssgp := omit }
09:48:29.370934 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9C41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } } id 6
09:48:29.371220 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:29.371387 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.371535 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:29.371657 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.371759 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:29.371846 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:29.371943 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9C41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } } id 6
09:48:29.372012 BSSGP_Emulation.ttcnpp:1154 Message with id 6 was extracted from the queue of BVC.
09:48:29.375292 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_mnc3(44) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { authenticationAndCipheringRequest := { messageType := '00010010'B, cipheringAlgorithm := { valueField := '000'B, spare := '0'B }, imeisvRequest := { valueField := '001'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, acReferenceNumber := { valueField := '1100'B }, authenticationParameterRAND := { elementIdentifier := '21'O ("!"), randValue := '759DCDD7DDE661B696F07F7FDD0942CB'O }, cipheringKeySequenceNumber := { keySequence := { keySequence := '000'B, spare := '0'B }, elementIdentifier := '1000'B }, authenticationParameterAUTN := omit } } } }
09:48:29.379058 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_mnc3(44) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C00808130C228890578E23094399990000100001F0380BFA'O } } } id 3
09:48:29.379263 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:29.379350 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_mnc3(44): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C00808130C228890578E23094399990000100001F0380BFA'O } } } id 3
09:48:29.379412 BSSGP_Emulation.ttcnpp:1218 Message with id 3 was extracted from the queue of BSSGP_SP.
09:48:29.379600 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9901C00808130C228890578E23094399990000100001F0380BFA'O, bssgp := omit }
09:48:29.386986 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9A01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } } id 7
09:48:29.387249 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:29.387404 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.387562 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:29.387699 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:29.387819 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:29.387919 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:29.388019 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9A01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } } id 7
09:48:29.388096 BSSGP_Emulation.ttcnpp:1154 Message with id 7 was extracted from the queue of BVC.
09:48:29.389613 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_mnc3(44) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'F5ECC758'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:48:29.393453 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E91C47EA'O, tlli := 'F5ECC758'O } id 2
09:48:29.393680 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:48:29.393750 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_unregister_client.
09:48:29.393876 BSSGP_Emulation.ttcnpp:1341 Matching on port BSSGP_PROC succeeded: { tlli_old := 'E91C47EA'O with ? matched, tlli := 'F5ECC758'O with ? matched }
09:48:29.393972 BSSGP_Emulation.ttcnpp:1341 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_mnc3(44): @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E91C47EA'O, tlli := 'F5ECC758'O } id 1
09:48:29.394035 BSSGP_Emulation.ttcnpp:1341 Operation with id 2 was extracted from the queue of BSSGP_PROC.
09:48:29.394232 BSSGP_Emulation.ttcnpp:1343 Replied on BSSGP_PROC to TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_llgmm_assign : { }
09:48:29.395485 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_mnc3(44) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F5ECC758'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:29.395666 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:29.395751 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_mnc3(44): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F5ECC758'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '0'H, mccDigit2 := '2'H, mccDigit3 := '3'H, mncDigit3 := '0'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:29.395817 BSSGP_Emulation.ttcnpp:1218 Message with id 4 was extracted from the queue of BSSGP_SP.
09:48:29.396000 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F5ECC7580050000888200324334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:29.447679 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000001001'H } id 3
09:48:29.448338 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:48:29.448673 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC succeeded: { imsi := '262420000001001'H with ? matched }
09:48:29.449070 BSSGP_Emulation.ttcnpp:1337 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_mnc3(44): @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000001001'H } id 1
09:48:29.449458 BSSGP_Emulation.ttcnpp:1337 Operation with id 3 was extracted from the queue of BSSGP_PROC.
09:48:29.449946 BSSGP_Emulation.ttcnpp:878 Removing Client IMSI='262420000001001'H, index=0
09:48:29.450243 BSSGP_Emulation.ttcnpp:1339 Replied on BSSGP_PROC to TC_attach_mnc3(44) @BSSGP_Emulation.BSSGP_unregister_client : { }
09:48:29.455813 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP to TC_attach_mnc3(44):BSSGP[0] was closed unexpectedly by the peer.
09:48:29.455940 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP was disconnected from TC_attach_mnc3(44):BSSGP[0].
09:48:29.456269 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP_SIG to TC_attach_mnc3(44):BSSGP_SIG[0] was closed unexpectedly by the peer.
09:48:29.456329 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG was disconnected from TC_attach_mnc3(44):BSSGP_SIG[0].
09:48:29.456990 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_PROC to TC_attach_mnc3(44):BSSGP_PROC[0] was closed unexpectedly by the peer.
09:48:29.457143 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC was disconnected from TC_attach_mnc3(44):BSSGP_PROC[0].
09:48:29.462831 BSSGP_Emulation.ttcnpp:1355 Kill was requested from MC.
09:48:29.463163 BSSGP_Emulation.ttcnpp:1355 Terminating test component execution.
09:48:29.465280 - Function f_bssgp_bvc_main was stopped. PTC terminates.
09:48:29.465903 - Terminating component type BSSGP_Emulation.BSSGP_BVC_CT.
09:48:29.466163 - Removing unterminated connection between port BVC and SGSN_Test-Gb0-BSSGP0(25):BVC.
09:48:29.466332 - Port BVC was stopped.
09:48:29.466496 - Port MGMT was stopped.
09:48:29.466708 - Port GLOBAL was stopped.
09:48:29.466808 - Port BSSGP_SP was stopped.
09:48:29.467054 - Port BSSGP_SP_SIG was stopped.
09:48:29.467363 - Port BSSGP_PROC was stopped.
09:48:29.467525 - Component type BSSGP_Emulation.BSSGP_BVC_CT was shut down inside testcase TC_attach_mnc3.
09:48:29.467894 - Final verdict of PTC: none
09:48:29.469497 - Disconnected from MC.
09:48:29.470088 - TTCN-3 Parallel Test Component finished.
