09:48:43.540207 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:43.540440 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: SGSN_Test-Gb0-NS0(87), component type: NS_Emulation.NS_CT, component name: SGSN_Test-Gb0-NS0. Version: 11.1.0.
09:48:43.540500 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:43.540595 - Connected to MC.
09:48:43.540654 - Initializing variables, timers and ports of component type NS_Emulation.NS_CT inside testcase TC_attach_timeout_after_pdp_act.
09:48:43.543747 - Port NS_SP was started.
09:48:43.543806 - Port NSVC was started.
09:48:43.543834 - Port NS_CTRL was started.
09:48:43.543861 - Port NSPIP_PROC was started.
09:48:43.543888 - Component type NS_Emulation.NS_CT was initialized.
09:48:43.546801 - Port NS_SP is waiting for connection from SGSN_Test-Gb0-BSSGP0(88):BSCP on UNIX pathname /tmp/ttcn3-portconn-f47eba4c.
09:48:43.548384 - Port NS_SP has accepted the connection from SGSN_Test-Gb0-BSSGP0(88):BSCP.
09:48:43.549016 - Starting function NSStart({ nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "").
09:48:43.549736 NS_Emulation.ttcnpp:320 Creating NSIP provider for "127.0.0.103":21010
09:48:43.549879 NS_Emulation.ttcnpp:322 Creating new alive PTC with component type NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:43.557075 NS_Emulation.ttcnpp:322 PTC was created. Component reference: 89, alive: yes, type: NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:43.557124 NS_Emulation.ttcnpp:323 Connecting ports SGSN_Test-Gb0-NS0(87):NSPIP_PROC and -NSVCI97-provIP(89):PROC.
09:48:43.557282 NS_Emulation.ttcnpp:323 Port NSPIP_PROC is waiting for connection from -NSVCI97-provIP(89):PROC on UNIX pathname /tmp/ttcn3-portconn-af20aa10.
09:48:43.559118 NS_Emulation.ttcnpp:323 Port NSPIP_PROC has accepted the connection from -NSVCI97-provIP(89):PROC.
09:48:43.559229 NS_Emulation.ttcnpp:323 Connect operation on SGSN_Test-Gb0-NS0(87):NSPIP_PROC and -NSVCI97-provIP(89):PROC finished.
09:48:43.559385 NS_Emulation.ttcnpp:324 Starting function main({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97") on component -NSVCI97-provIP(89).
09:48:43.560139 NS_Emulation.ttcnpp:324 Function was started.
09:48:43.560620 NS_Emulation.ttcnpp:346 Creating new alive PTC with component type NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:43.564201 NS_Emulation.ttcnpp:346 PTC was created. Component reference: 91, alive: yes, type: NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:43.564297 NS_Emulation.ttcnpp:349 Connecting ports SGSN_Test-Gb0-NS0(87):NSVC and -NSVCI97(91):NS_SP.
09:48:43.564533 NS_Emulation.ttcnpp:349 Port NSVC is waiting for connection from -NSVCI97(91):NS_SP on UNIX pathname /tmp/ttcn3-portconn-bb77a61f.
09:48:43.565291 NS_Emulation.ttcnpp:349 Port NSVC has accepted the connection from -NSVCI97(91):NS_SP.
09:48:43.565466 NS_Emulation.ttcnpp:349 Connect operation on SGSN_Test-Gb0-NS0(87):NSVC and -NSVCI97(91):NS_SP finished.
09:48:43.565502 NS_Emulation.ttcnpp:350 Starting NSVC component for { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }
09:48:43.565583 NS_Emulation.ttcnpp:351 Starting function NSVCStart({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97", -NSVCI97-provIP(89)) on component -NSVCI97(91).
09:48:43.565803 NS_Emulation.ttcnpp:351 Function was started.
09:48:43.566381 NS_Provider_IPL4.ttcn:214 Called on NSPIP_PROC to -NSVCI97-provIP(89) @NS_Provider_IPL4.NSPIP_add_nsvc : { remote_ip := "127.0.0.10", remote_port := 23000, vc_nsvc := -NSVCI97(91) }
09:48:43.567525 NS_Provider_IPL4.ttcn:214 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:43.570045 NS_Provider_IPL4.ttcn:214 Reply enqueued on NSPIP_PROC from -NSVCI97-provIP(89) @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:43.570187 NS_Provider_IPL4.ttcn:215 Matching on port NSPIP_PROC succeeded: { } with { } matched value 0 with ? matched
09:48:43.570306 NS_Provider_IPL4.ttcn:215 Getreply operation on port NSPIP_PROC succeeded, reply from -NSVCI97-provIP(89): @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:43.570380 NS_Provider_IPL4.ttcn:215 Operation with id 1 was extracted from the queue of NSPIP_PROC.
09:48:43.571101 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_DEAD_BLOCKED (1) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:43.571227 NS_Emulation.ttcnpp:448 Matching on port NSVC succeeded:  matched
09:48:43.571287 NS_Emulation.ttcnpp:448 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:43.571341 NS_Emulation.ttcnpp:448 Message with id 1 was extracted from the queue of NSVC.
09:48:43.571584 NS_Emulation.ttcnpp:455 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := true }
09:48:43.574509 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:43.574565 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:43.574696 NS_Emulation.ttcnpp:448 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_DEAD_BLOCKED (1) unmatched: First message in the queue does not match the template: 
09:48:43.574769 NS_Emulation.ttcnpp:457 Matching on port NSVC succeeded:  matched
09:48:43.574834 NS_Emulation.ttcnpp:457 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:43.574903 NS_Emulation.ttcnpp:457 Message with id 2 was extracted from the queue of NSVC.
09:48:43.574963 NS_Emulation.ttcnpp:459 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false }
09:48:43.576037 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:43.576115 NS_Emulation.ttcnpp:439 Matching on port NSVC succeeded:  matched
09:48:43.576161 NS_Emulation.ttcnpp:439 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:43.576202 NS_Emulation.ttcnpp:439 Message with id 3 was extracted from the queue of NSVC.
09:48:43.576601 NS_Emulation.ttcnpp:446 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := true }
09:48:43.579352 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:43.579445 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:43.579540 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:43.579558 NS_Emulation.ttcnpp:494 Message with id 1 was extracted from the queue of NS_SP.
09:48:43.579596 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit }
09:48:43.583606 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:43.583783 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.583803 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.583819 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.583834 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.583875 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:43.583895 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:43.583913 NS_Emulation.ttcnpp:474 Message with id 4 was extracted from the queue of NSVC.
09:48:43.583941 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:43.588409 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:48:43.588534 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:43.588582 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:48:43.588593 NS_Emulation.ttcnpp:494 Message with id 2 was extracted from the queue of NS_SP.
09:48:43.588605 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:48:43.589291 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:43.589309 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.589321 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.589331 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.589343 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.589356 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:43.589369 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:43.589385 NS_Emulation.ttcnpp:474 Message with id 5 was extracted from the queue of NSVC.
09:48:43.589427 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:43.986243 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00EA201C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O, bssgp := omit } id 3
09:48:43.986316 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:43.986340 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:43.986359 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00EA201C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O, bssgp := omit } id 3
09:48:43.986376 NS_Emulation.ttcnpp:499 Message with id 3 was extracted from the queue of NS_SP.
09:48:43.986396 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00EA201C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O, bssgp := omit }
09:48:43.989252 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:43.989555 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.989589 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.989613 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.989635 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:43.989673 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:43.989726 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:43.989763 NS_Emulation.ttcnpp:474 Message with id 6 was extracted from the queue of NSVC.
09:48:43.989806 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } }
09:48:44.000773 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9101C0040816084A99990000002001CA2F61'O, bssgp := omit } id 4
09:48:44.000847 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.000897 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.000942 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9101C0040816084A99990000002001CA2F61'O, bssgp := omit } id 4
09:48:44.000984 NS_Emulation.ttcnpp:499 Message with id 4 was extracted from the queue of NS_SP.
09:48:44.001032 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9101C0040816084A99990000002001CA2F61'O, bssgp := omit }
09:48:44.010037 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9C41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } } id 7
09:48:44.010176 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.010234 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.010287 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.010340 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.010413 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.010520 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9C41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } } id 7
09:48:44.010583 NS_Emulation.ttcnpp:474 Message with id 7 was extracted from the queue of NSVC.
09:48:44.010681 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9C41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } }
09:48:44.021270 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9901C008081303222B46941123094399990000002001F0A82DE6'O, bssgp := omit } id 5
09:48:44.021358 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.021426 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.021490 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9901C008081303222B46941123094399990000002001F0A82DE6'O, bssgp := omit } id 5
09:48:44.021549 NS_Emulation.ttcnpp:499 Message with id 5 was extracted from the queue of NS_SP.
09:48:44.021618 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9901C008081303222B46941123094399990000002001F0A82DE6'O, bssgp := omit }
09:48:44.024694 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } } id 8
09:48:44.024864 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.024933 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.024991 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.025047 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.025128 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.025244 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } } id 8
09:48:44.025317 NS_Emulation.ttcnpp:474 Message with id 8 was extracted from the queue of NSVC.
09:48:44.025418 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } }
09:48:44.036046 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:44.036134 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.036202 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.036263 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:44.036323 NS_Emulation.ttcnpp:499 Message with id 6 was extracted from the queue of NS_SP.
09:48:44.036391 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:44.092695 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0100A410503032302000201214A0E54'O, bssgp := omit } id 7
09:48:44.092909 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.093027 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.093127 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0100A410503032302000201214A0E54'O, bssgp := omit } id 7
09:48:44.093227 NS_Emulation.ttcnpp:499 Message with id 7 was extracted from the queue of NS_SP.
09:48:44.093336 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0100A410503032302000201214A0E54'O, bssgp := omit }
09:48:44.127324 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9D01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } } id 9
09:48:44.127581 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.127691 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.127749 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.127801 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.127887 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.128018 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9D01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } } id 9
09:48:44.128095 NS_Emulation.ttcnpp:474 Message with id 9 was extracted from the queue of NSVC.
09:48:44.128202 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9D01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } }
09:48:44.128427 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E80A8200000E8D43FB01001601F41A05DF8C7C4E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } } id 10
09:48:44.128511 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.128566 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.128617 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.128694 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.128755 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.128834 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E80A8200000E8D43FB01001601F41A05DF8C7C4E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } } id 10
09:48:44.128895 NS_Emulation.ttcnpp:474 Message with id 10 was extracted from the queue of NSVC.
09:48:44.128973 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E80A8200000E8D43FB01001601F41A05DF8C7C4E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } }
09:48:44.138999 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9F01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O, bssgp := omit } id 8
09:48:44.139081 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.139144 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.139203 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9F01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O, bssgp := omit } id 8
09:48:44.139256 NS_Emulation.ttcnpp:499 Message with id 8 was extracted from the queue of NS_SP.
09:48:44.139321 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9F01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O, bssgp := omit }
09:48:44.142103 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 11
09:48:44.142181 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.142230 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.142279 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.142330 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.142388 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.142473 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 11
09:48:44.142527 NS_Emulation.ttcnpp:474 Message with id 11 was extracted from the queue of NSVC.
09:48:44.142613 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } }
09:48:44.147666 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0180816084A99990000002001FFDE2B'O, bssgp := omit } id 9
09:48:44.147740 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:44.147797 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:44.147855 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0180816084A99990000002001FFDE2B'O, bssgp := omit } id 9
09:48:44.147909 NS_Emulation.ttcnpp:499 Message with id 9 was extracted from the queue of NS_SP.
09:48:44.147968 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(91) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0180816084A99990000002001FFDE2B'O, bssgp := omit }
09:48:44.153163 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } } id 12
09:48:44.153265 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.153324 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.153381 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.153438 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:44.153548 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:44.153652 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } } id 12
09:48:44.153718 NS_Emulation.ttcnpp:474 Message with id 12 was extracted from the queue of NSVC.
09:48:44.153810 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } }
09:48:50.158430 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } } id 13
09:48:50.158734 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:50.158810 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:50.158870 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:50.158926 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:50.159015 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:50.159126 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } } id 13
09:48:50.159203 NS_Emulation.ttcnpp:474 Message with id 13 was extracted from the queue of NSVC.
09:48:50.159309 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } }
09:48:56.159674 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } } id 14
09:48:56.160181 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:56.160549 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:56.160874 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:56.161177 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:56.161555 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:56.161941 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } } id 14
09:48:56.162159 NS_Emulation.ttcnpp:474 Message with id 14 was extracted from the queue of NSVC.
09:48:56.162361 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } }
09:49:02.160111 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } } id 15
09:49:02.160431 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:02.160549 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:02.160677 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:02.160771 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:02.160903 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:02.161065 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } } id 15
09:49:02.161174 NS_Emulation.ttcnpp:474 Message with id 15 was extracted from the queue of NSVC.
09:49:02.161295 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } }
09:49:08.161812 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(91) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } } id 16
09:49:08.162057 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:08.162186 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:08.162307 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:08.162401 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:08.162531 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:08.162693 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(91): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } } id 16
09:49:08.162767 NS_Emulation.ttcnpp:474 Message with id 16 was extracted from the queue of NSVC.
09:49:08.162873 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } }
09:49:14.682735 NS_Emulation.ttcnpp:420 Kill was requested from MC.
09:49:14.682952 NS_Emulation.ttcnpp:420 Terminating test component execution.
09:49:14.684583 - Function NSStart was stopped. PTC terminates.
09:49:14.684822 - Terminating component type NS_Emulation.NS_CT.
09:49:14.685405 - Removing unterminated connection between port NS_SP and SGSN_Test-Gb0-BSSGP0(88):BSCP.
09:49:14.685752 - Port NS_SP was stopped.
09:49:14.686882 - Removing unterminated connection between port NSVC and -NSVCI97(91):NS_SP.
09:49:14.687274 - Port NSVC was stopped.
09:49:14.687534 - Port NS_CTRL was stopped.
09:49:14.687865 - Removing unterminated connection between port NSPIP_PROC and -NSVCI97-provIP(89):PROC.
09:49:14.688119 - Port NSPIP_PROC was stopped.
09:49:14.689257 - Component type NS_Emulation.NS_CT was shut down inside testcase TC_attach_timeout_after_pdp_act.
09:49:14.689610 - Final verdict of PTC: none
09:49:14.690360 - Disconnected from MC.
09:49:14.690516 - TTCN-3 Parallel Test Component finished.
