09:50:12.701672 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:50:12.701810 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: TC_attach_gsup_lu_timeout-BVCI196(174), component type: BSSGP_Emulation.BSSGP_BVC_CT, component name: TC_attach_gsup_lu_timeout-BVCI196. Version: 11.1.0.
09:50:12.701850 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:50:12.701927 - Connected to MC.
09:50:12.701954 - Initializing variables, timers and ports of component type BSSGP_Emulation.BSSGP_BVC_CT inside testcase TC_attach_gsup_lu_timeout.
09:50:12.703659 - Port BVC was started.
09:50:12.703693 - Port MGMT was started.
09:50:12.703710 - Port GLOBAL was started.
09:50:12.703726 - Port BSSGP_SP was started.
09:50:12.703742 - Port BSSGP_SP_SIG was started.
09:50:12.703758 - Port BSSGP_PROC was started.
09:50:12.703773 - Component type BSSGP_Emulation.BSSGP_BVC_CT was initialized.
09:50:12.703824 - Port BVC has established the connection with SGSN_Test-Gb0-BSSGP0(172):BVC using transport type UNIX.
09:50:12.704307 - Starting function f_bssgp_bvc_main({ bvci := 196, cell_id := { ra_id := { lai := { mcc_mnc := '262F42'H, lac := 13135 }, rac := 0 }, cell_id := 20960 }, depth := BSSGP_DECODE_DEPTH_L3 (3), create_cb := refers(BSSGP_Emulation.DefaultCreateCallback) }, false, 96, "TC_attach_gsup_lu_timeout-BVCI196").
09:50:12.705566 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.706239 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:50:12.706367 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:50:12.706393 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.706412 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:50:12.706429 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:50:12.706486 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:50:12.706517 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:50:12.706547 BSSGP_Emulation.ttcnpp:1319 Message with id 1 was extracted from the queue of BVC.
09:50:12.706572 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.717131 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:50:12.717175 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:50:12.717192 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.717205 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:50:12.717215 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:50:12.717225 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:50:12.717236 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:50:12.717250 BSSGP_Emulation.ttcnpp:1319 Message with id 2 was extracted from the queue of BVC.
09:50:12.717264 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.717308 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:50:12.717340 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:50:12.717351 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:50:12.717395 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC succeeded:  matched
09:50:12.717439 BSSGP_Emulation.ttcnpp:1303 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:50:12.717451 BSSGP_Emulation.ttcnpp:1303 Message with id 3 was extracted from the queue of BVC.
09:50:12.718229 BSSGP_Emulation.ttcnpp:1044 Sent on BVC to SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 0, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:50:12.718328 BSSGP_Emulation.ttcnpp:1045 Start timer g_T2: 60 s
09:50:12.719971 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:50:12.720128 BSSGP_Emulation.ttcnpp:1071 Matching on port BVC succeeded:  matched
09:50:12.720143 BSSGP_Emulation.ttcnpp:1071 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:50:12.720155 BSSGP_Emulation.ttcnpp:1071 Message with id 4 was extracted from the queue of BVC.
09:50:12.720173 BSSGP_Emulation.ttcnpp:1072 Stop timer g_T2: 60 s
09:50:12.720186 BSSGP_Emulation.ttcnpp:1398 BVCI(196) State Transition: BVC_S_BLOCKED (2) -> BVC_S_UNBLOCKED (3)
09:50:14.091983 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP is waiting for connection from TC_attach_gsup_lu_timeout(191):BSSGP[0] on UNIX pathname /tmp/ttcn3-portconn-7575c5f3.
09:50:14.095595 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP has accepted the connection from TC_attach_gsup_lu_timeout(191):BSSGP[0].
09:50:14.095919 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG is waiting for connection from TC_attach_gsup_lu_timeout(191):BSSGP_SIG[0] on UNIX pathname /tmp/ttcn3-portconn-7563c5e5.
09:50:14.096233 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG has accepted the connection from TC_attach_gsup_lu_timeout(191):BSSGP_SIG[0].
09:50:14.097161 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC is waiting for connection from TC_attach_gsup_lu_timeout(191):BSSGP_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-6531bd83.
09:50:14.097426 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC has accepted the connection from TC_attach_gsup_lu_timeout(191):BSSGP_PROC[0].
09:50:14.122014 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_gsup_lu_timeout(191) @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000005'H, tlli := 'E0BE5591'O } id 1
09:50:14.122615 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000005'H with ? matched, tlli := 'E0BE5591'O with ? matched }
09:50:14.122854 BSSGP_Emulation.ttcnpp:1333 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_gsup_lu_timeout(191): @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000005'H, tlli := 'E0BE5591'O } id 1
09:50:14.122965 BSSGP_Emulation.ttcnpp:1333 Operation with id 1 was extracted from the queue of BSSGP_PROC.
09:50:14.123094 BSSGP_Emulation.ttcnpp:851 Adding Client=TC_attach_gsup_lu_timeout(191), IMSI='262420000000005'H, TLLI='E0BE5591'O, index=0
09:50:14.124164 BSSGP_Emulation.ttcnpp:1335 Replied on BSSGP_PROC to TC_attach_gsup_lu_timeout(191) @BSSGP_Emulation.BSSGP_register_client : { }
09:50:14.141483 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_gsup_lu_timeout(191) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000005062F2247930ED0512C7422000E218F2'O } } } id 1
09:50:14.141811 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:50:14.141865 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_gsup_lu_timeout(191): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000005062F2247930ED0512C7422000E218F2'O } } } id 1
09:50:14.141907 BSSGP_Emulation.ttcnpp:1218 Message with id 1 was extracted from the queue of BSSGP_SP.
09:50:14.142288 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E0BE5591005000088862F224334F0051E00EA201C000080101D571000008292624000000005062F2247930ED0512C7422000E218F2'O, bssgp := omit }
09:50:14.151605 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:50:14.152458 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:50:14.152663 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.152925 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:50:14.153074 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.153249 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:50:14.153349 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:50:14.153442 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:50:14.153516 BSSGP_Emulation.ttcnpp:1154 Message with id 5 was extracted from the queue of BVC.
09:50:14.158690 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_gsup_lu_timeout(191) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:50:14.161764 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_gsup_lu_timeout(191) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000000005CA2F61'O } } } id 2
09:50:14.161937 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:50:14.162014 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_gsup_lu_timeout(191): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000000005CA2F61'O } } } id 2
09:50:14.162076 BSSGP_Emulation.ttcnpp:1218 Message with id 2 was extracted from the queue of BSSGP_SP.
09:50:14.162267 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E0BE5591005000088862F224334F0051E00E9101C0040816084A99990000000005CA2F61'O, bssgp := omit }
09:50:14.175852 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E9C41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } } id 6
09:50:14.176030 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:50:14.176168 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.176311 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:50:14.176422 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.176536 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:50:14.176616 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:50:14.176737 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E9C41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210F021EC22A6215135A6B466325247DB2712C580875B05'O }, initialLLC_PDU := omit } } } id 6
09:50:14.176801 BSSGP_Emulation.ttcnpp:1154 Message with id 6 was extracted from the queue of BVC.
09:50:14.179991 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_gsup_lu_timeout(191) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { authenticationAndCipheringRequest := { messageType := '00010010'B, cipheringAlgorithm := { valueField := '000'B, spare := '0'B }, imeisvRequest := { valueField := '001'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, acReferenceNumber := { valueField := '1111'B }, authenticationParameterRAND := { elementIdentifier := '21'O ("!"), randValue := 'EC22A6215135A6B466325247DB2712C5'O }, cipheringKeySequenceNumber := { keySequence := { keySequence := '000'B, spare := '0'B }, elementIdentifier := '1000'B }, authenticationParameterAUTN := omit } } } }
09:50:14.183885 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_gsup_lu_timeout(191) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C00808130F22364BF07E23094399990000000005F0E8AAFC'O } } } id 3
09:50:14.184087 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:50:14.184176 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_gsup_lu_timeout(191): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C00808130F22364BF07E23094399990000000005F0E8AAFC'O } } } id 3
09:50:14.184240 BSSGP_Emulation.ttcnpp:1218 Message with id 3 was extracted from the queue of BSSGP_SP.
09:50:14.184427 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E0BE5591005000088862F224334F0051E00E9901C00808130F22364BF07E23094399990000000005F0E8AAFC'O, bssgp := omit }
09:50:14.191290 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(172) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E9A01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } } id 7
09:50:14.191470 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:50:14.191600 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.191736 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:50:14.191855 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:50:14.191950 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:50:14.192028 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:50:14.192118 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(172): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E0BE5591000020168203E8138512C74220000A8200000D8829262400000000500E9A01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E0BE5591'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000005'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F2EC956F92A679'O }, initialLLC_PDU := omit } } } id 7
09:50:14.192185 BSSGP_Emulation.ttcnpp:1154 Message with id 7 was extracted from the queue of BVC.
09:50:14.193710 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_gsup_lu_timeout(191) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'F2EC956F'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:50:14.197739 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_gsup_lu_timeout(191) @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E0BE5591'O, tlli := 'F2EC956F'O } id 2
09:50:14.197953 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:50:14.198017 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_unregister_client.
09:50:14.198139 BSSGP_Emulation.ttcnpp:1341 Matching on port BSSGP_PROC succeeded: { tlli_old := 'E0BE5591'O with ? matched, tlli := 'F2EC956F'O with ? matched }
09:50:14.198237 BSSGP_Emulation.ttcnpp:1341 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_gsup_lu_timeout(191): @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E0BE5591'O, tlli := 'F2EC956F'O } id 1
09:50:14.198298 BSSGP_Emulation.ttcnpp:1341 Operation with id 2 was extracted from the queue of BSSGP_PROC.
09:50:14.198497 BSSGP_Emulation.ttcnpp:1343 Replied on BSSGP_PROC to TC_attach_gsup_lu_timeout(191) @BSSGP_Emulation.BSSGP_llgmm_assign : { }
09:50:14.199494 BSSGP_Emulation.ttcnpp:1355 Kill was requested from MC.
09:50:14.199782 BSSGP_Emulation.ttcnpp:1355 Terminating test component execution.
09:50:14.202046 - Function f_bssgp_bvc_main was stopped. PTC terminates.
09:50:14.202424 - Terminating component type BSSGP_Emulation.BSSGP_BVC_CT.
09:50:14.202534 - Removing unterminated connection between port BVC and SGSN_Test-Gb0-BSSGP0(172):BVC.
09:50:14.202811 - Port BVC was stopped.
09:50:14.202955 - Port MGMT was stopped.
09:50:14.203113 - Port GLOBAL was stopped.
09:50:14.204265 - Removing unterminated connection between port BSSGP_SP and TC_attach_gsup_lu_timeout(191):BSSGP[0].
09:50:14.204699 - Port BSSGP_SP was stopped.
09:50:14.205815 - Removing unterminated connection between port BSSGP_SP_SIG and TC_attach_gsup_lu_timeout(191):BSSGP_SIG[0].
09:50:14.206213 - Port BSSGP_SP_SIG was stopped.
09:50:14.207084 - Removing unterminated connection between port BSSGP_PROC and TC_attach_gsup_lu_timeout(191):BSSGP_PROC[0].
09:50:14.207920 - Port BSSGP_PROC was stopped.
09:50:14.208162 - Component type BSSGP_Emulation.BSSGP_BVC_CT was shut down inside testcase TC_attach_gsup_lu_timeout.
09:50:14.208322 - Final verdict of PTC: none
09:50:14.208912 - Disconnected from MC.
09:50:14.209688 - TTCN-3 Parallel Test Component finished.
