09:49:18.346314 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:49:18.346657 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: SGSN_Test-Gb0-NS0(108), component type: NS_Emulation.NS_CT, component name: SGSN_Test-Gb0-NS0. Version: 11.1.0.
09:49:18.346799 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:49:18.346988 - Connected to MC.
09:49:18.347096 - Initializing variables, timers and ports of component type NS_Emulation.NS_CT inside testcase TC_attach_auth_id_timeout.
09:49:18.351524 - Port NS_SP was started.
09:49:18.351676 - Port NSVC was started.
09:49:18.351762 - Port NS_CTRL was started.
09:49:18.351776 - Port NSPIP_PROC was started.
09:49:18.351785 - Component type NS_Emulation.NS_CT was initialized.
09:49:18.353579 - Port NS_SP is waiting for connection from SGSN_Test-Gb0-BSSGP0(109):BSCP on UNIX pathname /tmp/ttcn3-portconn-a47eba77.
09:49:18.356678 - Port NS_SP has accepted the connection from SGSN_Test-Gb0-BSSGP0(109):BSCP.
09:49:18.357646 - Starting function NSStart({ nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "").
09:49:18.358966 NS_Emulation.ttcnpp:320 Creating NSIP provider for "127.0.0.103":21010
09:49:18.359186 NS_Emulation.ttcnpp:322 Creating new alive PTC with component type NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:49:18.367289 NS_Emulation.ttcnpp:322 PTC was created. Component reference: 110, alive: yes, type: NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:49:18.367402 NS_Emulation.ttcnpp:323 Connecting ports SGSN_Test-Gb0-NS0(108):NSPIP_PROC and -NSVCI97-provIP(110):PROC.
09:49:18.367638 NS_Emulation.ttcnpp:323 Port NSPIP_PROC is waiting for connection from -NSVCI97-provIP(110):PROC on UNIX pathname /tmp/ttcn3-portconn-fd20aa2b.
09:49:18.369750 NS_Emulation.ttcnpp:323 Port NSPIP_PROC has accepted the connection from -NSVCI97-provIP(110):PROC.
09:49:18.369776 NS_Emulation.ttcnpp:323 Connect operation on SGSN_Test-Gb0-NS0(108):NSPIP_PROC and -NSVCI97-provIP(110):PROC finished.
09:49:18.369827 NS_Emulation.ttcnpp:324 Starting function main({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97") on component -NSVCI97-provIP(110).
09:49:18.370109 NS_Emulation.ttcnpp:324 Function was started.
09:49:18.370318 NS_Emulation.ttcnpp:346 Creating new alive PTC with component type NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:49:18.373440 NS_Emulation.ttcnpp:346 PTC was created. Component reference: 112, alive: yes, type: NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:49:18.373478 NS_Emulation.ttcnpp:349 Connecting ports SGSN_Test-Gb0-NS0(108):NSVC and -NSVCI97(112):NS_SP.
09:49:18.373688 NS_Emulation.ttcnpp:349 Port NSVC is waiting for connection from -NSVCI97(112):NS_SP on UNIX pathname /tmp/ttcn3-portconn-f577a624.
09:49:18.374510 NS_Emulation.ttcnpp:349 Port NSVC has accepted the connection from -NSVCI97(112):NS_SP.
09:49:18.374529 NS_Emulation.ttcnpp:349 Connect operation on SGSN_Test-Gb0-NS0(108):NSVC and -NSVCI97(112):NS_SP finished.
09:49:18.374546 NS_Emulation.ttcnpp:350 Starting NSVC component for { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }
09:49:18.374579 NS_Emulation.ttcnpp:351 Starting function NSVCStart({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97", -NSVCI97-provIP(110)) on component -NSVCI97(112).
09:49:18.374759 NS_Emulation.ttcnpp:351 Function was started.
09:49:18.375009 NS_Provider_IPL4.ttcn:214 Called on NSPIP_PROC to -NSVCI97-provIP(110) @NS_Provider_IPL4.NSPIP_add_nsvc : { remote_ip := "127.0.0.10", remote_port := 23000, vc_nsvc := -NSVCI97(112) }
09:49:18.375731 NS_Provider_IPL4.ttcn:214 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:49:18.377290 NS_Provider_IPL4.ttcn:214 Reply enqueued on NSPIP_PROC from -NSVCI97-provIP(110) @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:49:18.377332 NS_Provider_IPL4.ttcn:215 Matching on port NSPIP_PROC succeeded: { } with { } matched value 0 with ? matched
09:49:18.377364 NS_Provider_IPL4.ttcn:215 Getreply operation on port NSPIP_PROC succeeded, reply from -NSVCI97-provIP(110): @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:49:18.377384 NS_Provider_IPL4.ttcn:215 Operation with id 1 was extracted from the queue of NSPIP_PROC.
09:49:18.377610 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_DEAD_BLOCKED (1) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:49:18.377654 NS_Emulation.ttcnpp:448 Matching on port NSVC succeeded:  matched
09:49:18.377672 NS_Emulation.ttcnpp:448 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:49:18.377689 NS_Emulation.ttcnpp:448 Message with id 1 was extracted from the queue of NSVC.
09:49:18.377774 NS_Emulation.ttcnpp:455 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := true }
09:49:18.380772 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:49:18.380793 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:49:18.380807 NS_Emulation.ttcnpp:448 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_DEAD_BLOCKED (1) unmatched: First message in the queue does not match the template: 
09:49:18.380820 NS_Emulation.ttcnpp:457 Matching on port NSVC succeeded:  matched
09:49:18.380834 NS_Emulation.ttcnpp:457 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:49:18.380905 NS_Emulation.ttcnpp:457 Message with id 2 was extracted from the queue of NSVC.
09:49:18.380992 NS_Emulation.ttcnpp:459 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false }
09:49:18.382499 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:49:18.382523 NS_Emulation.ttcnpp:439 Matching on port NSVC succeeded:  matched
09:49:18.382538 NS_Emulation.ttcnpp:439 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:49:18.382559 NS_Emulation.ttcnpp:439 Message with id 3 was extracted from the queue of NSVC.
09:49:18.382683 NS_Emulation.ttcnpp:446 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := true }
09:49:18.383657 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:49:18.383769 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:49:18.383906 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:49:18.383926 NS_Emulation.ttcnpp:494 Message with id 1 was extracted from the queue of NS_SP.
09:49:18.383969 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(112) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit }
09:49:18.387408 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:49:18.387902 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.387952 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.387988 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.388021 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.388128 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:18.388176 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:49:18.388218 NS_Emulation.ttcnpp:474 Message with id 4 was extracted from the queue of NSVC.
09:49:18.388300 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:49:18.391654 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:49:18.391684 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:49:18.391703 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:49:18.391723 NS_Emulation.ttcnpp:494 Message with id 2 was extracted from the queue of NS_SP.
09:49:18.391743 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(112) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:49:18.392734 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:49:18.392760 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.392778 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.392796 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.392814 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.392838 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:18.392856 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:49:18.392877 NS_Emulation.ttcnpp:474 Message with id 5 was extracted from the queue of NSVC.
09:49:18.392896 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:49:18.768854 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E659D156005000088862F224334F0051E00E9F01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O, bssgp := omit } id 3
09:49:18.768945 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:49:18.768981 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:49:18.769009 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E659D156005000088862F224334F0051E00E9F01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O, bssgp := omit } id 3
09:49:18.769033 NS_Emulation.ttcnpp:499 Message with id 3 was extracted from the queue of NS_SP.
09:49:18.769062 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(112) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E659D156005000088862F224334F0051E00E9F01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O, bssgp := omit }
09:49:18.772680 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:49:18.772817 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.772832 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.772842 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.772852 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:18.772868 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:18.772888 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:49:18.772903 NS_Emulation.ttcnpp:474 Message with id 6 was extracted from the queue of NSVC.
09:49:18.772920 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } }
09:49:24.776420 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C005081502E63132'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } } id 7
09:49:24.776870 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:24.776995 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:24.777089 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:24.777177 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:24.777302 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:24.777448 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C005081502E63132'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } } id 7
09:49:24.777529 NS_Emulation.ttcnpp:474 Message with id 7 was extracted from the queue of NSVC.
09:49:24.777630 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C005081502E63132'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } }
09:49:30.779223 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00908150215FB90'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } } id 8
09:49:30.779484 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:30.779607 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:30.779704 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:30.779796 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:30.779923 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:30.780074 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00908150215FB90'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } } id 8
09:49:30.780202 NS_Emulation.ttcnpp:474 Message with id 8 was extracted from the queue of NSVC.
09:49:30.780306 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00908150215FB90'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } }
09:49:36.780732 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00D0815022D4438'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } } id 9
09:49:36.781012 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:36.781371 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:36.781487 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:36.781579 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:36.781747 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:36.781918 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00D0815022D4438'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } } id 9
09:49:36.782068 NS_Emulation.ttcnpp:474 Message with id 9 was extracted from the queue of NSVC.
09:49:36.782215 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00D0815022D4438'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } }
09:49:42.782577 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 10
09:49:42.782838 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:42.782918 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:42.783024 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:42.783121 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:42.783249 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:42.783401 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 10
09:49:42.783526 NS_Emulation.ttcnpp:474 Message with id 10 was extracted from the queue of NSVC.
09:49:42.783636 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } }
09:49:48.784989 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(112) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E80A8200000E8901C015080409E916B3'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } } id 11
09:49:48.785325 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:48.785437 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:48.785528 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:48.785617 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:49:48.785740 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:49:48.785868 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(112): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E80A8200000E8901C015080409E916B3'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } } id 11
09:49:48.785945 NS_Emulation.ttcnpp:474 Message with id 11 was extracted from the queue of NSVC.
09:49:48.786032 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E80A8200000E8901C015080409E916B3'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } }
09:49:48.800319 NS_Emulation.ttcnpp:420 Kill was requested from MC.
09:49:48.800538 NS_Emulation.ttcnpp:420 Terminating test component execution.
09:49:48.801953 - Function NSStart was stopped. PTC terminates.
09:49:48.802124 - Terminating component type NS_Emulation.NS_CT.
09:49:48.802234 - Removing unterminated connection between port NS_SP and SGSN_Test-Gb0-BSSGP0(109):BSCP.
09:49:48.802433 - Port NS_SP was stopped.
09:49:48.802664 - Removing unterminated connection between port NSVC and -NSVCI97(112):NS_SP.
09:49:48.802957 - Port NSVC was stopped.
09:49:48.803224 - Port NS_CTRL was stopped.
09:49:48.803487 - Removing unterminated connection between port NSPIP_PROC and -NSVCI97-provIP(110):PROC.
09:49:48.803767 - Port NSPIP_PROC was stopped.
09:49:48.804019 - Component type NS_Emulation.NS_CT was shut down inside testcase TC_attach_auth_id_timeout.
09:49:48.804161 - Final verdict of PTC: none
09:49:48.804768 - Disconnected from MC.
09:49:48.804992 - TTCN-3 Parallel Test Component finished.
