09:49:18.370706 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:49:18.370861 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: TC_attach_auth_id_timeout-BVCI196(111), component type: BSSGP_Emulation.BSSGP_BVC_CT, component name: TC_attach_auth_id_timeout-BVCI196. Version: 11.1.0.
09:49:18.370895 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:49:18.370957 - Connected to MC.
09:49:18.371077 - Initializing variables, timers and ports of component type BSSGP_Emulation.BSSGP_BVC_CT inside testcase TC_attach_auth_id_timeout.
09:49:18.372460 - Port BVC was started.
09:49:18.372536 - Port MGMT was started.
09:49:18.372553 - Port GLOBAL was started.
09:49:18.372568 - Port BSSGP_SP was started.
09:49:18.372582 - Port BSSGP_SP_SIG was started.
09:49:18.372597 - Port BSSGP_PROC was started.
09:49:18.372611 - Component type BSSGP_Emulation.BSSGP_BVC_CT was initialized.
09:49:18.372666 - Port BVC has established the connection with SGSN_Test-Gb0-BSSGP0(109):BVC using transport type UNIX.
09:49:18.373069 - Starting function f_bssgp_bvc_main({ bvci := 196, cell_id := { ra_id := { lai := { mcc_mnc := '262F42'H, lac := 13135 }, rac := 0 }, cell_id := 20960 }, depth := BSSGP_DECODE_DEPTH_L3 (3), create_cb := refers(BSSGP_Emulation.DefaultCreateCallback) }, false, 96, "TC_attach_auth_id_timeout-BVCI196").
09:49:18.373991 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.374510 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:49:18.374615 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:49:18.374638 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.374660 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:49:18.374673 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:49:18.374721 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:49:18.374746 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:49:18.374781 BSSGP_Emulation.ttcnpp:1319 Message with id 1 was extracted from the queue of BVC.
09:49:18.374807 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.389642 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:49:18.389710 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:49:18.389736 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.389760 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:49:18.389780 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:49:18.389800 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:49:18.389820 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:49:18.389847 BSSGP_Emulation.ttcnpp:1319 Message with id 2 was extracted from the queue of BVC.
09:49:18.389873 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.389949 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:49:18.389998 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:49:18.390040 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:49:18.390111 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC succeeded:  matched
09:49:18.390143 BSSGP_Emulation.ttcnpp:1303 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:49:18.390169 BSSGP_Emulation.ttcnpp:1303 Message with id 3 was extracted from the queue of BVC.
09:49:18.391229 BSSGP_Emulation.ttcnpp:1044 Sent on BVC to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 0, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:49:18.391354 BSSGP_Emulation.ttcnpp:1045 Start timer g_T2: 60 s
09:49:18.393767 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:49:18.393960 BSSGP_Emulation.ttcnpp:1071 Matching on port BVC succeeded:  matched
09:49:18.393985 BSSGP_Emulation.ttcnpp:1071 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:49:18.394004 BSSGP_Emulation.ttcnpp:1071 Message with id 4 was extracted from the queue of BVC.
09:49:18.394030 BSSGP_Emulation.ttcnpp:1072 Stop timer g_T2: 60 s
09:49:18.394053 BSSGP_Emulation.ttcnpp:1398 BVCI(196) State Transition: BVC_S_BLOCKED (2) -> BVC_S_UNBLOCKED (3)
09:49:18.728463 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP is waiting for connection from TC_attach_auth_id_timeout(128):BSSGP[0] on UNIX pathname /tmp/ttcn3-portconn-5a7ac532.
09:49:18.730745 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP has accepted the connection from TC_attach_auth_id_timeout(128):BSSGP[0].
09:49:18.731162 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG is waiting for connection from TC_attach_auth_id_timeout(128):BSSGP_SIG[0] on UNIX pathname /tmp/ttcn3-portconn-5a6cc524.
09:49:18.731323 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG has accepted the connection from TC_attach_auth_id_timeout(128):BSSGP_SIG[0].
09:49:18.731734 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC is waiting for connection from TC_attach_auth_id_timeout(128):BSSGP_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-4a3ebd42.
09:49:18.731910 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC has accepted the connection from TC_attach_auth_id_timeout(128):BSSGP_PROC[0].
09:49:18.748465 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_auth_id_timeout(128) @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000002'H, tlli := 'E659D156'O } id 1
09:49:18.749016 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000002'H with ? matched, tlli := 'E659D156'O with ? matched }
09:49:18.749238 BSSGP_Emulation.ttcnpp:1333 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_auth_id_timeout(128): @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000002'H, tlli := 'E659D156'O } id 1
09:49:18.749348 BSSGP_Emulation.ttcnpp:1333 Operation with id 1 was extracted from the queue of BSSGP_PROC.
09:49:18.749476 BSSGP_Emulation.ttcnpp:851 Adding Client=TC_attach_auth_id_timeout(128), IMSI='262420000000002'H, TLLI='E659D156'O, index=0
09:49:18.750450 BSSGP_Emulation.ttcnpp:1335 Replied on BSSGP_PROC to TC_attach_auth_id_timeout(128) @BSSGP_Emulation.BSSGP_register_client : { }
09:49:18.767836 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_auth_id_timeout(128) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 31 }, lLC_PDU := '01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O } } } id 1
09:49:18.768096 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:49:18.768138 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_auth_id_timeout(128): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 31 }, lLC_PDU := '01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O } } } id 1
09:49:18.768175 BSSGP_Emulation.ttcnpp:1218 Message with id 1 was extracted from the queue of BSSGP_SP.
09:49:18.768520 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E659D156005000088862F224334F0051E00E9F01C000080101D571000005F4C000004A62F22474F67D0512C7422000E218F2'O, bssgp := omit }
09:49:18.773742 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:49:18.773931 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:18.773964 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:18.774017 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:18.774046 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:18.774077 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:18.774098 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:18.774116 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:49:18.774130 BSSGP_Emulation.ttcnpp:1154 Message with id 5 was extracted from the queue of BVC.
09:49:18.775715 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:49:24.779923 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C005081502E63132'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } } id 6
09:49:24.780354 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:24.780525 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:24.780701 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:24.780913 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:24.781125 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:24.781292 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:24.781475 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C005081502E63132'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C005081502E63132'O }, initialLLC_PDU := omit } } } id 6
09:49:24.781637 BSSGP_Emulation.ttcnpp:1154 Message with id 6 was extracted from the queue of BVC.
09:49:24.781940 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:49:30.783364 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00908150215FB90'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } } id 7
09:49:30.783848 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:30.784100 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:30.784354 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:30.784581 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:30.784776 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:30.784962 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:30.785152 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00908150215FB90'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00908150215FB90'O }, initialLLC_PDU := omit } } } id 7
09:49:30.785320 BSSGP_Emulation.ttcnpp:1154 Message with id 7 was extracted from the queue of BVC.
09:49:30.785624 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:49:36.784439 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00D0815022D4438'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } } id 8
09:49:36.784889 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:36.785166 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:36.785424 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:36.785663 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:36.785877 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:36.786057 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:36.786150 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C00D0815022D4438'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C00D0815022D4438'O }, initialLLC_PDU := omit } } } id 8
09:49:36.786226 BSSGP_Emulation.ttcnpp:1154 Message with id 8 was extracted from the queue of BVC.
09:49:36.786524 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:49:42.786093 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 9
09:49:42.786462 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:42.786626 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:42.786838 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:42.787024 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:42.787174 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:42.787305 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:42.787440 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E8138512C74220000A8200000E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 9
09:49:42.787514 BSSGP_Emulation.ttcnpp:1154 Message with id 9 was extracted from the queue of BVC.
09:49:42.787819 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:49:48.788416 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(109) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E80A8200000E8901C015080409E916B3'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } } id 10
09:49:48.788783 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:48.788978 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:48.789189 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:48.789352 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:48.789486 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:48.789615 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:48.789702 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(109): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E659D156000020168203E80A8200000E8901C015080409E916B3'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E659D156'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '01C015080409E916B3'O }, initialLLC_PDU := omit } } } id 10
09:49:48.789776 BSSGP_Emulation.ttcnpp:1154 Message with id 10 was extracted from the queue of BVC.
09:49:48.790313 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_auth_id_timeout(128) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachReject := { messageType := '00000100'B, gmmCause := { causeValue := '09'O ("\t") }, t3302 := omit, t3346 := omit } } } }
09:49:48.792401 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_auth_id_timeout(128) @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000002'H } id 2
09:49:48.792610 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:49:48.792786 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000002'H with ? matched }
09:49:48.792971 BSSGP_Emulation.ttcnpp:1337 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_auth_id_timeout(128): @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000002'H } id 1
09:49:48.793159 BSSGP_Emulation.ttcnpp:1337 Operation with id 2 was extracted from the queue of BSSGP_PROC.
09:49:48.793361 BSSGP_Emulation.ttcnpp:878 Removing Client IMSI='262420000000002'H, index=0
09:49:48.793628 BSSGP_Emulation.ttcnpp:1339 Replied on BSSGP_PROC to TC_attach_auth_id_timeout(128) @BSSGP_Emulation.BSSGP_unregister_client : { }
09:49:48.795552 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP to TC_attach_auth_id_timeout(128):BSSGP[0] was closed unexpectedly by the peer.
09:49:48.795625 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP was disconnected from TC_attach_auth_id_timeout(128):BSSGP[0].
09:49:48.795888 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP_SIG to TC_attach_auth_id_timeout(128):BSSGP_SIG[0] was closed unexpectedly by the peer.
09:49:48.795937 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG was disconnected from TC_attach_auth_id_timeout(128):BSSGP_SIG[0].
09:49:48.796810 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_PROC to TC_attach_auth_id_timeout(128):BSSGP_PROC[0] was closed unexpectedly by the peer.
09:49:48.796865 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC was disconnected from TC_attach_auth_id_timeout(128):BSSGP_PROC[0].
09:49:48.800346 BSSGP_Emulation.ttcnpp:1355 Kill was requested from MC.
09:49:48.800545 BSSGP_Emulation.ttcnpp:1355 Terminating test component execution.
09:49:48.802190 - Function f_bssgp_bvc_main was stopped. PTC terminates.
09:49:48.802394 - Terminating component type BSSGP_Emulation.BSSGP_BVC_CT.
09:49:48.802701 - Removing unterminated connection between port BVC and SGSN_Test-Gb0-BSSGP0(109):BVC.
09:49:48.802811 - Port BVC was stopped.
09:49:48.802937 - Port MGMT was stopped.
09:49:48.803139 - Port GLOBAL was stopped.
09:49:48.803300 - Port BSSGP_SP was stopped.
09:49:48.803370 - Port BSSGP_SP_SIG was stopped.
09:49:48.803453 - Port BSSGP_PROC was stopped.
09:49:48.803630 - Component type BSSGP_Emulation.BSSGP_BVC_CT was shut down inside testcase TC_attach_auth_id_timeout.
09:49:48.803891 - Final verdict of PTC: none
09:49:48.804472 - Disconnected from MC.
09:49:48.804848 - TTCN-3 Parallel Test Component finished.
