09:50:17.848942 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:50:17.849024 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: SGSN_Test-Gb0-NS0(192), component type: NS_Emulation.NS_CT, component name: SGSN_Test-Gb0-NS0. Version: 11.1.0.
09:50:17.849051 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:50:17.849090 - Connected to MC.
09:50:17.849112 - Initializing variables, timers and ports of component type NS_Emulation.NS_CT inside testcase TC_attach_gsup_lu_reject.
09:50:17.852257 - Port NS_SP was started.
09:50:17.852351 - Port NSVC was started.
09:50:17.852401 - Port NS_CTRL was started.
09:50:17.852449 - Port NSPIP_PROC was started.
09:50:17.852496 - Component type NS_Emulation.NS_CT was initialized.
09:50:17.855549 - Port NS_SP is waiting for connection from SGSN_Test-Gb0-BSSGP0(193):BSCP on UNIX pathname /tmp/ttcn3-portconn-d671badb.
09:50:17.857697 - Port NS_SP has accepted the connection from SGSN_Test-Gb0-BSSGP0(193):BSCP.
09:50:17.858734 - Starting function NSStart({ nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "").
09:50:17.859966 NS_Emulation.ttcnpp:320 Creating NSIP provider for "127.0.0.103":21010
09:50:17.860206 NS_Emulation.ttcnpp:322 Creating new alive PTC with component type NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:50:17.867230 NS_Emulation.ttcnpp:322 PTC was created. Component reference: 194, alive: yes, type: NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:50:17.867285 NS_Emulation.ttcnpp:323 Connecting ports SGSN_Test-Gb0-NS0(192):NSPIP_PROC and -NSVCI97-provIP(194):PROC.
09:50:17.867432 NS_Emulation.ttcnpp:323 Port NSPIP_PROC is waiting for connection from -NSVCI97-provIP(194):PROC on UNIX pathname /tmp/ttcn3-portconn-8f2faa87.
09:50:17.868260 NS_Emulation.ttcnpp:323 Port NSPIP_PROC has accepted the connection from -NSVCI97-provIP(194):PROC.
09:50:17.868275 NS_Emulation.ttcnpp:323 Connect operation on SGSN_Test-Gb0-NS0(192):NSPIP_PROC and -NSVCI97-provIP(194):PROC finished.
09:50:17.868302 NS_Emulation.ttcnpp:324 Starting function main({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97") on component -NSVCI97-provIP(194).
09:50:17.868459 NS_Emulation.ttcnpp:324 Function was started.
09:50:17.868578 NS_Emulation.ttcnpp:346 Creating new alive PTC with component type NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:50:17.870779 NS_Emulation.ttcnpp:346 PTC was created. Component reference: 196, alive: yes, type: NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:50:17.870814 NS_Emulation.ttcnpp:349 Connecting ports SGSN_Test-Gb0-NS0(192):NSVC and -NSVCI97(196):NS_SP.
09:50:17.871136 NS_Emulation.ttcnpp:349 Port NSVC is waiting for connection from -NSVCI97(196):NS_SP on UNIX pathname /tmp/ttcn3-portconn-9f78a688.
09:50:17.871606 NS_Emulation.ttcnpp:349 Port NSVC has accepted the connection from -NSVCI97(196):NS_SP.
09:50:17.871656 NS_Emulation.ttcnpp:349 Connect operation on SGSN_Test-Gb0-NS0(192):NSVC and -NSVCI97(196):NS_SP finished.
09:50:17.871669 NS_Emulation.ttcnpp:350 Starting NSVC component for { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }
09:50:17.871694 NS_Emulation.ttcnpp:351 Starting function NSVCStart({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97", -NSVCI97-provIP(194)) on component -NSVCI97(196).
09:50:17.871768 NS_Emulation.ttcnpp:351 Function was started.
09:50:17.872024 NS_Provider_IPL4.ttcn:214 Called on NSPIP_PROC to -NSVCI97-provIP(194) @NS_Provider_IPL4.NSPIP_add_nsvc : { remote_ip := "127.0.0.10", remote_port := 23000, vc_nsvc := -NSVCI97(196) }
09:50:17.873293 NS_Provider_IPL4.ttcn:214 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:50:17.875499 NS_Provider_IPL4.ttcn:214 Reply enqueued on NSPIP_PROC from -NSVCI97-provIP(194) @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:50:17.875626 NS_Provider_IPL4.ttcn:215 Matching on port NSPIP_PROC succeeded: { } with { } matched value 0 with ? matched
09:50:17.875723 NS_Provider_IPL4.ttcn:215 Getreply operation on port NSPIP_PROC succeeded, reply from -NSVCI97-provIP(194): @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:50:17.875780 NS_Provider_IPL4.ttcn:215 Operation with id 1 was extracted from the queue of NSPIP_PROC.
09:50:17.876379 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_DEAD_BLOCKED (1) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:50:17.876516 NS_Emulation.ttcnpp:448 Matching on port NSVC succeeded:  matched
09:50:17.876572 NS_Emulation.ttcnpp:448 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:50:17.876636 NS_Emulation.ttcnpp:448 Message with id 1 was extracted from the queue of NSVC.
09:50:17.876871 NS_Emulation.ttcnpp:455 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := true }
09:50:17.879808 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:50:17.879854 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:50:17.879889 NS_Emulation.ttcnpp:448 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_DEAD_BLOCKED (1) unmatched: First message in the queue does not match the template: 
09:50:17.879917 NS_Emulation.ttcnpp:457 Matching on port NSVC succeeded:  matched
09:50:17.879966 NS_Emulation.ttcnpp:457 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:50:17.880004 NS_Emulation.ttcnpp:457 Message with id 2 was extracted from the queue of NSVC.
09:50:17.880040 NS_Emulation.ttcnpp:459 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false }
09:50:17.881705 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:50:17.881792 NS_Emulation.ttcnpp:439 Matching on port NSVC succeeded:  matched
09:50:17.881852 NS_Emulation.ttcnpp:439 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:50:17.881899 NS_Emulation.ttcnpp:439 Message with id 3 was extracted from the queue of NSVC.
09:50:17.882305 NS_Emulation.ttcnpp:446 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := true }
09:50:17.883870 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:50:17.884193 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:50:17.884239 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(193): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:50:17.884291 NS_Emulation.ttcnpp:494 Message with id 1 was extracted from the queue of NS_SP.
09:50:17.884417 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(196) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit }
09:50:17.888424 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:50:17.888781 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.888817 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.888835 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.888851 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.888901 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:50:17.888930 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:50:17.888951 NS_Emulation.ttcnpp:474 Message with id 4 was extracted from the queue of NSVC.
09:50:17.888983 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:50:17.891363 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:50:17.891387 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:50:17.891400 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(193): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:50:17.891414 NS_Emulation.ttcnpp:494 Message with id 2 was extracted from the queue of NS_SP.
09:50:17.891429 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(196) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:50:17.892081 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:50:17.892102 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.892115 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.892126 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.892137 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:17.892151 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:50:17.892164 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:50:17.892177 NS_Emulation.ttcnpp:474 Message with id 5 was extracted from the queue of NSVC.
09:50:17.892189 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:50:19.314026 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00EA201C000080101D571000008292624000000006062F224540DD50512C7422000E218F2'O, bssgp := omit } id 3
09:50:19.314101 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:50:19.314133 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:50:19.314159 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(193): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00EA201C000080101D571000008292624000000006062F224540DD50512C7422000E218F2'O, bssgp := omit } id 3
09:50:19.314183 NS_Emulation.ttcnpp:499 Message with id 3 was extracted from the queue of NS_SP.
09:50:19.314211 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(196) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00EA201C000080101D571000008292624000000006062F224540DD50512C7422000E218F2'O, bssgp := omit }
09:50:19.317851 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:50:19.318163 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.318206 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.318236 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.318264 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.318309 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:50:19.318364 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:50:19.318413 NS_Emulation.ttcnpp:474 Message with id 6 was extracted from the queue of NSVC.
09:50:19.318461 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } }
09:50:19.327331 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9101C0040816084A99990000000006CA2F61'O, bssgp := omit } id 4
09:50:19.327399 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:50:19.327439 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:50:19.327477 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(193): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9101C0040816084A99990000000006CA2F61'O, bssgp := omit } id 4
09:50:19.327512 NS_Emulation.ttcnpp:499 Message with id 4 was extracted from the queue of NS_SP.
09:50:19.327552 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(196) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9101C0040816084A99990000000006CA2F61'O, bssgp := omit }
09:50:19.334631 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9C41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O }, initialLLC_PDU := omit } } } id 7
09:50:19.334741 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.334786 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.334831 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.334875 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.334935 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:50:19.335015 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9C41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O }, initialLLC_PDU := omit } } } id 7
09:50:19.335069 NS_Emulation.ttcnpp:474 Message with id 7 was extracted from the queue of NSVC.
09:50:19.335147 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9C41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812106021267DD3A6F66751B1F3E688ADAC40768280D8178D'O }, initialLLC_PDU := omit } } }
09:50:19.344173 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9901C0080813062229D87FFE23094399990000000006F0D8CFED'O, bssgp := omit } id 5
09:50:19.344270 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:50:19.344328 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:50:19.344384 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(193): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9901C0080813062229D87FFE23094399990000000006F0D8CFED'O, bssgp := omit } id 5
09:50:19.344434 NS_Emulation.ttcnpp:499 Message with id 5 was extracted from the queue of NS_SP.
09:50:19.344492 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(196) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01C620BA5A005000088862F224334F0051E00E9901C0080813062229D87FFE23094399990000000006F0D8CFED'O, bssgp := omit }
09:50:19.348086 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(196) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9A01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O }, initialLLC_PDU := omit } } } id 8
09:50:19.348314 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.348379 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.348431 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.348482 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:50:19.348554 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:50:19.348672 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(196): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9A01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O }, initialLLC_PDU := omit } } } id 8
09:50:19.348745 NS_Emulation.ttcnpp:474 Message with id 8 was extracted from the queue of NSVC.
09:50:19.348832 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(193) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00C620BA5A000020168203E8138512C74220000A8200000D8829262400000000600E9A01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'C620BA5A'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000006'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4E30C7EEEE86997'O }, initialLLC_PDU := omit } } }
09:50:19.357302 NS_Emulation.ttcnpp:420 Kill was requested from MC.
09:50:19.357371 NS_Emulation.ttcnpp:420 Terminating test component execution.
09:50:19.358531 - Function NSStart was stopped. PTC terminates.
09:50:19.359714 - Terminating component type NS_Emulation.NS_CT.
09:50:19.359814 - Removing unterminated connection between port NS_SP and SGSN_Test-Gb0-BSSGP0(193):BSCP.
09:50:19.360017 - Port NS_SP was stopped.
09:50:19.360372 - Removing unterminated connection between port NSVC and -NSVCI97(196):NS_SP.
09:50:19.360802 - Port NSVC was stopped.
09:50:19.361393 - Port NS_CTRL was stopped.
09:50:19.361658 - Removing unterminated connection between port NSPIP_PROC and -NSVCI97-provIP(194):PROC.
09:50:19.362110 - Port NSPIP_PROC was stopped.
09:50:19.362427 - Component type NS_Emulation.NS_CT was shut down inside testcase TC_attach_gsup_lu_reject.
09:50:19.362669 - Final verdict of PTC: none
09:50:19.363223 - Disconnected from MC.
09:50:19.363598 - TTCN-3 Parallel Test Component finished.
