09:48:43.561666 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:43.561985 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: TC_attach_timeout_after_pdp_act-BVCI196(90), component type: BSSGP_Emulation.BSSGP_BVC_CT, component name: TC_attach_timeout_after_pdp_act-BVCI196. Version: 11.1.0.
09:48:43.562153 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:43.562393 - Connected to MC.
09:48:43.562405 - Initializing variables, timers and ports of component type BSSGP_Emulation.BSSGP_BVC_CT inside testcase TC_attach_timeout_after_pdp_act.
09:48:43.563383 - Port BVC was started.
09:48:43.563402 - Port MGMT was started.
09:48:43.563411 - Port GLOBAL was started.
09:48:43.563420 - Port BSSGP_SP was started.
09:48:43.563428 - Port BSSGP_SP_SIG was started.
09:48:43.563437 - Port BSSGP_PROC was started.
09:48:43.563446 - Component type BSSGP_Emulation.BSSGP_BVC_CT was initialized.
09:48:43.563471 - Port BVC has established the connection with SGSN_Test-Gb0-BSSGP0(88):BVC using transport type UNIX.
09:48:43.563741 - Starting function f_bssgp_bvc_main({ bvci := 196, cell_id := { ra_id := { lai := { mcc_mnc := '262F42'H, lac := 13135 }, rac := 0 }, cell_id := 20960 }, depth := BSSGP_DECODE_DEPTH_L3 (3), create_cb := refers(BSSGP_Emulation.DefaultCreateCallback) }, false, 96, "TC_attach_timeout_after_pdp_act-BVCI196").
09:48:43.564523 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.564997 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:43.565188 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:43.565233 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.565265 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:43.565328 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:43.565440 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:43.565498 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:43.565563 BSSGP_Emulation.ttcnpp:1319 Message with id 1 was extracted from the queue of BVC.
09:48:43.565610 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.584789 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:43.584930 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:43.584964 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.585055 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:43.585157 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:43.585244 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:43.585322 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:43.585409 BSSGP_Emulation.ttcnpp:1319 Message with id 2 was extracted from the queue of BVC.
09:48:43.585529 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.585644 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:43.585727 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:43.585789 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:43.585867 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC succeeded:  matched
09:48:43.585896 BSSGP_Emulation.ttcnpp:1303 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:43.585923 BSSGP_Emulation.ttcnpp:1303 Message with id 3 was extracted from the queue of BVC.
09:48:43.587760 BSSGP_Emulation.ttcnpp:1044 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 0, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:48:43.587998 BSSGP_Emulation.ttcnpp:1045 Start timer g_T2: 60 s
09:48:43.590413 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:43.590782 BSSGP_Emulation.ttcnpp:1071 Matching on port BVC succeeded:  matched
09:48:43.590819 BSSGP_Emulation.ttcnpp:1071 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:43.590846 BSSGP_Emulation.ttcnpp:1071 Message with id 4 was extracted from the queue of BVC.
09:48:43.590892 BSSGP_Emulation.ttcnpp:1072 Stop timer g_T2: 60 s
09:48:43.590919 BSSGP_Emulation.ttcnpp:1398 BVCI(196) State Transition: BVC_S_BLOCKED (2) -> BVC_S_UNBLOCKED (3)
09:48:43.943308 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP is waiting for connection from TC_attach_timeout_after_pdp_act(107):BSSGP[0] on UNIX pathname /tmp/ttcn3-portconn-de7ac507.
09:48:43.945336 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP has accepted the connection from TC_attach_timeout_after_pdp_act(107):BSSGP[0].
09:48:43.946110 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG is waiting for connection from TC_attach_timeout_after_pdp_act(107):BSSGP_SIG[0] on UNIX pathname /tmp/ttcn3-portconn-de6cc511.
09:48:43.946551 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG has accepted the connection from TC_attach_timeout_after_pdp_act(107):BSSGP_SIG[0].
09:48:43.947163 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC is waiting for connection from TC_attach_timeout_after_pdp_act(107):BSSGP_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-ce3ebd77.
09:48:43.947545 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC has accepted the connection from TC_attach_timeout_after_pdp_act(107):BSSGP_PROC[0].
09:48:43.965889 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000021'H, tlli := 'F0310803'O } id 1
09:48:43.966987 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000021'H with ? matched, tlli := 'F0310803'O with ? matched }
09:48:43.967426 BSSGP_Emulation.ttcnpp:1333 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_timeout_after_pdp_act(107): @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000021'H, tlli := 'F0310803'O } id 1
09:48:43.967604 BSSGP_Emulation.ttcnpp:1333 Operation with id 1 was extracted from the queue of BSSGP_PROC.
09:48:43.967807 BSSGP_Emulation.ttcnpp:851 Adding Client=TC_attach_timeout_after_pdp_act(107), IMSI='262420000000021'H, TLLI='F0310803'O, index=0
09:48:43.969346 BSSGP_Emulation.ttcnpp:1335 Replied on BSSGP_PROC to TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_register_client : { }
09:48:43.985323 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O } } } id 1
09:48:43.985532 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:43.985564 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O } } } id 1
09:48:43.985599 BSSGP_Emulation.ttcnpp:1218 Message with id 1 was extracted from the queue of BSSGP_SP.
09:48:43.985869 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00EA201C000080101D571000008292624000000001262F2240F17110512C7422000E218F2'O, bssgp := omit }
09:48:43.991929 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:43.992477 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:43.992596 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:43.992787 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:43.992878 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:43.992981 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:43.993041 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:43.993098 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:43.993147 BSSGP_Emulation.ttcnpp:1154 Message with id 5 was extracted from the queue of BVC.
09:48:43.997208 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:48:43.999915 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000002001CA2F61'O } } } id 2
09:48:44.000062 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.000124 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000002001CA2F61'O } } } id 2
09:48:44.000183 BSSGP_Emulation.ttcnpp:1218 Message with id 2 was extracted from the queue of BSSGP_SP.
09:48:44.000324 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9101C0040816084A99990000002001CA2F61'O, bssgp := omit }
09:48:44.012340 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9C41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } } id 6
09:48:44.012538 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.012704 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.012852 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.012972 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.013081 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.013167 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.013263 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9C41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812103021F1AC3278AFEC7D3FDCBA85EE36D91F5C80D453BD'O }, initialLLC_PDU := omit } } } id 6
09:48:44.013329 BSSGP_Emulation.ttcnpp:1154 Message with id 6 was extracted from the queue of BVC.
09:48:44.016522 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { authenticationAndCipheringRequest := { messageType := '00010010'B, cipheringAlgorithm := { valueField := '000'B, spare := '0'B }, imeisvRequest := { valueField := '001'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, acReferenceNumber := { valueField := '0011'B }, authenticationParameterRAND := { elementIdentifier := '21'O ("!"), randValue := 'F1AC3278AFEC7D3FDCBA85EE36D91F5C'O }, cipheringKeySequenceNumber := { keySequence := { keySequence := '000'B, spare := '0'B }, elementIdentifier := '1000'B }, authenticationParameterAUTN := omit } } } }
09:48:44.020159 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C008081303222B46941123094399990000002001F0A82DE6'O } } } id 3
09:48:44.020344 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.020424 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C008081303222B46941123094399990000002001F0A82DE6'O } } } id 3
09:48:44.020487 BSSGP_Emulation.ttcnpp:1218 Message with id 3 was extracted from the queue of BSSGP_SP.
09:48:44.020687 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F0310803005000088862F224334F0051E00E9901C008081303222B46941123094399990000002001F0A82DE6'O, bssgp := omit }
09:48:44.026975 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } } id 7
09:48:44.027220 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.027355 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.027496 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.027617 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.027724 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.027804 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.027905 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F0310803000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F0310803'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F78EECD684CDC4'O }, initialLLC_PDU := omit } } } id 7
09:48:44.027978 BSSGP_Emulation.ttcnpp:1154 Message with id 7 was extracted from the queue of BVC.
09:48:44.029482 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'F78EECD6'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:48:44.032918 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'F0310803'O, tlli := 'F78EECD6'O } id 2
09:48:44.033138 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:48:44.033206 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_unregister_client.
09:48:44.033330 BSSGP_Emulation.ttcnpp:1341 Matching on port BSSGP_PROC succeeded: { tlli_old := 'F0310803'O with ? matched, tlli := 'F78EECD6'O with ? matched }
09:48:44.033431 BSSGP_Emulation.ttcnpp:1341 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_timeout_after_pdp_act(107): @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'F0310803'O, tlli := 'F78EECD6'O } id 1
09:48:44.033494 BSSGP_Emulation.ttcnpp:1341 Operation with id 2 was extracted from the queue of BSSGP_PROC.
09:48:44.033688 BSSGP_Emulation.ttcnpp:1343 Replied on BSSGP_PROC to TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_llgmm_assign : { }
09:48:44.034982 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:44.035143 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.035220 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:44.035282 BSSGP_Emulation.ttcnpp:1218 Message with id 4 was extracted from the queue of BSSGP_SP.
09:48:44.035463 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:44.089131 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0100A410503032302000201214A0E54'O } } } id 5
09:48:44.089784 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.090139 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0100A410503032302000201214A0E54'O } } } id 5
09:48:44.090495 BSSGP_Emulation.ttcnpp:1218 Message with id 5 was extracted from the queue of BSSGP_SP.
09:48:44.091037 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0100A410503032302000201214A0E54'O, bssgp := omit }
09:48:44.130443 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9D01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } } id 8
09:48:44.130645 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.130803 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.130962 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.131081 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.131201 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.131287 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.131386 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9D01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 29 }, lLC_PDU := '01C00D8A42030E23621F72993F3F1143FFFF000000042B020121E69AFA'O }, initialLLC_PDU := omit } } } id 8
09:48:44.131452 BSSGP_Emulation.ttcnpp:1154 Message with id 8 was extracted from the queue of BVC.
09:48:44.133179 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1010'B, tiOrSkip := { transactionId := { tio := '000'B, tiFlag := '1'B, tIExtension := omit } }, msgs := { gprs_sm := { activatePDPContextAccept := { messageType := '01000010'B, negotiatedLLCSAPI := { valueField := '0011'B, spare := '0000'B }, negotiatedQoS := { lengthIndicator := 14, qoSV := { reliabilityClass := '011'B, delayClass := '100'B, spare1 := '00'B, precedenceClass := '010'B, spare2 := '0'B, peakThroughput := '0110'B, meanThroughput := '11111'B, spare3 := '000'B, deliverErroneusSDU := '010'B, deliveryOrder := '10'B, trafficClass := '011'B, maxSDUSize := '99'O, maxBitrateUplink := '3F'O ("?"), maxBitrateDownlink := '3F'O ("?"), sduErrorRatio := '0001'B, residualBER := '0001'B, trafficHandlingPriority := '11'B, transferDelay := '010000'B, guaranteedBitRateUplink := 'FF'O, guaranteedBitRateDownlink := 'FF'O, sourceStatisticsDescriptor := '0000'B, signallingIndication := '0'B, spare4 := '000'B, maxBitrateDownlinkExt := '00'O, guaranteedBitRateDownlinkExt := '00'O, maxBitrateUplinkExt := omit, guaranteedBitRateUplinkExt := omit, maxBitrateDownlinkExt2 := omit, guaranteedBitRateDownlinkExt2 := omit, maxBitrateUplinkExt2 := omit, guaranteedBitRateUplinkExt2 := omit } }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, spare := '0000'B, pdpAddress := { elementIdentifier := '2B'O ("+"), pDPAddressLV := { lengthIndicator := 2, pdpAddressV := { pdpTypeOrg := '0001'B, spare := '0000'B, pdpTypeNum := '21'O ("!"), addressInfo := omit } } }, protocolConfigOpts := omit, packetFlowID := omit, sMCause2 := omit, connectivityType := omit, wLANOffloadIndication := omit, nBIFOM_Container := omit } } } }
09:48:44.133861 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E80A8200000E8D43FB01001601F41A05DF8C7C4E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } } id 9
09:48:44.134013 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.134420 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.134539 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.134633 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.134722 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.134794 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.134872 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E80A8200000E8D43FB01001601F41A05DF8C7C4E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := omit, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := omit, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 13 }, lLC_PDU := '43FB01001601F41A05DF8C7C4E'O }, initialLLC_PDU := omit } } } id 9
09:48:44.134936 BSSGP_Emulation.ttcnpp:1154 Message with id 9 was extracted from the queue of BVC.
09:48:44.135637 BSSGP_Emulation.ttcnpp:569 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @LLC_Types.PDU_LLC : { pDU_LLC_U := { address_field := { sAPI := '0011'B, spare := '00'B, cR := '1'B, pD := '0'B }, control_field := { mBits := '1011'B, pF := '1'B, format := '111'B }, information_field_U := { xID := { { xl := '0'B, typefield := '00000'B, xID_length := { short_len := 1 }, xID_Data := { version := { version_value := 0, spare := '0000'B } } }, { xl := '0'B, typefield := '00101'B, xID_length := { short_len := 2 }, xID_Data := { n201_U := { spare := '00000'B, n201UValue := 500 } } }, { xl := '0'B, typefield := '00110'B, xID_length := { short_len := 2 }, xID_Data := { n201_I := { spare := '00000'B, n201IValue := 1503 } } } } }, fCS := '000000'O } }
09:48:44.137941 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 31 }, lLC_PDU := '01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O } } } id 6
09:48:44.138121 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.138201 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 31 }, lLC_PDU := '01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O } } } id 6
09:48:44.138262 BSSGP_Emulation.ttcnpp:1218 Message with id 6 was extracted from the queue of BSSGP_SP.
09:48:44.138447 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9F01C014080101D571000005F4F78EECD662F224C002FF0512C7422000FCCAFA'O, bssgp := omit }
09:48:44.144079 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 10
09:48:44.144266 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.144399 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.144532 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.144675 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.144778 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.144857 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.144948 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E8941C01108150248658E'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C01108150248658E'O }, initialLLC_PDU := omit } } } id 10
09:48:44.145023 BSSGP_Emulation.ttcnpp:1154 Message with id 10 was extracted from the queue of BVC.
09:48:44.145277 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:48:44.146670 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach_timeout_after_pdp_act(107) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0180816084A99990000002001FFDE2B'O } } } id 7
09:48:44.146828 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:44.146904 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach_timeout_after_pdp_act(107): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0180816084A99990000002001FFDE2B'O } } } id 7
09:48:44.146973 BSSGP_Emulation.ttcnpp:1218 Message with id 7 was extracted from the queue of BSSGP_SP.
09:48:44.147148 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F78EECD6005000088862F224334F0051E00E9101C0180816084A99990000002001FFDE2B'O, bssgp := omit }
09:48:44.155328 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } } id 11
09:48:44.155542 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:44.155692 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.155833 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:44.155947 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:44.156064 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:44.156148 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:44.156244 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0150802012A4462F224334F0017161805F4ED9C7A6CE0C0A4'O }, initialLLC_PDU := omit } } } id 11
09:48:44.156311 BSSGP_Emulation.ttcnpp:1154 Message with id 11 was extracted from the queue of BVC.
09:48:44.156619 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'ED9C7A6C'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:48:50.161727 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } } id 12
09:48:50.161976 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:50.162136 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:50.162291 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:50.162424 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:50.162536 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:50.162621 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:50.162716 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0190802012A4462F224334F0017161805F4ED9C7A6CD648F7'O }, initialLLC_PDU := omit } } } id 12
09:48:50.162783 BSSGP_Emulation.ttcnpp:1154 Message with id 12 was extracted from the queue of BVC.
09:48:50.163148 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'ED9C7A6C'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:48:56.164999 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } } id 13
09:48:56.165361 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:56.165600 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:56.165824 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:56.166015 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:56.166173 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:56.166309 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:56.166457 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C01D0802012A4462F224334F0017161805F4ED9C7A6CC430C6'O }, initialLLC_PDU := omit } } } id 13
09:48:56.166547 BSSGP_Emulation.ttcnpp:1154 Message with id 13 was extracted from the queue of BVC.
09:48:56.166935 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'ED9C7A6C'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:49:02.163693 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } } id 14
09:49:02.163943 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:02.164100 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:02.164269 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:02.164411 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:02.164540 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:02.164655 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:02.164768 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0210802012A4462F224334F0017161805F4ED9C7A6C919380'O }, initialLLC_PDU := omit } } } id 14
09:49:02.164844 BSSGP_Emulation.ttcnpp:1154 Message with id 14 was extracted from the queue of BVC.
09:49:02.165219 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'ED9C7A6C'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:49:08.165332 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(88) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } } id 15
09:49:08.165719 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:49:08.165938 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:08.166150 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:49:08.166336 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:49:08.166490 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:49:08.166623 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:49:08.166767 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(88): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00F78EECD6000020168203E8138512C74220000A8200000D8829262400000000120E9A01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'F78EECD6'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000021'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0250802012A4462F224334F0017161805F4ED9C7A6C83EBB1'O }, initialLLC_PDU := omit } } } id 15
09:49:08.166847 BSSGP_Emulation.ttcnpp:1154 Message with id 15 was extracted from the queue of BVC.
09:49:08.167216 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach_timeout_after_pdp_act(107) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'ED9C7A6C'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:49:14.670335 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000021'H } id 3
09:49:14.671085 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:49:14.671489 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000021'H with ? matched }
09:49:14.671877 BSSGP_Emulation.ttcnpp:1337 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach_timeout_after_pdp_act(107): @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000021'H } id 1
09:49:14.672203 BSSGP_Emulation.ttcnpp:1337 Operation with id 3 was extracted from the queue of BSSGP_PROC.
09:49:14.672570 BSSGP_Emulation.ttcnpp:878 Removing Client IMSI='262420000000021'H, index=0
09:49:14.672801 BSSGP_Emulation.ttcnpp:1339 Replied on BSSGP_PROC to TC_attach_timeout_after_pdp_act(107) @BSSGP_Emulation.BSSGP_unregister_client : { }
09:49:14.675929 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP to TC_attach_timeout_after_pdp_act(107):BSSGP[0] was closed unexpectedly by the peer.
09:49:14.676049 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP was disconnected from TC_attach_timeout_after_pdp_act(107):BSSGP[0].
09:49:14.676558 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP_SIG to TC_attach_timeout_after_pdp_act(107):BSSGP_SIG[0] was closed unexpectedly by the peer.
09:49:14.676618 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG was disconnected from TC_attach_timeout_after_pdp_act(107):BSSGP_SIG[0].
09:49:14.678212 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_PROC to TC_attach_timeout_after_pdp_act(107):BSSGP_PROC[0] was closed unexpectedly by the peer.
09:49:14.678261 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC was disconnected from TC_attach_timeout_after_pdp_act(107):BSSGP_PROC[0].
09:49:14.682580 BSSGP_Emulation.ttcnpp:1355 Kill was requested from MC.
09:49:14.682833 BSSGP_Emulation.ttcnpp:1355 Terminating test component execution.
09:49:14.684948 - Function f_bssgp_bvc_main was stopped. PTC terminates.
09:49:14.685658 - Terminating component type BSSGP_Emulation.BSSGP_BVC_CT.
09:49:14.686769 - Removing unterminated connection between port BVC and SGSN_Test-Gb0-BSSGP0(88):BVC.
09:49:14.687008 - Port BVC was stopped.
09:49:14.687515 - Port MGMT was stopped.
09:49:14.687968 - Port GLOBAL was stopped.
09:49:14.689213 - Port BSSGP_SP was stopped.
09:49:14.689435 - Port BSSGP_SP_SIG was stopped.
09:49:14.704840 - Port BSSGP_PROC was stopped.
09:49:14.705147 - Component type BSSGP_Emulation.BSSGP_BVC_CT was shut down inside testcase TC_attach_timeout_after_pdp_act.
09:49:14.705410 - Final verdict of PTC: none
09:49:14.706796 - Disconnected from MC.
09:49:14.707460 - TTCN-3 Parallel Test Component finished.
