09:48:22.647389 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:22.647438 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: TC_attach-BVCI196(6), component type: BSSGP_Emulation.BSSGP_BVC_CT, component name: TC_attach-BVCI196. Version: 11.1.0.
09:48:22.647455 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:22.647488 - Connected to MC.
09:48:22.647581 - Initializing variables, timers and ports of component type BSSGP_Emulation.BSSGP_BVC_CT inside testcase TC_attach.
09:48:22.648508 - Port BVC was started.
09:48:22.648529 - Port MGMT was started.
09:48:22.648540 - Port GLOBAL was started.
09:48:22.648551 - Port BSSGP_SP was started.
09:48:22.648562 - Port BSSGP_SP_SIG was started.
09:48:22.648572 - Port BSSGP_PROC was started.
09:48:22.648583 - Component type BSSGP_Emulation.BSSGP_BVC_CT was initialized.
09:48:22.648617 - Port BVC has established the connection with SGSN_Test-Gb0-BSSGP0(4):BVC using transport type UNIX.
09:48:22.648916 - Starting function f_bssgp_bvc_main({ bvci := 196, cell_id := { ra_id := { lai := { mcc_mnc := '262F42'H, lac := 13135 }, rac := 0 }, cell_id := 20960 }, depth := BSSGP_DECODE_DEPTH_L3 (3), create_cb := refers(BSSGP_Emulation.DefaultCreateCallback) }, false, 96, "TC_attach-BVCI196").
09:48:22.649668 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.650078 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:22.650179 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:22.650197 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.650210 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:22.650223 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:22.650260 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:22.650280 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_WAIT_NS_ALIVE_UNBLOCKED (1) } id 1
09:48:22.650301 BSSGP_Emulation.ttcnpp:1319 Message with id 1 was extracted from the queue of BVC.
09:48:22.650320 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.659546 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:22.659601 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:22.659616 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.659630 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC failed: Type of the first message in the queue is not @BSSGP_Emulation.BssgpResetIndication.
09:48:22.659640 BSSGP_Emulation.ttcnpp:1318 Matching on port BVC failed: Type of the first message in the queue is not @Socket_API_Definitions.PortEvent.
09:48:22.659651 BSSGP_Emulation.ttcnpp:1319 Matching on port BVC succeeded:  matched
09:48:22.659661 BSSGP_Emulation.ttcnpp:1319 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @BSSGP_Emulation.BssgpStatusIndication : { nsei := 96, bvci := 0, state := BVC_S_UNBLOCKED (3) } id 2
09:48:22.659674 BSSGP_Emulation.ttcnpp:1319 Message with id 2 was extracted from the queue of BVC.
09:48:22.659692 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.659739 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:22.659781 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC failed: Type of the first message in the queue is not @NS_Emulation.NsUnitdataIndication.
09:48:22.659792 BSSGP_Emulation.ttcnpp:1078 Timeout operation on timer g_T2 failed: The timer is not started.
09:48:22.659819 BSSGP_Emulation.ttcnpp:1303 Matching on port BVC succeeded:  matched
09:48:22.659871 BSSGP_Emulation.ttcnpp:1303 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @BSSGP_Emulation.BssgpResetIndication : { bvci := 0 } id 3
09:48:22.659881 BSSGP_Emulation.ttcnpp:1303 Message with id 3 was extracted from the queue of BVC.
09:48:22.660652 BSSGP_Emulation.ttcnpp:1044 Sent on BVC to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 0, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:48:22.660764 BSSGP_Emulation.ttcnpp:1045 Start timer g_T2: 60 s
09:48:22.662682 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:22.662834 BSSGP_Emulation.ttcnpp:1071 Matching on port BVC succeeded:  matched
09:48:22.662853 BSSGP_Emulation.ttcnpp:1071 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:22.662867 BSSGP_Emulation.ttcnpp:1071 Message with id 4 was extracted from the queue of BVC.
09:48:22.662888 BSSGP_Emulation.ttcnpp:1072 Stop timer g_T2: 60 s
09:48:22.662903 BSSGP_Emulation.ttcnpp:1398 BVCI(196) State Transition: BVC_S_BLOCKED (2) -> BVC_S_UNBLOCKED (3)
09:48:24.050263 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP is waiting for connection from TC_attach(23):BSSGP[0] on UNIX pathname /tmp/ttcn3-portconn-4978c55b.
09:48:24.053924 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP has accepted the connection from TC_attach(23):BSSGP[0].
09:48:24.054520 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG is waiting for connection from TC_attach(23):BSSGP_SIG[0] on UNIX pathname /tmp/ttcn3-portconn-496ec54d.
09:48:24.055240 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG has accepted the connection from TC_attach(23):BSSGP_SIG[0].
09:48:24.056610 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC is waiting for connection from TC_attach(23):BSSGP_PROC[0] on UNIX pathname /tmp/ttcn3-portconn-593cbd2b.
09:48:24.057547 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC has accepted the connection from TC_attach(23):BSSGP_PROC[0].
09:48:24.082113 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach(23) @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000001'H, tlli := 'E9F62F3B'O } id 1
09:48:24.082626 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000001'H with ? matched, tlli := 'E9F62F3B'O with ? matched }
09:48:24.082837 BSSGP_Emulation.ttcnpp:1333 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach(23): @BSSGP_Emulation.BSSGP_register_client : { imsi := '262420000000001'H, tlli := 'E9F62F3B'O } id 1
09:48:24.082922 BSSGP_Emulation.ttcnpp:1333 Operation with id 1 was extracted from the queue of BSSGP_PROC.
09:48:24.083054 BSSGP_Emulation.ttcnpp:851 Adding Client=TC_attach(23), IMSI='262420000000001'H, TLLI='E9F62F3B'O, index=0
09:48:24.084031 BSSGP_Emulation.ttcnpp:1335 Replied on BSSGP_PROC to TC_attach(23) @BSSGP_Emulation.BSSGP_register_client : { }
09:48:24.101699 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach(23) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O } } } id 1
09:48:24.101938 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:24.101985 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach(23): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 34 }, lLC_PDU := '01C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O } } } id 1
09:48:24.102020 BSSGP_Emulation.ttcnpp:1218 Message with id 1 was extracted from the queue of BSSGP_SP.
09:48:24.102316 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00EA201C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O, bssgp := omit }
09:48:24.112491 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:24.113340 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:24.113499 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.113737 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:24.113883 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.114058 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:24.114155 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:24.114248 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 5
09:48:24.114322 BSSGP_Emulation.ttcnpp:1154 Message with id 5 was extracted from the queue of BVC.
09:48:24.119563 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach(23) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { identityRequest := { messageType := '00010101'B, identityType := { valueField := '010'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B } } } } }
09:48:24.123068 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach(23) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000000001CA2F61'O } } } id 2
09:48:24.123266 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:24.123347 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach(23): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 17 }, lLC_PDU := '01C0040816084A99990000000001CA2F61'O } } } id 2
09:48:24.123407 BSSGP_Emulation.ttcnpp:1218 Message with id 2 was extracted from the queue of BSSGP_SP.
09:48:24.123592 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9101C0040816084A99990000000001CA2F61'O, bssgp := omit }
09:48:24.138870 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9C41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } } id 6
09:48:24.139080 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:24.139229 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.139370 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:24.139487 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.139594 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:24.139671 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:24.139772 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9C41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } } id 6
09:48:24.139837 BSSGP_Emulation.ttcnpp:1154 Message with id 6 was extracted from the queue of BVC.
09:48:24.143017 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach(23) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { authenticationAndCipheringRequest := { messageType := '00010010'B, cipheringAlgorithm := { valueField := '000'B, spare := '0'B }, imeisvRequest := { valueField := '001'B, spare := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, acReferenceNumber := { valueField := '0101'B }, authenticationParameterRAND := { elementIdentifier := '21'O ("!"), randValue := 'B4CE6B59F16CF86E5AECD88532328305'O }, cipheringKeySequenceNumber := { keySequence := { keySequence := '000'B, spare := '0'B }, elementIdentifier := '1000'B }, authenticationParameterAUTN := omit } } } }
09:48:24.146947 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach(23) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C008081305221B4EA31123094399990000000001F0086EEB'O } } } id 3
09:48:24.147153 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:24.147236 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach(23): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 25 }, lLC_PDU := '01C008081305221B4EA31123094399990000000001F0086EEB'O } } } id 3
09:48:24.147298 BSSGP_Emulation.ttcnpp:1218 Message with id 3 was extracted from the queue of BSSGP_SP.
09:48:24.147483 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9901C008081305221B4EA31123094399990000000001F0086EEB'O, bssgp := omit }
09:48:24.155437 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BVC from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9A01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } } id 7
09:48:24.155695 BSSGP_Emulation.ttcnpp:1103 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_UNBLOCK := { bssgpPduType := '24'O ("$"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O } } } unmatched: First message in the queue does not match the template: 
09:48:24.155966 BSSGP_Emulation.ttcnpp:1107 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_BLOCK := { bssgpPduType := '20'O (" "), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.156118 BSSGP_Emulation.ttcnpp:1282 Matching on port BVC .bvci := 196 with 0 unmatched.bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_BVC_RESET := { bssgpPduType := '22'O ("\""), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cause := { iEI := '07'O ("\a"), ext := '1'B, lengthIndicator := { length1 := 1 }, cause_Value := ? }, cell_Identifier := omit, feature_bitmap := *, extended_Feature_Bitmap := * } } unmatched: First message in the queue does not match the template: 
09:48:24.156241 BSSGP_Emulation.ttcnpp:1137 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } with { pDU_BSSGP_FLOW_CONTROL_BVC_ACK := { bssgpPduType := '27'O ("'"), tag := { iEI := '1E'O, ext := '1'B, lengthIndicator := { length1 := 1 }, unstructured_Value := ? } } } unmatched: First message in the queue does not match the template: 
09:48:24.156354 BSSGP_Emulation.ttcnpp:1145 Matching on port BVC .bssgp{ pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } with ({ pDU_BSSGP_STATUS := ? }) unmatched: First message in the queue does not match the template: 
09:48:24.156453 BSSGP_Emulation.ttcnpp:1154 Matching on port BVC succeeded:  matched
09:48:24.156548 BSSGP_Emulation.ttcnpp:1154 Receive operation on port BVC succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9A01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } } id 7
09:48:24.156620 BSSGP_Emulation.ttcnpp:1154 Message with id 7 was extracted from the queue of BVC.
09:48:24.158342 BSSGP_Emulation.ttcnpp:561 Sent on BSSGP_SP to TC_attach(23) @MobileL3_Types.PDU_L3_SGSN_MS : { discriminator := '1000'B, tiOrSkip := { skipIndicator := '0000'B }, msgs := { gprs_mm := { attachAccept := { messageType := '00000010'B, attachResult := { resultOfAttach := '001'B, fop_l3 := '0'B }, forceToStandby := { forceToStandbyValue := '000'B, spare := '0'B }, updateTimer := { timerValue := '01010'B, unit := '001'B }, radioPriority := { priorityLevelValue := '100'B, spare := '0'B }, radioPriorityTOM8 := { priorityLevelValue := '100'B, spare := '0'B }, routingAreaIdentification := { mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O }, ptmsiSignature := omit, readyTimer := { elementIdentifier := '17'O, gprsTimerV := { timerValue := '10110'B, unit := '000'B } }, allocatedPTMSI := { elementIdentifier := '0011000'B, spare1 := '0'B, mobileIdentityLV := { lengthIndicator := 5, mobileIdentityV := { typeOfIdentity := '100'B, oddEvenInd_identity := { tmsi_ptmsi := { oddevenIndicator := '0'B, fillerDigit := '1111'B, octets := 'F185DA02'O } } } } }, msIdentity := omit, gmmCause := omit, t3302 := omit, cellNotification := omit, equivalentPLMNs := omit, networkFeatureSupport := omit, emergencyNumberList := omit, requestedMSInformation := omit, t3319 := omit, t3323 := omit, t3312_ExtendedValue := omit, additionalNetworkFeatureSupport := omit, t3324 := omit, extendedDRXParameters := omit } } } }
09:48:24.162032 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach(23) @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E9F62F3B'O, tlli := 'F185DA02'O } id 2
09:48:24.162283 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:48:24.162360 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_unregister_client.
09:48:24.162497 BSSGP_Emulation.ttcnpp:1341 Matching on port BSSGP_PROC succeeded: { tlli_old := 'E9F62F3B'O with ? matched, tlli := 'F185DA02'O with ? matched }
09:48:24.162603 BSSGP_Emulation.ttcnpp:1341 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach(23): @BSSGP_Emulation.BSSGP_llgmm_assign : { tlli_old := 'E9F62F3B'O, tlli := 'F185DA02'O } id 1
09:48:24.162670 BSSGP_Emulation.ttcnpp:1341 Operation with id 2 was extracted from the queue of BSSGP_PROC.
09:48:24.162872 BSSGP_Emulation.ttcnpp:1343 Replied on BSSGP_PROC to TC_attach(23) @BSSGP_Emulation.BSSGP_llgmm_assign : { }
09:48:24.164174 BSSGP_Emulation.ttcnpp:1355 Message enqueued on BSSGP_SP from TC_attach(23) @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F185DA02'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:24.164382 BSSGP_Emulation.ttcnpp:1218 Matching on port BSSGP_SP succeeded:  matched
09:48:24.164470 BSSGP_Emulation.ttcnpp:1218 Receive operation on port BSSGP_SP succeeded, message from TC_attach(23): @BSSGP_Types.PDU_BSSGP : { pDU_BSSGP_UL_UNITDATA := { bssgpPduType := '01'O, tLLI := 'F185DA02'O, qoS_Profile := { peak_Bit_Rate := '0050'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '0'B, peakBitRateGranularity := '00'B }, cell_Identifier := { iEI := '08'O ("\b"), ext := '1'B, lengthIndicator := { length1 := 8 }, mccDigit1 := '2'H, mccDigit2 := '6'H, mccDigit3 := '2'H, mncDigit3 := 'F'H, mncDigit1 := '4'H, mncDigit2 := '2'H, lac := '334F'O ("3O"), rac := '00'O, cI_value := '51E0'O }, pFI := omit, lSA_Identifier_List := omit, redirect_Attempt_Flag := omit, iMSI_BSSGP := omit, unconfirmed_Send_State_Variable := omit, selected_PLMN_ID := omit, selected_Operator := omit, cS_Registered_Operator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 8 }, lLC_PDU := '01C00C08038EAEFF'O } } } id 4
09:48:24.164539 BSSGP_Emulation.ttcnpp:1218 Message with id 4 was extracted from the queue of BSSGP_SP.
09:48:24.164764 BSSGP_Emulation.ttcnpp:1219 Sent on BVC to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 0, lsp := 196, sdu := '01F185DA02005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:24.215661 BSSGP_Emulation.ttcnpp:1355 Call enqueued on BSSGP_PROC from TC_attach(23) @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000001'H } id 3
09:48:24.216284 BSSGP_Emulation.ttcnpp:1333 Matching on port BSSGP_PROC failed: The first entity in the queue is not a call for signature @BSSGP_Emulation.BSSGP_register_client.
09:48:24.216454 BSSGP_Emulation.ttcnpp:1337 Matching on port BSSGP_PROC succeeded: { imsi := '262420000000001'H with ? matched }
09:48:24.216552 BSSGP_Emulation.ttcnpp:1337 Getcall operation on port BSSGP_PROC succeeded, call from TC_attach(23): @BSSGP_Emulation.BSSGP_unregister_client : { imsi := '262420000000001'H } id 1
09:48:24.216615 BSSGP_Emulation.ttcnpp:1337 Operation with id 3 was extracted from the queue of BSSGP_PROC.
09:48:24.216900 BSSGP_Emulation.ttcnpp:878 Removing Client IMSI='262420000000001'H, index=0
09:48:24.217094 BSSGP_Emulation.ttcnpp:1339 Replied on BSSGP_PROC to TC_attach(23) @BSSGP_Emulation.BSSGP_unregister_client : { }
09:48:24.219168 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP to TC_attach(23):BSSGP[0] was closed unexpectedly by the peer.
09:48:24.219224 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP was disconnected from TC_attach(23):BSSGP[0].
09:48:24.219453 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_SP_SIG to TC_attach(23):BSSGP_SIG[0] was closed unexpectedly by the peer.
09:48:24.219499 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_SP_SIG was disconnected from TC_attach(23):BSSGP_SIG[0].
09:48:24.220182 BSSGP_Emulation.ttcnpp:1355 Connection of port BSSGP_PROC to TC_attach(23):BSSGP_PROC[0] was closed unexpectedly by the peer.
09:48:24.220219 BSSGP_Emulation.ttcnpp:1355 Port BSSGP_PROC was disconnected from TC_attach(23):BSSGP_PROC[0].
09:48:24.227382 BSSGP_Emulation.ttcnpp:1355 Kill was requested from MC.
09:48:24.227501 BSSGP_Emulation.ttcnpp:1355 Terminating test component execution.
09:48:24.229090 - Function f_bssgp_bvc_main was stopped. PTC terminates.
09:48:24.229721 - Terminating component type BSSGP_Emulation.BSSGP_BVC_CT.
09:48:24.229857 - Removing unterminated connection between port BVC and SGSN_Test-Gb0-BSSGP0(4):BVC.
09:48:24.230444 - Port BVC was stopped.
09:48:24.230687 - Port MGMT was stopped.
09:48:24.231184 - Port GLOBAL was stopped.
09:48:24.231611 - Port BSSGP_SP was stopped.
09:48:24.231821 - Port BSSGP_SP_SIG was stopped.
09:48:24.232035 - Port BSSGP_PROC was stopped.
09:48:24.232232 - Component type BSSGP_Emulation.BSSGP_BVC_CT was shut down inside testcase TC_attach.
09:48:24.232415 - Final verdict of PTC: none
09:48:24.232844 - Disconnected from MC.
09:48:24.233256 - TTCN-3 Parallel Test Component finished.
