09:48:27.854756 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:27.854992 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: SGSN_Test-Gb0-NS0(24), component type: NS_Emulation.NS_CT, component name: SGSN_Test-Gb0-NS0. Version: 11.1.0.
09:48:27.855063 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:27.855203 - Connected to MC.
09:48:27.855283 - Initializing variables, timers and ports of component type NS_Emulation.NS_CT inside testcase TC_attach_mnc3.
09:48:27.858463 - Port NS_SP was started.
09:48:27.858561 - Port NSVC was started.
09:48:27.858617 - Port NS_CTRL was started.
09:48:27.858666 - Port NSPIP_PROC was started.
09:48:27.858715 - Component type NS_Emulation.NS_CT was initialized.
09:48:27.861719 - Port NS_SP is waiting for connection from SGSN_Test-Gb0-BSSGP0(25):BSCP on UNIX pathname /tmp/ttcn3-portconn-9a7fba03.
09:48:27.863390 - Port NS_SP has accepted the connection from SGSN_Test-Gb0-BSSGP0(25):BSCP.
09:48:27.864120 - Starting function NSStart({ nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "").
09:48:27.864817 NS_Emulation.ttcnpp:320 Creating NSIP provider for "127.0.0.103":21010
09:48:27.864947 NS_Emulation.ttcnpp:322 Creating new alive PTC with component type NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:27.869795 NS_Emulation.ttcnpp:322 PTC was created. Component reference: 26, alive: yes, type: NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:27.869866 NS_Emulation.ttcnpp:323 Connecting ports SGSN_Test-Gb0-NS0(24):NSPIP_PROC and -NSVCI97-provIP(26):PROC.
09:48:27.870077 NS_Emulation.ttcnpp:323 Port NSPIP_PROC is waiting for connection from -NSVCI97-provIP(26):PROC on UNIX pathname /tmp/ttcn3-portconn-c321aa5f.
09:48:27.871441 NS_Emulation.ttcnpp:323 Port NSPIP_PROC has accepted the connection from -NSVCI97-provIP(26):PROC.
09:48:27.871458 NS_Emulation.ttcnpp:323 Connect operation on SGSN_Test-Gb0-NS0(24):NSPIP_PROC and -NSVCI97-provIP(26):PROC finished.
09:48:27.871493 NS_Emulation.ttcnpp:324 Starting function main({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97") on component -NSVCI97-provIP(26).
09:48:27.871705 NS_Emulation.ttcnpp:324 Function was started.
09:48:27.871848 NS_Emulation.ttcnpp:346 Creating new alive PTC with component type NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:27.874127 NS_Emulation.ttcnpp:346 PTC was created. Component reference: 28, alive: yes, type: NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:27.874167 NS_Emulation.ttcnpp:349 Connecting ports SGSN_Test-Gb0-NS0(24):NSVC and -NSVCI97(28):NS_SP.
09:48:27.874285 NS_Emulation.ttcnpp:349 Port NSVC is waiting for connection from -NSVCI97(28):NS_SP on UNIX pathname /tmp/ttcn3-portconn-d376a650.
09:48:27.874983 NS_Emulation.ttcnpp:349 Port NSVC has accepted the connection from -NSVCI97(28):NS_SP.
09:48:27.874996 NS_Emulation.ttcnpp:349 Connect operation on SGSN_Test-Gb0-NS0(24):NSVC and -NSVCI97(28):NS_SP finished.
09:48:27.875006 NS_Emulation.ttcnpp:350 Starting NSVC component for { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }
09:48:27.875029 NS_Emulation.ttcnpp:351 Starting function NSVCStart({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97", -NSVCI97-provIP(26)) on component -NSVCI97(28).
09:48:27.875107 NS_Emulation.ttcnpp:351 Function was started.
09:48:27.875307 NS_Provider_IPL4.ttcn:214 Called on NSPIP_PROC to -NSVCI97-provIP(26) @NS_Provider_IPL4.NSPIP_add_nsvc : { remote_ip := "127.0.0.10", remote_port := 23000, vc_nsvc := -NSVCI97(28) }
09:48:27.875756 NS_Provider_IPL4.ttcn:214 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:27.876570 NS_Provider_IPL4.ttcn:214 Reply enqueued on NSPIP_PROC from -NSVCI97-provIP(26) @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:27.876612 NS_Provider_IPL4.ttcn:215 Matching on port NSPIP_PROC succeeded: { } with { } matched value 0 with ? matched
09:48:27.876655 NS_Provider_IPL4.ttcn:215 Getreply operation on port NSPIP_PROC succeeded, reply from -NSVCI97-provIP(26): @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:27.876678 NS_Provider_IPL4.ttcn:215 Operation with id 1 was extracted from the queue of NSPIP_PROC.
09:48:27.876897 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_DEAD_BLOCKED (1) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:27.876940 NS_Emulation.ttcnpp:448 Matching on port NSVC succeeded:  matched
09:48:27.876961 NS_Emulation.ttcnpp:448 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:27.876979 NS_Emulation.ttcnpp:448 Message with id 1 was extracted from the queue of NSVC.
09:48:27.877062 NS_Emulation.ttcnpp:455 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := true }
09:48:27.878277 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:27.878301 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:27.878314 NS_Emulation.ttcnpp:448 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_DEAD_BLOCKED (1) unmatched: First message in the queue does not match the template: 
09:48:27.878333 NS_Emulation.ttcnpp:457 Matching on port NSVC succeeded:  matched
09:48:27.878345 NS_Emulation.ttcnpp:457 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:27.878358 NS_Emulation.ttcnpp:457 Message with id 2 was extracted from the queue of NSVC.
09:48:27.878596 NS_Emulation.ttcnpp:459 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false }
09:48:27.878934 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:27.878985 NS_Emulation.ttcnpp:439 Matching on port NSVC succeeded:  matched
09:48:27.879013 NS_Emulation.ttcnpp:439 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:27.879035 NS_Emulation.ttcnpp:439 Message with id 3 was extracted from the queue of NSVC.
09:48:27.879229 NS_Emulation.ttcnpp:446 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := true }
09:48:27.880122 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:27.880314 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:27.880345 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:27.880378 NS_Emulation.ttcnpp:494 Message with id 1 was extracted from the queue of NS_SP.
09:48:27.880455 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit }
09:48:27.883104 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:27.883418 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.883449 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.883470 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.883489 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.883553 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:27.883581 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:27.883605 NS_Emulation.ttcnpp:474 Message with id 4 was extracted from the queue of NSVC.
09:48:27.883651 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:27.885940 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C40781080888200324334F0051E0'O, bssgp := omit } id 2
09:48:27.885991 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:27.886017 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C40781080888200324334F0051E0'O, bssgp := omit } id 2
09:48:27.886038 NS_Emulation.ttcnpp:494 Message with id 2 was extracted from the queue of NS_SP.
09:48:27.886063 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C40781080888200324334F0051E0'O, bssgp := omit }
09:48:27.886702 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:27.886735 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.886826 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.886847 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.886867 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:27.886893 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:27.886918 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:27.886940 NS_Emulation.ttcnpp:474 Message with id 5 was extracted from the queue of NSVC.
09:48:27.886965 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:29.336616 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00EA201C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O, bssgp := omit } id 3
09:48:29.336863 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:29.336934 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:29.336978 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00EA201C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O, bssgp := omit } id 3
09:48:29.337019 NS_Emulation.ttcnpp:499 Message with id 3 was extracted from the queue of NS_SP.
09:48:29.337063 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00EA201C000080101D571000008292624000000011062F224C4B61E0512C7422000E218F2'O, bssgp := omit }
09:48:29.341226 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:29.341680 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.341731 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.341766 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.341804 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.341864 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:29.341942 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:29.341992 NS_Emulation.ttcnpp:474 Message with id 6 was extracted from the queue of NSVC.
09:48:29.342054 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } }
09:48:29.358133 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9101C0040816084A99990000100001CA2F61'O, bssgp := omit } id 4
09:48:29.358239 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:29.358310 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:29.358375 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9101C0040816084A99990000100001CA2F61'O, bssgp := omit } id 4
09:48:29.358434 NS_Emulation.ttcnpp:499 Message with id 4 was extracted from the queue of NS_SP.
09:48:29.358502 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9101C0040816084A99990000100001CA2F61'O, bssgp := omit }
09:48:29.368616 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9C41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } } id 7
09:48:29.368773 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.368830 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.368883 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.368936 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.369009 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:29.369110 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9C41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } } id 7
09:48:29.369174 NS_Emulation.ttcnpp:474 Message with id 7 was extracted from the queue of NSVC.
09:48:29.369273 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9C41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C005081210C021759DCDD7DDE661B696F07F7FDD0942CB801E6FFA'O }, initialLLC_PDU := omit } } }
09:48:29.380171 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9901C00808130C228890578E23094399990000100001F0380BFA'O, bssgp := omit } id 5
09:48:29.380251 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:29.380313 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:29.380372 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9901C00808130C228890578E23094399990000100001F0380BFA'O, bssgp := omit } id 5
09:48:29.380426 NS_Emulation.ttcnpp:499 Message with id 5 was extracted from the queue of NS_SP.
09:48:29.380490 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E91C47EA0050000888200324334F0051E00E9901C00808130C228890578E23094399990000100001F0380BFA'O, bssgp := omit }
09:48:29.383828 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(28) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9A01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } } id 8
09:48:29.384110 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.384235 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.384337 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.384421 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:29.384552 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:29.384847 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(28): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9A01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } } id 8
09:48:29.385057 NS_Emulation.ttcnpp:474 Message with id 8 was extracted from the queue of NSVC.
09:48:29.385210 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E91C47EA000020168203E8138512C74220000A8200000D8829262400000001100E9A01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E91C47EA'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000001001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A44200324334F0017161805F4F5ECC758C1B201'O }, initialLLC_PDU := omit } } }
09:48:29.396611 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(25) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F5ECC7580050000888200324334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:29.396726 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:29.396809 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:29.396875 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(25): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F5ECC7580050000888200324334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:29.396936 NS_Emulation.ttcnpp:499 Message with id 6 was extracted from the queue of NS_SP.
09:48:29.397005 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(28) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F5ECC7580050000888200324334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:29.462889 NS_Emulation.ttcnpp:420 Kill was requested from MC.
09:48:29.463193 NS_Emulation.ttcnpp:420 Terminating test component execution.
09:48:29.467381 - Function NSStart was stopped. PTC terminates.
09:48:29.467679 - Terminating component type NS_Emulation.NS_CT.
09:48:29.468718 - Removing unterminated connection between port NS_SP and SGSN_Test-Gb0-BSSGP0(25):BSCP.
09:48:29.469222 - Port NS_SP was stopped.
09:48:29.469660 - Removing unterminated connection between port NSVC and -NSVCI97(28):NS_SP.
09:48:29.470030 - Port NSVC was stopped.
09:48:29.470440 - Port NS_CTRL was stopped.
09:48:29.470664 - Removing unterminated connection between port NSPIP_PROC and -NSVCI97-provIP(26):PROC.
09:48:29.470939 - Port NSPIP_PROC was stopped.
09:48:29.471143 - Component type NS_Emulation.NS_CT was shut down inside testcase TC_attach_mnc3.
09:48:29.471639 - Final verdict of PTC: none
09:48:29.484907 - Disconnected from MC.
09:48:29.485292 - TTCN-3 Parallel Test Component finished.
