09:48:22.635700 - Warning: A plug-in from the same path `libjunitlogger2' is already active, skipping plug-in
09:48:22.635873 - TTCN-3 Parallel Test Component started on 2df32e2774f1. Component reference: SGSN_Test-Gb0-NS0(3), component type: NS_Emulation.NS_CT, component name: SGSN_Test-Gb0-NS0. Version: 11.1.0.
09:48:22.635948 - TTCN Logger v2.2 options: TimeStampFormat:=Time; LogEntityName:=No; LogEventTypes:=No; SourceInfoFormat:=Single; LogSensitiveData:=No; *.FileMask:=LOG_ALL | MATCHING; *.ConsoleMask:=ERROR | TESTCASE | USER | VERDICTOP | WARNING; LogFileSize:=0; LogFileNumber:=1; DiskFullAction:=Error
09:48:22.636021 - Connected to MC.
09:48:22.636053 - Initializing variables, timers and ports of component type NS_Emulation.NS_CT inside testcase TC_attach.
09:48:22.638178 - Port NS_SP was started.
09:48:22.638242 - Port NSVC was started.
09:48:22.638278 - Port NS_CTRL was started.
09:48:22.638299 - Port NSPIP_PROC was started.
09:48:22.638318 - Component type NS_Emulation.NS_CT was initialized.
09:48:22.640477 - Port NS_SP is waiting for connection from SGSN_Test-Gb0-BSSGP0(4):BSCP on UNIX pathname /tmp/ttcn3-portconn-517cba18.
09:48:22.641710 - Port NS_SP has accepted the connection from SGSN_Test-Gb0-BSSGP0(4):BSCP.
09:48:22.642355 - Starting function NSStart({ nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "").
09:48:22.642775 NS_Emulation.ttcnpp:320 Creating NSIP provider for "127.0.0.103":21010
09:48:22.642855 NS_Emulation.ttcnpp:322 Creating new alive PTC with component type NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:22.645767 NS_Emulation.ttcnpp:322 PTC was created. Component reference: 5, alive: yes, type: NS_Provider_IPL4.NS_Provider_IPL4_CT, component name: -NSVCI97-provIP.
09:48:22.645821 NS_Emulation.ttcnpp:323 Connecting ports SGSN_Test-Gb0-NS0(3):NSPIP_PROC and -NSVCI97-provIP(5):PROC.
09:48:22.645932 NS_Emulation.ttcnpp:323 Port NSPIP_PROC is waiting for connection from -NSVCI97-provIP(5):PROC on UNIX pathname /tmp/ttcn3-portconn-a22aa44.
09:48:22.646934 NS_Emulation.ttcnpp:323 Port NSPIP_PROC has accepted the connection from -NSVCI97-provIP(5):PROC.
09:48:22.646947 NS_Emulation.ttcnpp:323 Connect operation on SGSN_Test-Gb0-NS0(3):NSPIP_PROC and -NSVCI97-provIP(5):PROC finished.
09:48:22.646975 NS_Emulation.ttcnpp:324 Starting function main({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97") on component -NSVCI97-provIP(5).
09:48:22.647117 NS_Emulation.ttcnpp:324 Function was started.
09:48:22.647224 NS_Emulation.ttcnpp:346 Creating new alive PTC with component type NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:22.649233 NS_Emulation.ttcnpp:346 PTC was created. Component reference: 7, alive: yes, type: NS_Emulation.NSVC_CT, component name: -NSVCI97.
09:48:22.649270 NS_Emulation.ttcnpp:349 Connecting ports SGSN_Test-Gb0-NS0(3):NSVC and -NSVCI97(7):NS_SP.
09:48:22.649432 NS_Emulation.ttcnpp:349 Port NSVC is waiting for connection from -NSVCI97(7):NS_SP on UNIX pathname /tmp/ttcn3-portconn-1e75a64b.
09:48:22.650110 NS_Emulation.ttcnpp:349 Port NSVC has accepted the connection from -NSVCI97(7):NS_SP.
09:48:22.650124 NS_Emulation.ttcnpp:349 Connect operation on SGSN_Test-Gb0-NS0(3):NSVC and -NSVCI97(7):NS_SP finished.
09:48:22.650137 NS_Emulation.ttcnpp:350 Starting NSVC component for { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }
09:48:22.650162 NS_Emulation.ttcnpp:351 Starting function NSVCStart({ provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 }, { nsei := 96, role_sgsn := false, handle_sns := false, nsvc := { { provider := { ip := { address_family := AF_INET (2), local_udp_port := 21010, local_ip := "127.0.0.103", remote_udp_port := 23000, remote_ip := "127.0.0.10", data_weight := 1, signalling_weight := 1 } }, nsvci := 97 } } }, "-NSVCI97", -NSVCI97-provIP(5)) on component -NSVCI97(7).
09:48:22.650229 NS_Emulation.ttcnpp:351 Function was started.
09:48:22.650423 NS_Provider_IPL4.ttcn:214 Called on NSPIP_PROC to -NSVCI97-provIP(5) @NS_Provider_IPL4.NSPIP_add_nsvc : { remote_ip := "127.0.0.10", remote_port := 23000, vc_nsvc := -NSVCI97(7) }
09:48:22.650933 NS_Provider_IPL4.ttcn:214 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:22.651719 NS_Provider_IPL4.ttcn:214 Reply enqueued on NSPIP_PROC from -NSVCI97-provIP(5) @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:22.651761 NS_Provider_IPL4.ttcn:215 Matching on port NSPIP_PROC succeeded: { } with { } matched value 0 with ? matched
09:48:22.651795 NS_Provider_IPL4.ttcn:215 Getreply operation on port NSPIP_PROC succeeded, reply from -NSVCI97-provIP(5): @NS_Provider_IPL4.NSPIP_add_nsvc : { } value 0 id 1
09:48:22.651817 NS_Provider_IPL4.ttcn:215 Operation with id 1 was extracted from the queue of NSPIP_PROC.
09:48:22.652047 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_DEAD_BLOCKED (1) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:22.652093 NS_Emulation.ttcnpp:448 Matching on port NSVC succeeded:  matched
09:48:22.652114 NS_Emulation.ttcnpp:448 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := false } id 1
09:48:22.652134 NS_Emulation.ttcnpp:448 Message with id 1 was extracted from the queue of NSVC.
09:48:22.652223 NS_Emulation.ttcnpp:455 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_DEAD_BLOCKED (1), new_state := NSVC_S_DEAD_BLOCKED (1), first_or_last := true }
09:48:22.653452 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:22.653475 NS_Emulation.ttcnpp:439 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_ALIVE_UNBLOCKED (4) unmatched: First message in the queue does not match the template: 
09:48:22.653488 NS_Emulation.ttcnpp:448 Matching on port NSVC NSVC_S_ALIVE_BLOCKED (3) with NSVC_S_DEAD_BLOCKED (1) unmatched: First message in the queue does not match the template: 
09:48:22.653517 NS_Emulation.ttcnpp:457 Matching on port NSVC succeeded:  matched
09:48:22.653531 NS_Emulation.ttcnpp:457 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false } id 2
09:48:22.653542 NS_Emulation.ttcnpp:457 Message with id 2 was extracted from the queue of NSVC.
09:48:22.653554 NS_Emulation.ttcnpp:459 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_WAIT_RESET (2), new_state := NSVC_S_ALIVE_BLOCKED (3), first_or_last := false }
09:48:22.654174 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:22.654220 NS_Emulation.ttcnpp:439 Matching on port NSVC succeeded:  matched
09:48:22.654247 NS_Emulation.ttcnpp:439 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := false } id 3
09:48:22.654269 NS_Emulation.ttcnpp:439 Message with id 3 was extracted from the queue of NSVC.
09:48:22.654455 NS_Emulation.ttcnpp:446 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsStatusIndication : { nsei := 96, nsvci := 97, old_state := NSVC_S_ALIVE_BLOCKED (3), new_state := NSVC_S_ALIVE_UNBLOCKED (4), first_or_last := true }
09:48:22.655305 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:22.655496 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:22.655523 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit } id 1
09:48:22.655553 NS_Emulation.ttcnpp:494 Message with id 1 was extracted from the queue of NS_SP.
09:48:22.655627 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 0, sdu := '2204820000078108'O, bssgp := omit }
09:48:22.658267 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:22.658560 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.658590 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.658608 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.658626 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.658689 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:22.658714 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 4
09:48:22.658734 NS_Emulation.ttcnpp:474 Message with id 4 was extracted from the queue of NSVC.
09:48:22.658777 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '2304820000'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '0000'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:22.660949 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:48:22.660990 NS_Emulation.ttcnpp:494 Matching on port NS_SP succeeded:  matched
09:48:22.661019 NS_Emulation.ttcnpp:494 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit } id 2
09:48:22.661040 NS_Emulation.ttcnpp:494 Message with id 2 was extracted from the queue of NS_SP.
09:48:22.661066 NS_Emulation.ttcnpp:497 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 0, nsei := 96, lsp := 196, sdu := '22048200C4078108088862F224334F0051E0'O, bssgp := omit }
09:48:22.661803 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:22.661839 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.661861 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.661881 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.661901 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:22.661925 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:22.661960 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } } id 5
09:48:22.661984 NS_Emulation.ttcnpp:474 Message with id 5 was extracted from the queue of NSVC.
09:48:22.662008 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 0, nsei := 96, nsvci := 97, sdu := '23048200C4'O, bssgp := { pDU_BSSGP_BVC_RESET_ACK := { bssgpPduType := '23'O ("#"), bVCI := { iEI := '04'O, ext := '1'B, lengthIndicator := { length1 := 2 }, unstructured_value := '00C4'O }, cell_Identifier := omit, feature_bitmap := omit, extended_Feature_Bitmap := omit } } }
09:48:24.102725 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00EA201C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O, bssgp := omit } id 3
09:48:24.102876 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:24.102930 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:24.102973 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00EA201C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O, bssgp := omit } id 3
09:48:24.103023 NS_Emulation.ttcnpp:499 Message with id 3 was extracted from the queue of NS_SP.
09:48:24.103068 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00EA201C000080101D571000008292624000000001062F224AABDA30512C7422000E218F2'O, bssgp := omit }
09:48:24.107320 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:24.108170 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.108270 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.108346 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.108410 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.108544 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:24.108729 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } } id 6
09:48:24.108844 NS_Emulation.ttcnpp:474 Message with id 6 was extracted from the queue of NSVC.
09:48:24.108991 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E8941C001081502DE8E9A'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 9 }, lLC_PDU := '41C001081502DE8E9A'O }, initialLLC_PDU := omit } } }
09:48:24.124335 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9101C0040816084A99990000000001CA2F61'O, bssgp := omit } id 4
09:48:24.124581 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:24.124736 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:24.124964 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9101C0040816084A99990000000001CA2F61'O, bssgp := omit } id 4
09:48:24.125082 NS_Emulation.ttcnpp:499 Message with id 4 was extracted from the queue of NS_SP.
09:48:24.125217 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9101C0040816084A99990000000001CA2F61'O, bssgp := omit }
09:48:24.135939 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9C41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } } id 7
09:48:24.136227 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.136339 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.136448 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.136548 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.136721 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:24.136922 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9C41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } } id 7
09:48:24.137056 NS_Emulation.ttcnpp:474 Message with id 7 was extracted from the queue of NSVC.
09:48:24.137223 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9C41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 28 }, lLC_PDU := '41C0050812105021B4CE6B59F16CF86E5AECD8853232830580205ED2'O }, initialLLC_PDU := omit } } }
09:48:24.148061 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9901C008081305221B4EA31123094399990000000001F0086EEB'O, bssgp := omit } id 5
09:48:24.148250 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:24.148386 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:24.148506 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9901C008081305221B4EA31123094399990000000001F0086EEB'O, bssgp := omit } id 5
09:48:24.148615 NS_Emulation.ttcnpp:499 Message with id 5 was extracted from the queue of NS_SP.
09:48:24.148758 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01E9F62F3B005000088862F224334F0051E00E9901C008081305221B4EA31123094399990000000001F0086EEB'O, bssgp := omit }
09:48:24.152585 NS_Emulation.ttcnpp:420 Message enqueued on NSVC from -NSVCI97(7) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9A01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } } id 8
09:48:24.152800 NS_Emulation.ttcnpp:439 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.152912 NS_Emulation.ttcnpp:448 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.153008 NS_Emulation.ttcnpp:457 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.153101 NS_Emulation.ttcnpp:461 Matching on port NSVC failed: Type of the first message in the queue is not @NS_Emulation.NsStatusIndication.
09:48:24.153239 NS_Emulation.ttcnpp:474 Matching on port NSVC succeeded:  matched
09:48:24.153405 NS_Emulation.ttcnpp:474 Receive operation on port NSVC succeeded, message from -NSVCI97(7): @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9A01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } } id 8
09:48:24.153522 NS_Emulation.ttcnpp:474 Message with id 8 was extracted from the queue of NSVC.
09:48:24.153850 NS_Emulation.ttcnpp:475 Sent on NS_SP to SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataIndication : { bvci := 196, nsei := 96, nsvci := 97, sdu := '00E9F62F3B000020168203E8138512C74220000A8200000D8829262400000000100E9A01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O, bssgp := { pDU_BSSGP_DL_UNITDATA := { bssgpPduType := '00'O, tLLI_current := 'E9F62F3B'O, qoS_Profile := { peak_Bit_Rate := '0000'O, precedence := '000'B, a_bit := '0'B, t_bit := '0'B, c_r_bit := '1'B, peakBitRateGranularity := '00'B }, pDU_Lifetime := { iEI := '16'O, ext := '1'B, lengthIndicator := { length1 := 2 }, delay_Value := '03E8'O }, mS_Radio_Access_Capability := { iEI := '13'O, ext := '1'B, lengthIndicator := { length1 := 5 }, mSRadioAccessCapabilityV_BSSGP := { { mSRACapabilityValues := { mSRACapabilityValuesExclude1111 := { accessTechnType := '0001'B, accessCapabilities := { lengthIndicator := 22, accessCapabilities := { rfPowerCapability := '001'B, presenceBitA5 := '1'B, a5bits := { a51 := '1'B, a52 := '0'B, a53 := '1'B, a54 := '0'B, a55 := '0'B, a56 := '0'B, a57 := '0'B }, esind := '1'B, psbit := '0'B, vgcs := '0'B, vbs := '0'B, presenceBitMultislot := '1'B, multislotcap := { presenceBitHscsd := '0'B, hscsdmultislotclass := omit, presenceBitGprs := '0'B, gprsmultislot := omit, presenceBitSms := '0'B, multislotCap_SMS := omit, multislotCapAdditionsAfterRel97 := { presenceBitEcsdmulti := '0'B, ecsdmultislotclass := omit, presenceBitEgprsmulti := '0'B, multislotCap_EGPRS := omit, presenceBitDtmGprsmulti := '0'B, multislotCapdtmgprsmultislotsubclass := omit } }, accessCapAdditionsAfterRel97 := omit }, spare_bits := omit } } }, presenceBitMSRACap := '0'B } } }, priority := omit, dRX_Parameters := { iEI := '0A'O ("\n"), ext := '1'B, lengthIndicator := { length1 := 2 }, splitPG_CycleCode := '00'O, nonDRXTimer := '000'B, splitOnCCCH := '0'B, cnSpecificDRXCycleLength := '0000'B }, iMSI := { iEI := '0D'O ("\r"), ext := '1'B, lengthIndicator := { length1 := 8 }, type_of_Identity := '001'B, oddevenIndicator := '1'B, digits := '262420000000001'H }, tLLI_old := omit, pFI := omit, lSA_Information := omit, service_UTRAN_CCO := omit, service_Class_Indicator := omit, subscriber_Profile_ID_For_RAT_Priority := omit, redirection_Indication := omit, redirection_Completed := omit, unconfirmed_Send_State_Variable := omit, sCI := omit, gGSN_PGW_Location := omit, eDRX_Paremeters := omit, old_Routing_Area_Identification := omit, attach_Indicator := omit, alignment_octets := omit, lLC_PDU := { iEI := '0E'O, ext := '1'B, lengthIndicator := { length1 := 26 }, lLC_PDU := '01C0090802012A4462F224334F0017161805F4F185DA02EC6245'O }, initialLLC_PDU := omit } } }
09:48:24.165420 NS_Emulation.ttcnpp:420 Message enqueued on NS_SP from SGSN_Test-Gb0-BSSGP0(4) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F185DA02005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:24.165653 NS_Emulation.ttcnpp:494 Matching on port NS_SP .bvci := 196 with 0 unmatched: First message in the queue does not match the template: 
09:48:24.165778 NS_Emulation.ttcnpp:499 Matching on port NS_SP succeeded:  matched
09:48:24.165899 NS_Emulation.ttcnpp:499 Receive operation on port NS_SP succeeded, message from SGSN_Test-Gb0-BSSGP0(4): @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F185DA02005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit } id 6
09:48:24.166005 NS_Emulation.ttcnpp:499 Message with id 6 was extracted from the queue of NS_SP.
09:48:24.166128 NS_Emulation.ttcnpp:502 Sent on NSVC to -NSVCI97(7) @NS_Emulation.NsUnitdataRequest : { bvci := 196, nsei := 96, lsp := 196, sdu := '01F185DA02005000088862F224334F0051E00E8801C00C08038EAEFF'O, bssgp := omit }
09:48:24.227389 NS_Emulation.ttcnpp:420 Kill was requested from MC.
09:48:24.227581 NS_Emulation.ttcnpp:420 Terminating test component execution.
09:48:24.229616 - Function NSStart was stopped. PTC terminates.
09:48:24.230096 - Terminating component type NS_Emulation.NS_CT.
09:48:24.230229 - Removing unterminated connection between port NS_SP and SGSN_Test-Gb0-BSSGP0(4):BSCP.
09:48:24.231082 - Port NS_SP was stopped.
09:48:24.231512 - Removing unterminated connection between port NSVC and -NSVCI97(7):NS_SP.
09:48:24.232093 - Port NSVC was stopped.
09:48:24.232384 - Port NS_CTRL was stopped.
09:48:24.232557 - Removing unterminated connection between port NSPIP_PROC and -NSVCI97-provIP(5):PROC.
09:48:24.233059 - Port NSPIP_PROC was stopped.
09:48:24.248741 - Component type NS_Emulation.NS_CT was shut down inside testcase TC_attach.
09:48:24.249025 - Final verdict of PTC: none
09:48:24.249671 - Disconnected from MC.
09:48:24.249788 - TTCN-3 Parallel Test Component finished.
