(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "icE1usb - GPS")
    (date "2022-09-05")
    (rev "1.1")
    (comment 1 "CERN-OHL-S")
    (comment 2 "(C) 2020-2022 Sylvain Munaut")
  )
  (lib_symbols
    (symbol "Device:Battery_Cell" (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "BT" (id 0) (at 2.54 2.54 0))
      (property "Value" "Battery_Cell" (id 1) (at 2.54 0 0))
      (property "Footprint" "" (id 2) (at 0 1.524 90))
      (property "Datasheet" "~" (id 3) (at 0 1.524 90))
      (property "ki_keywords" "battery cell" (id 4) (at 0 0 0))
      (property "ki_description" "Single-cell battery" (id 5) (at 0 0 0))
      (symbol "Battery_Cell_0_1"
        (rectangle (start -2.286 1.778) (end 2.286 1.524)
          (fill (type outline))
        )
        (rectangle (start -1.5748 1.1938) (end 1.4732 0.6858)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 0 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.778)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 3.429)
            (xy 1.524 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 3.937)
            (xy 1.016 2.921)
          )
          (fill (type none))
        )
      )
      (symbol "Battery_Cell_1_1"
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "+")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.54)
          (name "-")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "C_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "capacitor cap" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_Small_0_1"
        (polyline
          (pts
            (xy -1.524 -0.508)
            (xy 1.524 -0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
      )
      (symbol "C_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:D_Schottky_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at -1.27 2.032 0))
      (property "Value" "D_Schottky_Small" (id 1) (at -7.112 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 90))
      (property "ki_keywords" "diode Schottky" (id 4) (at 0 0 0))
      (property "ki_description" "Schottky diode, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_Schottky_Small_0_1"
        (polyline
          (pts
            (xy -0.762 0)
            (xy 0.762 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.762 -1.016)
            (xy -0.762 0)
            (xy 0.762 1.016)
            (xy 0.762 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0.762)
            (xy -1.27 1.016)
            (xy -0.762 1.016)
            (xy -0.762 -1.016)
            (xy -0.254 -1.016)
            (xy -0.254 -0.762)
          )
          (fill (type none))
        )
      )
      (symbol "D_Schottky_Small_1_1"
        (pin passive line (at -2.54 0 0) (length 1.778)
          (name "K")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.778)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:D_TVS" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "D_TVS" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode TVS thyrector" (id 4) (at 0 0 0))
      (property "ki_description" "Bidirectional transient-voltage-suppression diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO-???* *_Diode_* *SingleDiode* D_*" (id 6) (at 0 0 0))
      (symbol "D_TVS_0_1"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.508 1.27)
            (xy 0 1.27)
            (xy 0 -1.27)
            (xy -0.508 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.27)
            (xy -2.54 -1.27)
            (xy 2.54 1.27)
            (xy 2.54 -1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "D_TVS_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at 0.762 1.016 0))
      (property "Value" "L_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_Small_0_1"
        (arc (start 0 -2.032) (mid 0.508 -1.524) (end 0 -1.016)
          (fill (type none))
        )
        (arc (start 0 -1.016) (mid 0.508 -0.508) (end 0 0)
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.508 0.508) (end 0 1.016)
          (fill (type none))
        )
        (arc (start 0 1.016) (mid 0.508 1.524) (end 0 2.032)
          (fill (type none))
        )
      )
      (symbol "L_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.508)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.508)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Pack04" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at -7.62 0 90))
      (property "Value" "R_Pack04" (id 1) (at 5.08 0 90))
      (property "Footprint" "" (id 2) (at 6.985 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network parallel topology isolated" (id 4) (at 0 0 0))
      (property "ki_description" "4 resistor network, parallel topology" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* SOIC* R*Array*Concave* R*Array*Convex*" (id 6) (at 0 0 0))
      (symbol "R_Pack04_0_1"
        (rectangle (start -6.35 -2.413) (end 3.81 2.413)
          (fill (type background))
        )
        (rectangle (start -5.715 1.905) (end -4.445 -1.905)
          (fill (type none))
        )
        (rectangle (start -3.175 1.905) (end -1.905 -1.905)
          (fill (type none))
        )
        (rectangle (start -0.635 1.905) (end 0.635 -1.905)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 -2.54)
            (xy -5.08 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.08 1.905)
            (xy -5.08 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -2.54)
            (xy -2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 1.905)
            (xy -2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.905)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 2.54 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.905)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (rectangle (start 1.905 1.905) (end 3.175 -1.905)
          (fill (type none))
        )
      )
      (symbol "R_Pack04_1_1"
        (pin passive line (at -5.08 -5.08 90) (length 2.54)
          (name "R1.1")
          (number "1")
        )
        (pin passive line (at -2.54 -5.08 90) (length 2.54)
          (name "R2.1")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "R3.1")
          (number "3")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "R4.1")
          (number "4")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "R4.2")
          (number "5")
        )
        (pin passive line (at 0 5.08 270) (length 2.54)
          (name "R3.2")
          (number "6")
        )
        (pin passive line (at -2.54 5.08 270) (length 2.54)
          (name "R2.2")
          (number "7")
        )
        (pin passive line (at -5.08 5.08 270) (length 2.54)
          (name "R1.2")
          (number "8")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Bridged" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0))
      (property "Value" "SolderJumper_2_Bridged" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "solder jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Solder Jumper, 2-pole, closed/bridged" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Bridged*" (id 6) (at 0 0 0))
      (symbol "SolderJumper_2_Bridged_0_1"
        (rectangle (start -0.508 0.508) (end 0.508 -0.508)
          (fill (type outline))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Bridged_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "Jumper:SolderJumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0))
      (property "Value" "SolderJumper_2_Open" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "solder jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Solder Jumper, 2-pole, open" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Open*" (id 6) (at 0 0 0))
      (symbol "SolderJumper_2_Open_0_1"
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type none))
        )
        (arc (start -0.254 1.016) (mid -1.27 0) (end -0.254 -1.016)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -0.254 1.016)
            (xy -0.254 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.254 1.016)
            (xy 0.254 -1.016)
          )
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type none))
        )
        (arc (start 0.254 -1.016) (mid 1.27 0) (end 0.254 1.016)
          (fill (type outline))
        )
      )
      (symbol "SolderJumper_2_Open_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "RF_GPS:MAX-M8W" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -10.16 16.51 0))
      (property "Value" "MAX-M8W" (id 1) (at 12.7 16.51 0))
      (property "Footprint" "RF_GPS:ublox_MAX" (id 2) (at 10.16 -16.51 0))
      (property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-M8-FW3_DataSheet_%28UBX-15031506%29.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "ublox GPS GNSS module" (id 4) (at 0 0 0))
      (property "ki_description" "GNSS Module MAX M8, VCC 2.7V to 3.6V" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "ublox*MAX*" (id 6) (at 0 0 0))
      (symbol "MAX-M8W_0_1"
        (rectangle (start 12.7 15.24) (end -12.7 -15.24)
          (fill (type background))
        )
      )
      (symbol "MAX-M8W_1_1"
        (pin power_in line (at 0 -17.78 90) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin passive line (at 0 -17.78 90) (length 2.54) hide
          (name "GND")
          (number "10")
        )
        (pin input line (at 15.24 0 180) (length 2.54)
          (name "RF_IN")
          (number "11")
        )
        (pin passive line (at 0 -17.78 90) (length 2.54) hide
          (name "GND")
          (number "12")
        )
        (pin no_connect line (at 12.7 -5.08 180) (length 2.54) hide
          (name "Reserved")
          (number "13")
        )
        (pin power_out line (at 5.08 17.78 270) (length 2.54)
          (name "VCC_RF")
          (number "14")
        )
        (pin power_in line (at 2.54 17.78 270) (length 2.54)
          (name "V_ANT")
          (number "15")
        )
        (pin bidirectional line (at -15.24 2.54 0) (length 2.54)
          (name "SDA")
          (number "16")
        )
        (pin input line (at -15.24 0 0) (length 2.54)
          (name "SCL")
          (number "17")
        )
        (pin input line (at -15.24 -7.62 0) (length 2.54)
          (name "~{SAFEBOOT}")
          (number "18")
        )
        (pin output line (at -15.24 7.62 0) (length 2.54)
          (name "TXD")
          (number "2")
        )
        (pin input line (at -15.24 10.16 0) (length 2.54)
          (name "RXD")
          (number "3")
        )
        (pin output line (at 15.24 -7.62 180) (length 2.54)
          (name "TIMEPULSE")
          (number "4")
        )
        (pin input line (at -15.24 -5.08 0) (length 2.54)
          (name "EXTINT")
          (number "5")
        )
        (pin power_in line (at 0 17.78 270) (length 2.54)
          (name "V_BCKP")
          (number "6")
        )
        (pin power_in line (at -2.54 17.78 270) (length 2.54)
          (name "VCC_IO")
          (number "7")
        )
        (pin power_in line (at -5.08 17.78 270) (length 2.54)
          (name "VCC")
          (number "8")
        )
        (pin input line (at -15.24 -10.16 0) (length 2.54)
          (name "~{RESET}")
          (number "9")
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:PWR_FLAG" (power) (pin_numbers hide) (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "#FLG" (id 0) (at 0 1.905 0))
      (property "Value" "PWR_FLAG" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Special symbol for telling ERC where power comes from" (id 5) (at 0 0 0))
      (symbol "PWR_FLAG_0_0"
        (pin power_out line (at 0 0 90) (length 0)
          (name "pwr")
          (number "1")
        )
      )
      (symbol "PWR_FLAG_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 1.27)
            (xy -1.016 1.905)
            (xy 0 2.54)
            (xy 1.016 1.905)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
    )
  )
  (junction (at 203.2 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 119.38 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 96.52 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 88.9) (diameter 0) (color 0 0 0 0))
  (junction (at 50.8 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 210.82 99.06) (diameter 0) (color 0 0 0 0))
  (junction (at 111.76 58.42) (diameter 0) (color 0 0 0 0))
  (no_connect (at 116.84 101.6))
  (no_connect (at 116.84 104.14))
  (wire (pts (xy 144.78 88.9) (xy 139.7 88.9)))
  (wire (pts (xy 119.38 91.44) (xy 129.54 91.44)))
  (wire (pts (xy 111.76 58.42) (xy 119.38 58.42)))
  (wire (pts (xy 116.84 93.98) (xy 119.38 93.98)))
  (wire (pts (xy 203.2 88.9) (xy 203.2 99.06)))
  (wire (pts (xy 177.8 99.06) (xy 182.88 99.06)))
  (wire (pts (xy 106.68 55.88) (xy 106.68 58.42)))
  (wire (pts (xy 144.78 93.98) (xy 139.7 93.98)))
  (wire (pts (xy 127 93.98) (xy 129.54 93.98)))
  (wire (pts (xy 203.2 101.6) (xy 203.2 99.06)))
  (wire (pts (xy 101.6 114.3) (xy 101.6 116.84)))
  (wire (pts (xy 144.78 106.68) (xy 116.84 106.68)))
  (wire (pts (xy 81.28 104.14) (xy 81.28 127)))
  (wire (pts (xy 119.38 58.42) (xy 119.38 60.96)))
  (wire (pts (xy 203.2 109.22) (xy 203.2 111.76)))
  (wire (pts (xy 86.36 104.14) (xy 81.28 104.14)))
  (wire (pts (xy 50.8 111.76) (xy 50.8 116.84)))
  (wire (pts (xy 210.82 99.06) (xy 210.82 104.14)))
  (wire (pts (xy 101.6 58.42) (xy 101.6 78.74)))
  (wire (pts (xy 96.52 55.88) (xy 96.52 58.42)))
  (wire (pts (xy 71.12 96.52) (xy 86.36 96.52)))
  (wire (pts (xy 116.84 88.9) (xy 119.38 88.9)))
  (wire (pts (xy 200.66 88.9) (xy 203.2 88.9)))
  (wire (pts (xy 127 66.04) (xy 127 68.58)))
  (wire (pts (xy 210.82 96.52) (xy 210.82 99.06)))
  (wire (pts (xy 116.84 96.52) (xy 119.38 96.52)))
  (wire (pts (xy 198.12 99.06) (xy 203.2 99.06)))
  (wire (pts (xy 88.9 58.42) (xy 88.9 60.96)))
  (wire (pts (xy 88.9 66.04) (xy 88.9 68.58)))
  (wire (pts (xy 119.38 58.42) (xy 127 58.42)))
  (wire (pts (xy 119.38 88.9) (xy 119.38 91.44)))
  (wire (pts (xy 99.06 78.74) (xy 99.06 58.42)))
  (wire (pts (xy 121.92 88.9) (xy 121.92 86.36)))
  (wire (pts (xy 121.92 86.36) (xy 116.84 86.36)))
  (wire (pts (xy 203.2 99.06) (xy 210.82 99.06)))
  (wire (pts (xy 106.68 58.42) (xy 111.76 58.42)))
  (wire (pts (xy 104.14 78.74) (xy 104.14 76.2)))
  (wire (pts (xy 104.14 76.2) (xy 106.68 76.2)))
  (wire (pts (xy 50.8 104.14) (xy 50.8 96.52)))
  (wire (pts (xy 111.76 58.42) (xy 111.76 60.96)))
  (wire (pts (xy 96.52 58.42) (xy 88.9 58.42)))
  (wire (pts (xy 81.28 127) (xy 144.78 127)))
  (wire (pts (xy 177.8 88.9) (xy 193.04 88.9)))
  (wire (pts (xy 38.1 96.52) (xy 50.8 96.52)))
  (wire (pts (xy 106.68 76.2) (xy 106.68 78.74)))
  (wire (pts (xy 127 96.52) (xy 129.54 96.52)))
  (wire (pts (xy 50.8 96.52) (xy 71.12 96.52)))
  (wire (pts (xy 96.52 58.42) (xy 96.52 60.96)))
  (wire (pts (xy 71.12 76.2) (xy 71.12 86.36)))
  (wire (pts (xy 127 58.42) (xy 127 60.96)))
  (wire (pts (xy 71.12 76.2) (xy 96.52 76.2)))
  (wire (pts (xy 144.78 96.52) (xy 139.7 96.52)))
  (wire (pts (xy 71.12 91.44) (xy 71.12 96.52)))
  (wire (pts (xy 177.8 88.9) (xy 177.8 99.06)))
  (wire (pts (xy 144.78 91.44) (xy 139.7 91.44)))
  (wire (pts (xy 193.04 99.06) (xy 187.96 99.06)))
  (wire (pts (xy 119.38 66.04) (xy 119.38 68.58)))
  (wire (pts (xy 177.8 83.82) (xy 177.8 88.9)))
  (wire (pts (xy 96.52 76.2) (xy 96.52 78.74)))
  (wire (pts (xy 96.52 76.2) (xy 96.52 66.04)))
  (wire (pts (xy 210.82 109.22) (xy 210.82 111.76)))
  (wire (pts (xy 210.82 99.06) (xy 226.06 99.06)))
  (wire (pts (xy 111.76 66.04) (xy 111.76 68.58)))
  (wire (pts (xy 129.54 88.9) (xy 121.92 88.9)))
  (wire (pts (xy 99.06 58.42) (xy 96.52 58.42)))
  (wire (pts (xy 106.68 58.42) (xy 106.68 76.2)))
  (text "For M8W:\n - Place C & R between\n   Vcc_RF and V_ant\n\nFor ATGM336H:\n - Place the bias inductor\n"
    (at 53.34 71.12 0)
  )
  (text "Battery and charging circuit\nis DNP by default" (at 210.82 88.9 0))
  (label "vbackup" (at 101.6 58.42 270))
  (label "vbackup" (at 226.06 99.06 180))
  (hierarchical_label "i2c_sda" (shape bidirectional) (at 144.78 93.98 0))
  (hierarchical_label "rx" (shape input) (at 144.78 88.9 0))
  (hierarchical_label "i2c_scl" (shape bidirectional) (at 144.78 96.52 0))
  (hierarchical_label "~{reset}" (shape input) (at 144.78 106.68 0))
  (hierarchical_label "RF" (shape input) (at 38.1 96.52 180))
  (hierarchical_label "tx" (shape output) (at 144.78 91.44 0))
  (hierarchical_label "pps" (shape output) (at 144.78 127 0))
  (symbol (lib_id "RF_GPS:MAX-M8W") (at 101.6 96.52 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U8" (id 0) (at 114.3 114.3 0))
    (property "Value" "MAX-M8W" (id 1) (at 111.76 116.84 0))
    (property "Footprint" "s47-misc:ublox_MAX" (id 2) (at 91.44 113.03 0))
    (property "Datasheet" "https://www.u-blox.com/sites/default/files/MAX-M8-FW3_DataSheet_%28UBX-15031506%29.pdf" (id 3) (at 101.6 96.52 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 101.6 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR046" (id 0) (at 101.6 123.19 0))
    (property "Value" "GND" (id 1) (at 101.727 121.2342 0))
    (property "Footprint" "" (id 2) (at 101.6 116.84 0))
    (property "Datasheet" "" (id 3) (at 101.6 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 119.38 63.5 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C23" (id 0) (at 121.7168 62.3316 0))
    (property "Value" "100n" (id 1) (at 121.7168 64.643 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 119.38 63.5 0))
    (property "Datasheet" "~" (id 3) (at 119.38 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Small") (at 71.12 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L1" (id 0) (at 72.3392 87.7316 0))
    (property "Value" "47n" (id 1) (at 72.3392 90.043 0))
    (property "Footprint" "Inductor_SMD:L_0402_1005Metric" (id 2) (at 71.12 88.9 0))
    (property "Datasheet" "~" (id 3) (at 71.12 88.9 0))
    (property "MPN" "Murata LQW15AN47NG00D" (id 4) (at 71.12 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V3") (at 106.68 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR047" (id 0) (at 106.68 59.69 0))
    (property "Value" "+3V3" (id 1) (at 107.061 51.4858 0))
    (property "Footprint" "" (id 2) (at 106.68 55.88 0))
    (property "Datasheet" "" (id 3) (at 106.68 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 127 63.5 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C24" (id 0) (at 129.3368 62.3316 0))
    (property "Value" "1u" (id 1) (at 129.3368 64.643 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 127 63.5 0))
    (property "Datasheet" "~" (id 3) (at 127 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 111.76 63.5 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C22" (id 0) (at 114.0968 62.3316 0))
    (property "Value" "100n" (id 1) (at 114.0968 64.643 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 111.76 63.5 0))
    (property "Datasheet" "~" (id 3) (at 111.76 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 111.76 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR048" (id 0) (at 111.76 74.93 0))
    (property "Value" "GND" (id 1) (at 111.887 72.9742 0))
    (property "Footprint" "" (id 2) (at 111.76 68.58 0))
    (property "Datasheet" "" (id 3) (at 111.76 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 119.38 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR049" (id 0) (at 119.38 74.93 0))
    (property "Value" "GND" (id 1) (at 119.507 72.9742 0))
    (property "Footprint" "" (id 2) (at 119.38 68.58 0))
    (property "Datasheet" "" (id 3) (at 119.38 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 127 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR050" (id 0) (at 127 74.93 0))
    (property "Value" "GND" (id 1) (at 127.127 72.9742 0))
    (property "Footprint" "" (id 2) (at 127 68.58 0))
    (property "Datasheet" "" (id 3) (at 127 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 96.52 63.5 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R18" (id 0) (at 95.0214 61.1886 0))
    (property "Value" "10R" (id 1) (at 95.0214 63.5 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 96.52 63.5 0))
    (property "Datasheet" "~" (id 3) (at 96.52 63.5 0))
    (property "DNP" "DNP" (id 4) (at 95.0214 65.8114 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C_Small") (at 88.9 63.5 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C21" (id 0) (at 86.5632 61.1886 0))
    (property "Value" "100n" (id 1) (at 86.5632 63.5 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 88.9 63.5 0))
    (property "Datasheet" "~" (id 3) (at 88.9 63.5 0))
    (property "DNP" "DNP" (id 4) (at 86.5632 65.8114 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 88.9 68.58 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR045" (id 0) (at 88.9 74.93 0))
    (property "Value" "GND" (id 1) (at 89.027 72.9742 0))
    (property "Footprint" "" (id 2) (at 88.9 68.58 0))
    (property "Datasheet" "" (id 3) (at 88.9 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Battery_Cell") (at 203.2 106.68 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "BT1" (id 0) (at 200.2282 103.0986 0))
    (property "Value" "VL-1220/VCN" (id 1) (at 200.2282 105.41 0))
    (property "Footprint" "Battery:Battery_Panasonic_CR1220-VCN_Vertical_CircularHoles" (id 2) (at 203.2 105.156 90))
    (property "Datasheet" "~" (id 3) (at 203.2 105.156 90))
    (property "DNP" "DNP" (id 4) (at 200.2282 107.7214 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 203.2 111.76 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR052" (id 0) (at 203.2 118.11 0))
    (property "Value" "GND" (id 1) (at 203.327 116.1542 0))
    (property "Footprint" "" (id 2) (at 203.2 111.76 0))
    (property "Datasheet" "" (id 3) (at 203.2 111.76 0))
    (pin "1")
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Bridged") (at 196.85 88.9 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP1" (id 0) (at 196.85 83.5152 0))
    (property "Value" "BatBypass" (id 1) (at 196.85 85.8266 0))
    (property "Footprint" "s47-misc:J_NC_0603_30" (id 2) (at 196.85 88.9 0))
    (property "Datasheet" "~" (id 3) (at 196.85 88.9 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3V3") (at 177.8 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR051" (id 0) (at 177.8 87.63 0))
    (property "Value" "+3V3" (id 1) (at 178.181 79.4258 0))
    (property "Footprint" "" (id 2) (at 177.8 83.82 0))
    (property "Datasheet" "" (id 3) (at 177.8 83.82 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Small") (at 210.82 106.68 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C25" (id 0) (at 213.1568 105.5116 0))
    (property "Value" "100n" (id 1) (at 213.1568 107.823 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 210.82 106.68 0))
    (property "Datasheet" "~" (id 3) (at 210.82 106.68 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 210.82 111.76 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR053" (id 0) (at 210.82 118.11 0))
    (property "Value" "GND" (id 1) (at 210.947 116.1542 0))
    (property "Footprint" "" (id 2) (at 210.82 111.76 0))
    (property "Datasheet" "" (id 3) (at 210.82 111.76 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small") (at 195.58 99.06 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R19" (id 0) (at 195.58 91.7956 90))
    (property "Value" "330R" (id 1) (at 195.58 94.107 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 195.58 99.06 0))
    (property "Datasheet" "~" (id 3) (at 195.58 99.06 0))
    (property "DNP" "DNP" (id 4) (at 195.58 96.4184 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D_Schottky_Small") (at 185.42 99.06 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D4" (id 0) (at 185.42 91.567 0))
    (property "Value" "SDM02U30LP3" (id 1) (at 185.42 93.8784 0))
    (property "Footprint" "Diode_SMD:D_0603_1608Metric" (id 2) (at 185.42 99.06 90))
    (property "Datasheet" "~" (id 3) (at 185.42 99.06 90))
    (property "DNP" "DNP" (id 4) (at 185.42 96.1898 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:D_TVS") (at 50.8 107.95 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D3" (id 0) (at 52.8066 106.7816 90))
    (property "Value" "PESD0402-140" (id 1) (at 52.8066 109.093 90))
    (property "Footprint" "Diode_SMD:D_0402_1005Metric" (id 2) (at 50.8 107.95 0))
    (property "Datasheet" "~" (id 3) (at 50.8 107.95 0))
    (property "MPN" "Little Fuse PESD0402-140" (id 4) (at 50.8 107.95 90))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 50.8 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR044" (id 0) (at 50.8 123.19 0))
    (property "Value" "GND" (id 1) (at 50.927 121.2342 0))
    (property "Footprint" "" (id 2) (at 50.8 116.84 0))
    (property "Datasheet" "" (id 3) (at 50.8 116.84 0))
    (pin "1")
  )
  (symbol (lib_id "power:PWR_FLAG") (at 210.82 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#FLG03" (id 0) (at 210.82 94.615 0))
    (property "Value" "PWR_FLAG" (id 1) (at 210.82 92.1258 0))
    (property "Footprint" "" (id 2) (at 210.82 96.52 0))
    (property "Datasheet" "~" (id 3) (at 210.82 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "power:PWR_FLAG") (at 96.52 55.88 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#FLG02" (id 0) (at 96.52 53.975 0))
    (property "Value" "PWR_FLAG" (id 1) (at 96.52 51.4858 0))
    (property "Footprint" "" (id 2) (at 96.52 55.88 0))
    (property "Datasheet" "~" (id 3) (at 96.52 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04") (at 134.62 93.98 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN6" (id 0) (at 134.62 83.3882 90))
    (property "Value" "33R" (id 1) (at 134.62 85.6996 90))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x0603" (id 2) (at 134.62 100.965 90))
    (property "Datasheet" "~" (id 3) (at 134.62 93.98 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 123.19 93.98 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP2" (id 0) (at 128.27 92.71 0))
    (property "Value" "GPS SDA" (id 1) (at 123.19 91.9281 0))
    (property "Footprint" "s47-misc:J_0402" (id 2) (at 123.19 93.98 0))
    (property "Datasheet" "~" (id 3) (at 123.19 93.98 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:SolderJumper_2_Open") (at 123.19 96.52 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP3" (id 0) (at 128.27 95.25 0))
    (property "Value" "GPS SCL" (id 1) (at 123.19 94.4681 0))
    (property "Footprint" "s47-misc:J_0402" (id 2) (at 123.19 96.52 0))
    (property "Datasheet" "~" (id 3) (at 123.19 96.52 0))
    (pin "1")
    (pin "2")
  )
)
