/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               SGmbInterface_3GPP_TS29061_980.ddf
//  Description:        DDF for SGmb according to 3GPP TS 29.061 V9.8.0
//  Rev:                R13A04
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: SGMB
// APPLICATION-REVISION: V9_8_0

// AVP implementations according to: 
// 3GPP TS 29.061 V9.8.0 - Interworking between the Public Land Mobile Network (PLMN) supporting packet based services and Packet Data Networks (PDN)

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-Access-Indicator (923) 3GPP (10415)
// 20.5a.1
type enumerated MBMS_Access_Indicator
{
  UTRAN                 (0),
  E_UTRAN               (1),
  UTRAN_AND_E_UTRAN     (2)
}

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GW-SSM-IP-Address (924) 3GPP (10415)
// 20.5a.2
type AVP_OctetString MBMS_GW_SSM_IP_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GW-SSM-IPv6-Address (925) 3GPP (10415)
// 20.5a.3
type AVP_OctetString MBMS_GW_SSM_IPv6_Address;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-BMSC-SSM-UDP-Port (926) 3GPP (10415)
// 20.5a.4
type AVP_OctetString MBMS_BMSC_SSM_UDP_Port;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GW-UDP-Port (927) 3GPP (10415)
// 20.5a.5
type AVP_OctetString MBMS_GW_UDP_Port;

// 3GPP TS 29.061 V9.8.0
// AVP: MBMS-GW-UDP-Port-Indicator (928) 3GPP (10415) 
// 20.5a.6
type enumerated MBMS_GW_UDP_Port_Indicator
{
  UDP_PORT_REQUIRED (1)
}
