/**
*    @author   ETSI / TTF041
*    @version  $URL$
*              $Id$
*    @desc     This module provides PICS for NGAP tests.
*    @copyright   ETSI Copyright Notification
*                 No part may be reproduced except as authorized by written permission.
*                 The copyright and the foregoing restriction extend to reproduction in all media.
*                 All rights reserved.
*    @see      ETSI TS 
*/
module Lib_NG_NAS_Pixits {

    import from CommonDefs all;
    import from NAS_CommonTypeDefs all;

    modulepar B4_Type PX_SUPI_FORMAT := '0000'B;

    modulepar octetstring PX_SUPI_DIGITS := '00f110214300014444330302'O;

    modulepar O16_Type PX_USIM_OPERATOR_VARIANT_ALGORITHM_CONFIGURATION := '00000000000000000000000000000000'O;

    modulepar B128_Type PX_USIM_SECRET_KEY := oct2bit('00000000000000000000000000000000'O);

    modulepar NAS_PlmnId PX_PLMN := '000000'O;

} // End of module Lib_NG_NAS_Pixits