/**
*    @author   ETSI / TTF033
*    @version  $URL$
*              $Id$
*    @desc     This module provides PIXITs for NGAP tests.
*    @copyright   ETSI Copyright Notification
*                 No part may be reproduced except as authorized by written permission.
*                 The copyright and the foregoing restriction extend to reproduction in all media.
*                 All rights reserved.
*    @see      ETSI TS 
*/
module NGAP_Pixits {

    //  LibCommon
    import from LibCommon_BasicTypesAndValues all;
    import from LibCommon_DataStrings all;

    // LibNGAP
    import from NGAP_CommonDataTypes language "ASN.1:1997" all;
    import from NGAP_IEs language "ASN.1:2002" all;

    group NGAP_Port_and_addresses {

        group NGAP_TS_Port_and_addresses {

            /** @desc    
             * IP address of the test system
             */
            modulepar charstring PX_NGAP_ETS_IPADDR := "1.1.1.10";

            /** @desc    
             * Port number of the test system
             */
            modulepar integer PX_NGAP_ETS_PORT := 3868;

            /** @desc    
             * IP address of the test system
             */
            modulepar charstring PX_NGAP_ETS_IPADDR2 := "1.1.1.13";

            /** @desc    
             * Port number of the test system
             */
            modulepar integer PX_NGAP_ETS_PORT2 := 3868;


        } // End of group NGAP_TS_Port_and_addresses

        group NGAP_SUT_Port_and_addresses {

            /** @desc    
             * IP address of the system under test
             */
            modulepar charstring PX_NGAP_SUT_IPADDR := "1.1.2.10";

            /** @desc   
             * Port number of the system under test
             */
            modulepar integer PX_NGAP_SUT_PORT := 3868;

        } // End of group NGAP_SUT_Port_and_addresses{

    } // End of group NGAP_Port_and_addresses

    group NGAP_CommonData {

        /** 
         * @desc    integer for variant selection, 
         * @see ETSI 
         */
        modulepar integer PX_VA := 1;

        /**
         * @desc Variant for Criticality values
         */
        modulepar Criticality PX_VA_CRITICALITY := reject;

      /** 
        * @desc    integer for timer TNGRELOCOverall, 
        * @see ETSI  TS 138 413, chapter 9.6
        */
        modulepar float PX_TNGRELOCOverall := 10.0;

    } // End of group NGAP_CommonData

} // End of module NGAP_Pixits
