/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Timea Moder
******************************************************************************/
//
//  File:               SGmbInterface_3GPP_TS29061_b90.ddf
//  Description:        DDF for SGmb according to 3GPP TS 29.061 V11.9.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: SGMB
// APPLICATION-REVISION: V11_9_0

// AVP implementations according to: 
// 3GPP TS 29.061 V11.9.0 - Interworking between the Public Land Mobile Network (PLMN) supporting packet based services and Packet Data Networks (PDN)

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-Access-Indicator (923) 3GPP (10415)
// 20.5a.1
type enumerated MBMS_Access_Indicator
{
  UTRAN                 (0),
  E_UTRAN               (1),
  UTRAN_AND_E_UTRAN     (2)
}

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-GW-SSM-IP-Address (924) 3GPP (10415)
// 20.5a.2
type AVP_OctetString MBMS_GW_SSM_IP_Address;

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-GW-SSM-IPv6-Address (925) 3GPP (10415)
// 20.5a.3
type AVP_OctetString MBMS_GW_SSM_IPv6_Address;

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-BMSC-SSM-UDP-Port (926) 3GPP (10415)
// 20.5a.4
type AVP_OctetString MBMS_BMSC_SSM_UDP_Port;

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-GW-UDP-Port (927) 3GPP (10415)
// 20.5a.5
type AVP_OctetString MBMS_GW_UDP_Port;

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-GW-UDP-Port-Indicator (928) 3GPP (10415) 
// 20.5a.6
type enumerated MBMS_GW_UDP_Port_Indicator
{
  UDP_PORT_REQUIRED (1)
}

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-Data-Transfer-Start (929) 3GPP (10415)
// 20.5a.7
type AVP_Unsigned64 MBMS_Data_Transfer_Start;

// 3GPP TS 29.061 V11.9.0
// AVP: MBMS-Data-Transfer-Stop (930) 3GPP (10415)
// 20.5a.8
type AVP_Unsigned64 MBMS_Data_Transfer_Stop;
