--  Reference:          3GPP TS 29.002 10.6.0

MAP-PDU-Defs 

DEFINITIONS IMPLICIT TAGS ::=

BEGIN

IMPORTS

      Supported-MAP-Operations
      FROM
      MAP-Protocol



  OPERATION, ERROR
    FROM Remote-Operations-Information-Objects {joint-iso-itu-t
      remote-operations(4) informationObjects(5) version1(0)}
	  
  Invoke{}, ReturnResult{}, ReturnError{},
  Invoke-help{}, ReturnResult-help{}, ReturnError-help{},
  Errors{}, PresentInvokeId
	FROM Remote-Operations-Generic-ROS-PDUs {joint-iso-itu-t
	  remote-operations(4) generic-ROS-PDUs(6) version1(0)};


-- MAP Invoke, ReturnResult, ReturnError types
-- (these are accessible from TTCN3)

MAP-Invoke ::= Invoke{{PresentInvokeId}, {Supported-MAP-Operations}}

MAP-ReturnResult ::= ReturnResult{{Supported-MAP-Operations}}

MAP-ReturnError ::= ReturnError{{Errors {{Supported-MAP-Operations}}}}

MAP-Invoke-help ::= Invoke-help{{PresentInvokeId}, {Supported-MAP-Operations}}

MAP-ReturnResult-help ::= ReturnResult-help{{Supported-MAP-Operations}}

MAP-ReturnError-help ::= ReturnError-help{{Errors {{Supported-MAP-Operations}}}}

END
