/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               AAAInterface_3GPP_TS29272_940.ddf
//  Description:        DDF for S6a/S6d and S13 Interfaces according to 3GPP TS 29.272 V9.4.0
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////


// APPLICATION-NAME: AAA
// APPLICATION-REVISION: V9_4_0

// AVP implementations according to: 
// 3GPP TS 29.272 V9.4.0 - Evolved Packet System (EPS); Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) related interfaces based on Diameter protocol

// 3GPP TS 29.272 V9.4.0
// 7.3.27
// AVP: Context-Identifier (1423) 3GPP (10415)
type AVP_Unsigned32 Context_Identifier

// 3GPP TS 29.272 V9.4.0
// 7.3.37
// AVP: EPS-Subscribed-QoS-Profile (1431) 3GPP (10415)
type AVP_Grouped EPS_Subscribed_QoS_Profile

// 3GPP TS 29.272 V9.4.0
// 7.3.41
// AVP: AMBR (1435) 3GPP (10415)
type AVP_Grouped AMBR

// 3GPP TS 29.272 V9.4.0
// 7.3.62
// AVP: PDN-Type (1456) 3GPP (10415)
type enumerated PDN_Type
{
  IPv4 (0),
  IPv6 (1),
  IPv4v6 (2),
  IPv4_OR_IPv6 (3)  
}
