/******************************************************************************
* Copyright (c) 2000-2019 Ericsson Telecom AB
* All rights reserved. This program and the accompanying materials
* are made available under the terms of the Eclipse Public License v2.0
* which accompanies this distribution, and is available at
* https://www.eclipse.org/org/documents/epl-2.0/EPL-2.0.html
*
* Contributors:
*   Roland Gecse - initial implementation and initial documentation
*   Akos Pernek
*   Antal Wuh.Hen.Chang
*   Attila Fulop
*   Balazs Barcsik
*   Bence Molnar
*   Csaba Koppany
*   David Juhasz
*   Eduard Czimbalmos
*   Elemer Lelik
*   Endre Kiss
*   Endre Kulcsar
*   Gabor Szalai
*   Gabor Tatarka
*   Gergely Futo
*   Istvan Sandor
*   Krisztian Pandi
*   Kulcsár Endre
*   Laszlo Tamas Zeke
*   Norbert Pinter
*   Roland Gecse
*   Tibor Bende
*   Tibor Szabo
*   Timea Moder
*   Zoltan Medve
*   Zsolt Nandor Torok
*   Zsolt Szalai
******************************************************************************/
//
//  File:               Vimpelcom_Specific.ddf
//  Description:        Vimpelcom specific AVPs
//  Rev:                R55A
//  Prodnr:             CNL 113 462
///////////////////////////////////////////////

// APPLICATION-NAME: VIMP
// APPLICATION-REVISION:


// AVP: DPI-flow-identity (660) Vimpelcom_sadpi (50000)
type AVP_OctetString DPI_flow_identity;

// AVP: DPI-DSCP-Mark (661) Vimpelcom_sadpi (50000)
type AVP_Unsigned32 DPI_DSCP_Mark;

// AVP: DPI-Traffic-Priority (662) Vimpelcom_sadpi (50000)
type AVP_Unsigned32 DPI_Traffic_Priority;

// AVP: DPI-VoIP-Alteration (663) Vimpelcom_sadpi (50000)
type AVP_Unsigned32 DPI_VoIP_Alteration;

// AVP: DPI-Redirect-ID (664) Vimpelcom_sadpi (50000)
type AVP_Grouped DPI_Redirect_ID;

// AVP: TOA-Termination-Flag (665) Vimpelcom_toa (50001)
type AVP_Unsigned32 TOA_Termination_Flag;

// AVP: TOA-Adapt-Status (666) Vimpelcom_toa (50001)
type AVP_Unsigned32 TOA_Adapt_Status;

// AVP: TOA-Opt-Status (667) Vimpelcom_toa (50001)
type AVP_Unsigned32 TOA_Opt_Status;

// AVP: DPI-Specific-Flow-Id (668) Vimpelcom_sadpi (50000)
type AVP_OctetString DPI_Specific_Flow_Id;

// AVP: DPI-Flow-Info (669) Vimpelcom_sadpi (50000)
type AVP_Grouped DPI_Flow_Info;

