--  Reference:          3GPP TS 29.002 10.6.0

MAP-CommonDataTypes {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-CommonDataTypes (18) version13 (13)}

DEFINITIONS

IMPLICIT TAGS

::=

BEGIN

EXPORTS

	-- general data types and values
	AddressString,
	ISDN-AddressString,
	maxISDN-AddressLength,
	FTN-AddressString,
	ISDN-SubaddressString,
	ExternalSignalInfo, 
	Ext-ExternalSignalInfo, 
AccessNetworkSignalInfo,
	SignalInfo,
	maxSignalInfoLength,
	AlertingPattern,
	TBCD-STRING,
	DiameterIdentity,
	Time,

	-- data types for numbering and identification
	IMSI,
	IMSI-MAP,  -- for compatibility with CAP v7.3.0		
	TMSI, 
	Identity,
	SubscriberId,
	IMEI,
	IMEI-MAP,  -- for compatibility with CAP v7.3.0	
	HLR-List,
	LMSI,
	GlobalCellId,
	NetworkResource,
	AdditionalNetworkResource,
	NAEA-PreferredCI, 
	NAEA-CIC, 
	ASCI-CallReference,
	SubscriberIdentity,
	PLMN-Id,
	E-UTRAN-CGI,
	TA-Id,
	RAIdentity,

	-- data types for CAMEL
	CellGlobalIdOrServiceAreaIdOrLAI, 
	CellGlobalIdOrServiceAreaIdFixedLength,
	LAIFixedLength,

	-- data types for subscriber management
	BasicServiceCode,
	Ext-BasicServiceCode,
	EMLPP-Info,
	EMLPP-Priority, 
	MC-SS-Info,
	MaxMC-Bearers,
	MC-Bearers,
	Ext-SS-Status,

	-- data types for geographic location
	AgeOfLocationInformation,
	LCSClientExternalID,
	LCSClientInternalID,
	LCSServiceTypeID,

	-- gprs location registration types
	GSN-Address

;

IMPORTS
	TeleserviceCode,
	Ext-TeleserviceCode
FROM MAP-TS-Code {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-TS-Code (19) version13 (13)}

	BearerServiceCode,
	Ext-BearerServiceCode
FROM MAP-BS-Code {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-BS-Code (20) version13 (13)}

	SS-Code
FROM MAP-SS-Code {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-SS-Code (15) version13 (13)}

	ExtensionContainer
FROM MAP-ExtensionDataTypes {
   itu-t identified-organization (4) etsi (0) mobileDomain (0)
   gsm-Network (1) modules (3) map-ExtensionDataTypes (21) version13 (13)}
;


-- general data types

TBCD-STRING ::= OCTET STRING
	-- This type (Telephony Binary Coded Decimal String) is used to
	-- represent several digits from 0 through 9, *, #, a, b, c, two
	-- digits per octet, each digit encoded 0000 to 1001 (0 to 9),
	-- 1010 (*), 1011 (#), 1100 (a), 1101 (b) or 1110 (c); 1111 used
	-- as filler when there is an odd number of digits.

	-- bits 8765 of octet n encoding digit 2n
	-- bits 4321 of octet n encoding digit 2(n-1) +1

DiameterIdentity ::= OCTET STRING (SIZE(9..55))
-- content of DiameterIdentity is defined in IETF RFC 3588 [139]

AddressString ::= OCTET STRING (SIZE (1..maxAddressLength))
	-- This type is used to represent a number for addressing
	-- purposes. It is composed of
	--	a)	one octet for nature of address, and numbering plan
	--		indicator.
	--	b)	digits of an address encoded as TBCD-String.

	-- a)	The first octet includes a one bit extension indicator, a
	--		3 bits nature of address indicator and a 4 bits numbering
	--		plan indicator, encoded as follows:

	-- bit 8: 1  (no extension)

	-- bits 765: nature of address indicator
	--	000  unknown
	--	001  international number
	--	010  national significant number
	--	011  network specific number
	--	100  subscriber number
	--	101  reserved
	--	110  abbreviated number
	--	111  reserved for extension

	-- bits 4321: numbering plan indicator
	--	0000  unknown
	--	0001  ISDN/Telephony Numbering Plan (Rec ITU-T E.164)
	--	0010  spare
	--	0011  data numbering plan (ITU-T Rec X.121)
	--	0100  telex numbering plan (ITU-T Rec F.69)
	--	0101  spare
	--	0110  land mobile numbering plan (ITU-T Rec E.212)
	--	0111  spare
	--	1000  national numbering plan
	--	1001  private numbering plan
	--	1111  reserved for extension

	--	all other values are reserved.

	-- b)	The following octets representing digits of an address
	--		encoded as a TBCD-STRING.

maxAddressLength  INTEGER ::= 20

ISDN-AddressString ::= 
			AddressString (SIZE (1..maxISDN-AddressLength))
	-- This type is used to represent ISDN numbers.

maxISDN-AddressLength  INTEGER ::= 9

FTN-AddressString ::= 
			AddressString (SIZE (1..maxFTN-AddressLength))
	-- This type is used to represent forwarded-to numbers. 
	-- If NAI = international the first digits represent the country code (CC)
	-- and the network destination code (NDC) as for E.164.

maxFTN-AddressLength  INTEGER ::= 15

ISDN-SubaddressString ::= 
			OCTET STRING (SIZE (1..maxISDN-SubaddressLength))
	-- This type is used to represent ISDN subaddresses.
	-- It is composed of
	--	a)	one octet for type of subaddress and odd/even indicator.
	--	b)	20 octets for subaddress information.

	--	a)	The first octet includes a one bit extension indicator, a
	--		3 bits type of subaddress and a one bit odd/even indicator,
	--		encoded as follows:

	--	bit 8: 1  (no extension)

	--	bits 765: type of subaddress
	--		000  NSAP (X.213/ISO 8348 AD2)
	--		010  User Specified
	--		All other values are reserved

	--	bit 4: odd/even indicator
	--		0  even number of address signals
	--		1  odd number of address signals
	--		The odd/even indicator is used when the type of subaddress
	--		is "user specified" and the coding is BCD.

	--	bits 321: 000 (unused)

	--	b) Subaddress information.
	--	The NSAP X.213/ISO8348AD2 address shall be formatted as specified
	--	by octet 4 which contains the Authority and Format Identifier
	--	(AFI). The encoding is made according to the "preferred binary
	--	encoding" as defined in X.213/ISO834AD2. For the definition
	--	of this type of subaddress, see ITU-T Rec I.334.

	--	For User-specific subaddress, this field is encoded according
	--	to the user specification, subject to a maximum length of 20
	--	octets. When interworking with X.25 networks BCD coding should
	--	be applied.

maxISDN-SubaddressLength  INTEGER ::= 21

ExternalSignalInfo ::= SEQUENCE {
	protocolId	ProtocolId,
	signalInfo	SignalInfo,
	-- Information about the internal structure is given in
	-- clause 7.6.9.
	extensionContainer	ExtensionContainer	OPTIONAL,
	-- extensionContainer must not be used in version 2
	...}

SignalInfo ::= OCTET STRING (SIZE (1..maxSignalInfoLength))

maxSignalInfoLength  INTEGER ::= 200
	-- This NamedValue represents the theoretical maximum number of octets which is
	-- available to carry a single instance of the SignalInfo data type,
	-- without requiring segmentation to cope with the network layer service.
	-- However, the actual maximum size available for an instance of the data
	-- type may be lower, especially when other information elements
	-- have to be included in the same component.

ProtocolId ::= ENUMERATED {
	gsm-0408  (1),
	gsm-0806  (2),
	gsm-BSSMAP  (3),
	-- Value 3 is reserved and must not be used
	ets-300102-1  (4)}

Ext-ExternalSignalInfo ::= SEQUENCE {
	ext-ProtocolId	Ext-ProtocolId,
	signalInfo	SignalInfo,
	-- Information about the internal structure is given in
	-- clause 7.6.9.10
	extensionContainer	ExtensionContainer	OPTIONAL,
	...}

Ext-ProtocolId ::= ENUMERATED {
	ets-300356  (1),
	... 
	 }
-- exception handling:
-- For Ext-ExternalSignalInfo sequences containing this parameter with any
-- other value than the ones listed the receiver shall ignore the whole 
-- Ext-ExternalSignalInfo sequence.

AccessNetworkSignalInfo ::= SEQUENCE {
	accessNetworkProtocolId	AccessNetworkProtocolId,
	signalInfo	LongSignalInfo,
	-- Information about the internal structure is given in clause 7.6.9.1
	
	extensionContainer	ExtensionContainer	OPTIONAL,
	...}

LongSignalInfo ::= OCTET STRING (SIZE (1..maxLongSignalInfoLength))

maxLongSignalInfoLength  INTEGER ::= 2560
	-- This Named Value represents the maximum number of octets which is available
	-- to carry a single instance of the LongSignalInfo data type using
	-- White Book SCCP with the maximum number of segments.
	-- It takes account of the octets used by the lower layers of the protocol, and
	-- other information elements which may be included in the same component.

AccessNetworkProtocolId ::= ENUMERATED {
	ts3G-48006   (1),
	ts3G-25413 (2),
	...}
	-- exception handling:
	-- For AccessNetworkSignalInfo sequences containing this parameter with any
	-- other value than the ones listed the receiver shall ignore the whole 
	-- AccessNetworkSignalInfo sequence.

AlertingPattern ::= OCTET STRING (SIZE (1) )
	-- This type is used to represent Alerting Pattern

	--	bits 8765 : 0000 (unused)

	--	bits 43 : type of Pattern
	--		00 level
	--		01 category
	--		10 category
	--		all other values are reserved.

	--	bits 21 : type of alerting

alertingLevel-0   AlertingPattern ::= '00000000'B
alertingLevel-1   AlertingPattern ::= '00000001'B
alertingLevel-2   AlertingPattern ::= '00000010'B
	-- all other values of Alerting level are reserved
	-- Alerting Levels are defined in GSM 02.07
	
alertingCategory-1   AlertingPattern ::= '00000100'B
alertingCategory-2   AlertingPattern ::= '00000101'B
alertingCategory-3   AlertingPattern ::= '00000110'B
alertingCategory-4   AlertingPattern ::= '00000111'B
alertingCategory-5   AlertingPattern ::= '00001000'B
	-- all other values of Alerting Category are reserved
	-- Alerting categories are defined in GSM 02.07

GSN-Address ::= OCTET STRING (SIZE (5..17))
	-- Octets are coded according to TS 3GPP TS 23.003 [17]

Time ::= OCTET STRING (SIZE (4))
	-- Octets are coded according to IETF RFC 3588 [139]


-- data types for numbering and identification

IMSI ::= TBCD-STRING (SIZE (3..8))
	-- digits of MCC, MNC, MSIN are concatenated in this order.
	
IMSI-MAP ::= IMSI -- for compatibility with CAP v7.3.0		

Identity ::= CHOICE {
	imsi			IMSI,
	imsi-WithLMSI	IMSI-WithLMSI}

IMSI-WithLMSI ::= SEQUENCE {
	imsi			IMSI,
	lmsi			LMSI,
	-- a special value 00000000 indicates that the LMSI is not in use
	...}

ASCI-CallReference ::= TBCD-STRING (SIZE (1..8))
	-- digits of VGCS/VBS-area,Group-ID are concatenated in this order if there is a
	-- VGCS/VBS-area.

TMSI ::= OCTET STRING (SIZE (1..4))

SubscriberId ::= CHOICE {
	imsi			[0] IMSI,
	tmsi			[1] TMSI}

IMEI ::= TBCD-STRING (SIZE (8))
	--	Refers to International Mobile Station Equipment Identity
	--	and Software Version Number (SVN) defined in TS 3GPP TS 23.003 [17].
	--	If the SVN is not present the last octet shall contain the
	--	digit 0 and a filler.
	--	If present the SVN shall be included in the last octet.

IMEI-MAP ::= IMEI   -- for compatibility with CAP v7.3.0

HLR-Id ::= IMSI
	-- leading digits of IMSI, i.e. (MCC, MNC, leading digits of
	-- MSIN) forming HLR Id defined in TS 3GPP TS 23.003 [17].

HLR-List ::= SEQUENCE SIZE (1..maxNumOfHLR-Id) OF
				HLR-Id

maxNumOfHLR-Id  INTEGER ::= 50

LMSI ::= OCTET STRING (SIZE (4))

GlobalCellId ::= OCTET STRING (SIZE (5..7))
	-- Refers to Cell Global Identification defined in TS 3GPP TS 23.003 [17].
	-- The internal structure is defined as follows:
	-- octet 1 bits 4321	Mobile Country Code 1st digit
	--         bits 8765	Mobile Country Code 2nd digit
	-- octet 2 bits 4321	Mobile Country Code 3rd digit
	--         bits 8765	Mobile Network Code 3rd digit
	--			or filler (1111) for 2 digit MNCs
	-- octet 3 bits 4321	Mobile Network Code 1st digit
	--         bits 8765	Mobile Network Code 2nd digit
	-- octets 4 and 5	Location Area Code according to TS 3GPP TS 24.008 [35]
	-- octets 6 and 7	Cell Identity (CI) according to TS 3GPP TS 24.008 [35]

NetworkResource ::= ENUMERATED {
	plmn  (0),
	hlr  (1),
	vlr  (2),
	pvlr  (3),
	controllingMSC  (4),
	vmsc  (5),
	eir  (6),
	rss  (7)}

AdditionalNetworkResource ::= ENUMERATED {
	sgsn (0),
	ggsn (1),
	gmlc (2),
	gsmSCF (3),
	nplr (4),
	auc (5),
	... ,
	ue (6),
	mme (7)}
	-- if unknown value is received in AdditionalNetworkResource
	-- it shall be ignored.


NAEA-PreferredCI ::= SEQUENCE {
	naea-PreferredCIC	[0] NAEA-CIC,
	extensionContainer	[1] ExtensionContainer	OPTIONAL,
	...}

NAEA-CIC ::= OCTET STRING (SIZE (3))
	-- The internal structure is defined by the Carrier Identification
	-- parameter in ANSI T1.113.3. Carrier codes between 000 and 999 may
	-- be encoded as 3 digits using 000 to 999 or as 4 digits using 
	-- 0000 to 0999. Carrier codes between 1000 and 9999 are encoded
	-- using 4 digits.

SubscriberIdentity ::= CHOICE {
	imsi			[0] IMSI,
	msisdn		[1] ISDN-AddressString
	}

LCSClientExternalID ::= SEQUENCE {
	externalAddress	[0] ISDN-AddressString	OPTIONAL,
	extensionContainer	[1] ExtensionContainer	OPTIONAL,
	... }

LCSClientInternalID ::= ENUMERATED {
	broadcastService	(0),
	o-andM-HPLMN	(1),
	o-andM-VPLMN	(2),
	anonymousLocation	(3),
	targetMSsubscribedService	(4),
	... }
-- for a CAMEL phase 3 PLMN operator client, the value targetMSsubscribedService shall be used

LCSServiceTypeID ::= INTEGER (0..127)
	-- the integer values 0-63 are reserved for Standard LCS service types
	-- the integer values 64-127 are reserved for Non Standard LCS service types

-- Standard LCS Service Types
emergencyServices		LCSServiceTypeID ::= 0
emergencyAlertServices		LCSServiceTypeID ::= 1
personTracking			LCSServiceTypeID ::= 2
fleetManagement		LCSServiceTypeID ::= 3
assetManagement		LCSServiceTypeID ::= 4
trafficCongestionReporting		LCSServiceTypeID ::= 5
roadsideAssistance		LCSServiceTypeID ::= 6
routingToNearestCommercialEnterprise		LCSServiceTypeID ::= 7
navigation			LCSServiceTypeID ::= 8
	--this service type is reserved for use in previous releases
citySightseeing		LCSServiceTypeID ::= 9
localizedAdvertising		LCSServiceTypeID ::= 10
mobileYellowPages		LCSServiceTypeID ::= 11 
trafficAndPublicTransportationInfo		LCSServiceTypeID ::= 12
weather				LCSServiceTypeID ::= 13
assetAndServiceFinding		LCSServiceTypeID ::= 14
gaming				LCSServiceTypeID ::= 15
findYourFriend			LCSServiceTypeID ::= 16
dating				LCSServiceTypeID ::= 17
chatting				LCSServiceTypeID ::= 18
routeFinding			LCSServiceTypeID ::= 19
whereAmI				LCSServiceTypeID ::= 20

-- The values of LCSServiceTypeID are defined according to 3GPP TS 22.071.

-- Non Standard LCS Service Types
serv64				LCSServiceTypeID ::= 64
serv65				LCSServiceTypeID ::= 65
serv66				LCSServiceTypeID ::= 66
serv67				LCSServiceTypeID ::= 67
serv68				LCSServiceTypeID ::= 68
serv69				LCSServiceTypeID ::= 69
serv70				LCSServiceTypeID ::= 70
serv71				LCSServiceTypeID ::= 71
serv72				LCSServiceTypeID ::= 72
serv73				LCSServiceTypeID ::= 73
serv74				LCSServiceTypeID ::= 74
serv75				LCSServiceTypeID ::= 75
serv76				LCSServiceTypeID ::= 76
serv77				LCSServiceTypeID ::= 77
serv78				LCSServiceTypeID ::= 78
serv79				LCSServiceTypeID ::= 79
serv80				LCSServiceTypeID ::= 80
serv81				LCSServiceTypeID ::= 81
serv82				LCSServiceTypeID ::= 82
serv83				LCSServiceTypeID ::= 83
serv84				LCSServiceTypeID ::= 84
serv85				LCSServiceTypeID ::= 85
serv86				LCSServiceTypeID ::= 86
serv87				LCSServiceTypeID ::= 87
serv88				LCSServiceTypeID ::= 88
serv89				LCSServiceTypeID ::= 89
serv90				LCSServiceTypeID ::= 90
serv91				LCSServiceTypeID ::= 91
serv92				LCSServiceTypeID ::= 92
serv93				LCSServiceTypeID ::= 93
serv94				LCSServiceTypeID ::= 94
serv95				LCSServiceTypeID ::= 95
serv96				LCSServiceTypeID ::= 96
serv97				LCSServiceTypeID ::= 97
serv98				LCSServiceTypeID ::= 98
serv99				LCSServiceTypeID ::= 99
serv100				LCSServiceTypeID ::= 100
serv101				LCSServiceTypeID ::= 101
serv102				LCSServiceTypeID ::= 102
serv103				LCSServiceTypeID ::= 103
serv104				LCSServiceTypeID ::= 104
serv105				LCSServiceTypeID ::= 105
serv106				LCSServiceTypeID ::= 106
serv107				LCSServiceTypeID ::= 107
serv108				LCSServiceTypeID ::= 108
serv109				LCSServiceTypeID ::= 109
serv110				LCSServiceTypeID ::= 110
serv111				LCSServiceTypeID ::= 111
serv112				LCSServiceTypeID ::= 112
serv113				LCSServiceTypeID ::= 113
serv114				LCSServiceTypeID ::= 114
serv115				LCSServiceTypeID ::= 115
serv116				LCSServiceTypeID ::= 116
serv117				LCSServiceTypeID ::= 117
serv118				LCSServiceTypeID ::= 118
serv119				LCSServiceTypeID ::= 119
serv120				LCSServiceTypeID ::= 120
serv121				LCSServiceTypeID ::= 121
serv122				LCSServiceTypeID ::= 122
serv123				LCSServiceTypeID ::= 123
serv124				LCSServiceTypeID ::= 124
serv125				LCSServiceTypeID ::= 125
serv126				LCSServiceTypeID ::= 126
serv127				LCSServiceTypeID ::= 127

PLMN-Id ::= OCTET STRING (SIZE (3))
	-- The internal structure is defined as follows:
	-- octet 1 bits 4321	Mobile Country Code 1st digit
	--         bits 8765	Mobile Country Code 2nd digit
	-- octet 2 bits 4321	Mobile Country Code 3rd digit
	--         bits 8765	Mobile Network Code 3rd digit
	--			or filler (1111) for 2 digit MNCs
	-- octet 3 bits 4321	Mobile Network Code 1st digit
	--         bits 8765	Mobile Network Code 2nd digit

E-UTRAN-CGI ::= OCTET STRING (SIZE (7))
	-- Octets are coded as described in 3GPP TS 29.118.

TA-Id ::= OCTET STRING (SIZE (5))
	-- Octets are coded as described in 3GPP TS 29.118.

RAIdentity ::= OCTET STRING (SIZE (6))
-- Routing Area Identity is coded in accordance with 3GPP TS 29.060 [105].
-- It shall contain the value part defined in 3GPP TS 29.060 only. I.e. the 3GPP TS 29.060
-- type identifier octet shall not be included.

-- data types for CAMEL

CellGlobalIdOrServiceAreaIdOrLAI ::= CHOICE {
	cellGlobalIdOrServiceAreaIdFixedLength	[0] CellGlobalIdOrServiceAreaIdFixedLength,
	laiFixedLength	[1] LAIFixedLength}

CellGlobalIdOrServiceAreaIdFixedLength ::= OCTET STRING (SIZE (7))
	-- Refers to Cell Global Identification or Service Are Identification
	-- defined in 3GPP TS 23.003.
	-- The internal structure is defined as follows:
	-- octet 1 bits 4321	Mobile Country Code 1st digit
	--         bits 8765	Mobile Country Code 2nd digit
	-- octet 2 bits 4321	Mobile Country Code 3rd digit
	--         bits 8765	Mobile Network Code 3rd digit
	--			or filler (1111) for 2 digit MNCs
	-- octet 3 bits 4321	Mobile Network Code 1st digit
	--         bits 8765	Mobile Network Code 2nd digit
	-- octets 4 and 5	Location Area Code according to 3GPP TS 24.008
	-- octets 6 and 7	Cell Identity (CI) value or 
	-- 			Service Area Code (SAC) value 
	--			according to 3GPP TS 23.003

LAIFixedLength ::= OCTET STRING (SIZE (5))
	-- Refers to Location Area Identification defined in 3GPP TS 23.003 [17].
	-- The internal structure is defined as follows:
	-- octet 1 bits 4321	Mobile Country Code 1st digit
	--         bits 8765	Mobile Country Code 2nd digit
	-- octet 2 bits 4321	Mobile Country Code 3rd digit
	--         bits 8765	Mobile Network Code 3rd digit
	--			or filler (1111) for 2 digit MNCs
	-- octet 3 bits 4321	Mobile Network Code 1st digit
	--         bits 8765	Mobile Network Code 2nd digit
	-- octets 4 and 5	Location Area Code according to 3GPP TS 24.008 [35]

-- data types for subscriber management

BasicServiceCode ::= CHOICE {
	bearerService	[2] BearerServiceCode,
	teleservice	[3] TeleserviceCode}

Ext-BasicServiceCode ::= CHOICE {
	ext-BearerService	[2] Ext-BearerServiceCode,
	ext-Teleservice	[3] Ext-TeleserviceCode}

EMLPP-Info ::= SEQUENCE {
	maximumentitledPriority	EMLPP-Priority,
	defaultPriority	EMLPP-Priority,
	extensionContainer	ExtensionContainer	OPTIONAL,
	...}

EMLPP-Priority ::= INTEGER (0..15)
	-- The mapping from the values A,B,0,1,2,3,4 to the integer-value is
	-- specified as follows where A is the highest and 4 is the lowest
	-- priority level
	-- the integer values 7-15 are spare and shall be mapped to value 4

priorityLevelA		EMLPP-Priority ::= 6
priorityLevelB		EMLPP-Priority ::= 5
priorityLevel0		EMLPP-Priority ::= 0
priorityLevel1		EMLPP-Priority ::= 1
priorityLevel2		EMLPP-Priority ::= 2
priorityLevel3		EMLPP-Priority ::= 3
priorityLevel4		EMLPP-Priority ::= 4

MC-SS-Info ::= SEQUENCE {
	ss-Code		[0] SS-Code,
	ss-Status		[1] Ext-SS-Status,
	nbrSB		[2] MaxMC-Bearers,
	nbrUser		[3] MC-Bearers,
	extensionContainer	[4] ExtensionContainer	OPTIONAL,
	...}

MaxMC-Bearers ::= INTEGER (2..maxNumOfMC-Bearers)

MC-Bearers ::= INTEGER (1..maxNumOfMC-Bearers)

maxNumOfMC-Bearers  INTEGER ::= 7

Ext-SS-Status ::= OCTET STRING (SIZE (1..5))

	-- OCTET 1:
	--
	-- bits 8765: 0000 (unused)
	-- bits 4321: Used to convey the "P bit","R bit","A bit" and "Q bit",
	--		    representing supplementary service state information
	--		    as defined in TS 3GPP TS 23.011 [22]

	-- bit 4: "Q bit"

	-- bit 3: "P bit"

	-- bit 2: "R bit"

	-- bit 1: "A bit"

	-- OCTETS 2-5: reserved for future use. They shall be discarded if
	-- received and not understood.


	-- data types for geographic location

AgeOfLocationInformation ::= INTEGER (0..32767)
-- the value represents the elapsed time in minutes since the last
-- network contact of the mobile station (i.e. the actuality of the
-- location information).
-- value 0 indicates that the MS is currently in contact with the
--           network
-- value 32767 indicates that the location information is at least
--               32767 minutes old

END
