ST-Ericsson COH 901 571/3 GPIO controller

Required properties:
- compatible: Compatible property value should be "stericsson,gpio-coh901"
- reg: Physical base address of the controller and length of memory mapped
  region.
- interrupts: the 0...n interrupts assigned to the different GPIO ports/banks.
