Mediatek vdecsys controller
============================

The Mediatek vdecsys controller provides various clocks to the system.

Required Properties:

- compatible: Should be one of:
	- "mediatek,mt2701-vdecsys", "syscon"
	- "mediatek,mt2712-vdecsys", "syscon"
	- "mediatek,mt6779-vdecsys", "syscon"
	- "mediatek,mt6797-vdecsys", "syscon"
	- "mediatek,mt7623-vdecsys", "mediatek,mt2701-vdecsys", "syscon"
	- "mediatek,mt8167-vdecsys", "syscon"
	- "mediatek,mt8173-vdecsys", "syscon"
	- "mediatek,mt8183-vdecsys", "syscon"
- #clock-cells: Must be 1

The vdecsys controller uses the common clk binding from
Documentation/devicetree/bindings/clock/clock-bindings.txt
The available clocks are defined in dt-bindings/clock/mt*-clk.h.

Example:

vdecsys: clock-controller@16000000 {
	compatible = "mediatek,mt8173-vdecsys", "syscon";
	reg = <0 0x16000000 0 0x1000>;
	#clock-cells = <1>;
};
