TPS65217 Charger

Required Properties:
-compatible: "ti,tps65217-charger"
-interrupts: TPS65217 interrupt numbers for the AC and USB charger input change.
             Should be <0> for the USB charger and <1> for the AC adapter.
-interrupt-names: Should be "USB" and "AC"

This node is a subnode of the tps65217 PMIC.

Example:

	tps65217-charger {
		compatible = "ti,tps65217-charger";
		interrupts = <0>, <1>;
		interrupt-names = "USB", "AC";
	};
