-----------------------------------------------------------------
Device Tree Bindings for the Xilinx Zynq MPSoC Firmware Interface
-----------------------------------------------------------------

The zynqmp-firmware node describes the interface to platform firmware.
ZynqMP has an interface to communicate with secure firmware. Firmware
driver provides an interface to firmware APIs. Interface APIs can be
used by any driver to communicate to PMUFW(Platform Management Unit).
These requests include clock management, pin control, device control,
power management service, FPGA service and other platform management
services.

Required properties:
 - compatible:	Must contain any of below:
		"xlnx,zynqmp-firmware" for Zynq Ultrascale+ MPSoC
		"xlnx,versal-firmware" for Versal
 - method:	The method of calling the PM-API firmware layer.
		Permitted values are:
		  - "smc" : SMC #0, following the SMCCC
		  - "hvc" : HVC #0, following the SMCCC

-------
Example
-------

Zynq Ultrascale+ MPSoC
----------------------
firmware {
	zynqmp_firmware: zynqmp-firmware {
		compatible = "xlnx,zynqmp-firmware";
		method = "smc";
		...
	};
};

Versal
------
firmware {
	versal_firmware: versal-firmware {
		compatible = "xlnx,versal-firmware";
		method = "smc";
		...
	};
};
