What:           /sys/kernel/debug/genwqe/genwqe<n>_card/ddcb_info
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    DDCB queue dump used for debugging queueing problems.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/curr_regs
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Dump of the current error registers.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/curr_dbg_uid0
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID0 (unit id 0).
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/curr_dbg_uid1
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID1.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/curr_dbg_uid2
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID2.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/prev_regs
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Dump of the error registers before the last reset of
                the card occured.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/prev_dbg_uid0
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID0 before card was reset.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/prev_dbg_uid1
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID1 before card was reset.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/prev_dbg_uid2
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Internal chip state of UID2 before card was reset.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/info
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Comprehensive summary of bitstream version and software
                version. Used bitstream and bitstream clocking information.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/err_inject
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Possibility to inject error cases to ensure that the drivers
                error handling code works well.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/vf<0..14>_jobtimeout_msec
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Default VF timeout 250ms. Testing might require 1000ms.
                Using 0 will use the cards default value (whatever that is).

                The timeout depends on the max number of available cards
                in the system and the maximum allowed queue size.

                The driver ensures that the settings are done just before
                the VFs get enabled. Changing the timeouts in flight is not
                possible.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/jobtimer
Date:           Oct 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Dump job timeout register values for PF and VFs.
                Only available for PF.

What:           /sys/kernel/debug/genwqe/genwqe<n>_card/queue_working_time
Date:           Dec 2013
Contact:        haver@linux.vnet.ibm.com
Description:    Dump queue working time register values for PF and VFs.
                Only available for PF.
