ARM Versatile Character LCD
-----------------------------------------------------
This binding defines the character LCD interface found on ARM Versatile AB
and PB reference platforms.

Required properties:
- compatible : "arm,versatile-clcd"
- reg : Location and size of character LCD registers

Optional properties:
- interrupts - single interrupt for character LCD. The character LCD can
  operate in polled mode without an interrupt.

Example:
	lcd@10008000 {
		compatible = "arm,versatile-lcd";
		reg = <0x10008000 0x1000>;
	};
