MediaTek MT7621/MT7628 I2C master controller

Required properties:

- compatible: Should be one of the following:
  - "mediatek,mt7621-i2c": for MT7621/MT7628/MT7688 platforms
- #address-cells: should be 1.
- #size-cells: should be 0.
- reg: Address and length of the register set for the device
- resets: phandle to the reset controller asserting this device in
          reset
  See ../reset/reset.txt for details.

Optional properties :

Example:

i2c: i2c@900 {
	compatible = "mediatek,mt7621-i2c";
	reg = <0x900 0x100>;
	#address-cells = <1>;
	#size-cells = <0>;
	resets = <&rstctrl 16>;
	reset-names = "i2c";
};
