ARM Versatile system registers
--------------------------------------

This is a system control registers block, providing multiple low level
platform functions like board detection and identification, software
interrupt generation, MMC and NOR Flash control etc.

Required node properties:
- compatible value : = "arm,versatile-sysreg", "syscon"
- reg : physical base address and the size of the registers window
