Davicom DM9000 Fast Ethernet controller

Required properties:
- compatible = "davicom,dm9000";
- reg : physical addresses and sizes of registers, must contain 2 entries:
    first entry : address register,
    second entry : data register.
- interrupts : interrupt specifier specific to interrupt controller

Optional properties:
- davicom,no-eeprom : Configuration EEPROM is not available
- davicom,ext-phy : Use external PHY
- reset-gpios : phandle of gpio that will be used to reset chip during probe
- vcc-supply : phandle of regulator that will be used to enable power to chip

Example:

	ethernet@18000000 {
		compatible = "davicom,dm9000";
		reg = <0x18000000 0x2 0x18000004 0x2>;
		interrupt-parent = <&gpn>;
		interrupts = <7 4>;
		local-mac-address = [00 00 de ad be ef];
		davicom,no-eeprom;
		reset-gpios = <&gpf 12 GPIO_ACTIVE_LOW>;
		vcc-supply = <&eth0_power>;
	};
