Chinese translated version of Documentation/arm64/tagged-pointers.rst

If you have any comment or update to the content, please contact the
original document maintainer directly.  However, if you have a problem
communicating in English you can also ask the Chinese maintainer for
help.  Contact the Chinese maintainer if this translation is outdated
or if there is a problem with the translation.

Maintainer: Will Deacon <will.deacon@arm.com>
Chinese maintainer: Fu Wei <wefu@redhat.com>
---------------------------------------------------------------------
Documentation/arm64/tagged-pointers.rst 的中文翻译

如果想评论或更新本文的内容，请直接联系原文档的维护者。如果你使用英文
交流有困难的话，也可以向中文版维护者求助。如果本翻译更新不及时或者翻
译存在问题，请联系中文版维护者。

英文版维护者： Will Deacon <will.deacon@arm.com>
中文版维护者： 傅炜  Fu Wei <wefu@redhat.com>
中文版翻译者： 傅炜  Fu Wei <wefu@redhat.com>
中文版校译者： 傅炜  Fu Wei <wefu@redhat.com>

以下为正文
---------------------------------------------------------------------
		Linux 在 AArch64 中带标记的虚拟地址
		=================================

作者: Will Deacon <will.deacon@arm.com>
日期: 2013 年 06 月 12 日

本文档简述了在 AArch64 地址转换系统中提供的带标记的虚拟地址及其在
AArch64 Linux 中的潜在用途。

内核提供的地址转换表配置使通过 TTBR0 完成的虚拟地址转换（即用户空间
映射），其虚拟地址的最高 8 位（63:56）会被转换硬件所忽略。这种机制
让这些位可供应用程序自由使用，其注意事项如下：

	(1) 内核要求所有传递到 EL1 的用户空间地址带有 0x00 标记。
	    这意味着任何携带用户空间虚拟地址的系统调用（syscall）
	    参数 *必须* 在陷入内核前使它们的最高字节被清零。

	(2) 非零标记在传递信号时不被保存。这意味着在应用程序中利用了
	    标记的信号处理函数无法依赖 siginfo_t 的用户空间虚拟
	    地址所携带的包含其内部域信息的标记。此规则的一个例外是
	    当信号是在调试观察点的异常处理程序中产生的，此时标记的
	    信息将被保存。

	(3) 当使用带标记的指针时需特别留心，因为仅对两个虚拟地址
	    的高字节，C 编译器很可能无法判断它们是不同的。

此构架会阻止对带标记的 PC 指针的利用，因此在异常返回时，其高字节
将被设置成一个为 “55” 的扩展符。
