Bosch Sensortec BME680 pressure/temperature/humidity/voc sensors

Required properties:
- compatible: must be "bosch,bme680"

Example:

bme680@76 {
          compatible = "bosch,bme680";
          reg = <0x76>;
};
