NXP PCF85263/PCF85363 Real Time Clock
============================

Required properties:
- compatible: Should contain "nxp,pcf85263" or "nxp,pcf85363".
- reg: I2C address for chip.

Optional properties:
- interrupts: IRQ line for the RTC (not implemented).

Example:

pcf85363: pcf85363@51 {
	compatible = "nxp,pcf85363";
	reg = <0x51>;
};

