* Omnivision 1/4-Inch 5Mp CMOS Digital Image Sensor

The Omnivision OV5645 is a 1/4-Inch CMOS active pixel digital image sensor with
an active array size of 2592H x 1944V. It is programmable through a serial I2C
interface.

Required Properties:
- compatible: Value should be "ovti,ov5645".
- clocks: Reference to the xclk clock.
- clock-names: Should be "xclk".
- clock-frequency: Frequency of the xclk clock.
- enable-gpios: Chip enable GPIO. Polarity is GPIO_ACTIVE_HIGH. This corresponds
  to the hardware pin PWDNB which is physically active low.
- reset-gpios: Chip reset GPIO. Polarity is GPIO_ACTIVE_LOW. This corresponds to
  the hardware pin RESETB.
- vdddo-supply: Chip digital IO regulator.
- vdda-supply: Chip analog regulator.
- vddd-supply: Chip digital core regulator.

The device node must contain one 'port' child node for its digital output
video port, in accordance with the video interface bindings defined in
Documentation/devicetree/bindings/media/video-interfaces.txt.

Example:

	&i2c1 {
		...

		ov5645: ov5645@3c {
			compatible = "ovti,ov5645";
			reg = <0x3c>;

			enable-gpios = <&gpio1 6 GPIO_ACTIVE_HIGH>;
			reset-gpios = <&gpio5 20 GPIO_ACTIVE_LOW>;
			pinctrl-names = "default";
			pinctrl-0 = <&camera_rear_default>;

			clocks = <&clks 200>;
			clock-names = "xclk";
			clock-frequency = <24000000>;

			vdddo-supply = <&camera_dovdd_1v8>;
			vdda-supply = <&camera_avdd_2v8>;
			vddd-supply = <&camera_dvdd_1v2>;

			port {
				ov5645_ep: endpoint {
					clock-lanes = <1>;
					data-lanes = <0 2>;
					remote-endpoint = <&csi0_ep>;
				};
			};
		};
	};
