Cadence DPHY
============

Cadence DPHY block.

Required properties:
- compatible: should be set to "cdns,dphy".
- reg: physical base address and length of the DPHY registers.
- clocks: DPHY reference clocks.
- clock-names: must contain "psm" and "pll_ref".
- #phy-cells: must be set to 0.

Example:
	dphy0: dphy@fd0e0000{
		compatible = "cdns,dphy";
		reg = <0x0 0xfd0e0000 0x0 0x1000>;
		clocks = <&psm_clk>, <&pll_ref_clk>;
		clock-names = "psm", "pll_ref";
		#phy-cells = <0>;
	};
