* SiRFprimII/marco/atlas6 SDHCI Controller

This file documents differences between the core properties in mmc.txt
and the properties used by the sdhci-sirf driver.

Required properties:
- compatible: sirf,prima2-sdhc

Optional properties:
- cd-gpios: card detect gpio, with zero flags.

Example:

	sd0: sdhci@56000000 {
		compatible = "sirf,prima2-sdhc";
		reg = <0xcd000000 0x100000>;
		cd-gpios = <&gpio 6 0>;
	};
