SiRF internal audio CODEC

Required properties:

  - compatible : "sirf,atlas6-audio-codec" or "sirf,prima2-audio-codec"

  - reg : the register address of the device.

  - clocks: the clock of SiRF internal audio codec

Example:

audiocodec: audiocodec@b0040000 {
	compatible = "sirf,atlas6-audio-codec";
	reg = <0xb0040000 0x10000>;
	clocks = <&clks 27>;
};
