Kernel driver max6642
=====================

Supported chips:

  * Maxim MAX6642

    Prefix: 'max6642'

    Addresses scanned: I2C 0x48-0x4f

    Datasheet: Publicly available at the Maxim website

	       http://datasheets.maxim-ic.com/en/ds/MAX6642.pdf

Authors:

	Per Dalen <per.dalen@appeartv.com>

Description
-----------

The MAX6642 is a digital temperature sensor. It senses its own temperature as
well as the temperature on one external diode.

All temperature values are given in degrees Celsius. Resolution
is 0.25 degree for the local temperature and for the remote temperature.
