* Mediatek UART APDMA Controller

Required properties:
- compatible should contain:
  * "mediatek,mt2712-uart-dma" for MT2712 compatible APDMA
  * "mediatek,mt6577-uart-dma" for MT6577 and all of the above

- reg: The base address of the APDMA register bank.

- interrupts: A single interrupt specifier.
 One interrupt per dma-requests, or 8 if no dma-requests property is present

- dma-requests: The number of DMA channels

- clocks : Must contain an entry for each entry in clock-names.
  See ../clocks/clock-bindings.txt for details.
- clock-names: The APDMA clock for register accesses

- mediatek,dma-33bits: Present if the DMA requires support

Examples:

	apdma: dma-controller@11000400 {
		compatible = "mediatek,mt2712-uart-dma",
			     "mediatek,mt6577-uart-dma";
		reg = <0 0x11000400 0 0x80>,
		      <0 0x11000480 0 0x80>,
		      <0 0x11000500 0 0x80>,
		      <0 0x11000580 0 0x80>,
		      <0 0x11000600 0 0x80>,
		      <0 0x11000680 0 0x80>,
		      <0 0x11000700 0 0x80>,
		      <0 0x11000780 0 0x80>,
		      <0 0x11000800 0 0x80>,
		      <0 0x11000880 0 0x80>,
		      <0 0x11000900 0 0x80>,
		      <0 0x11000980 0 0x80>;
		interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 104 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 105 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 106 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 107 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 108 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 109 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 110 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 111 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 112 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 113 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_SPI 114 IRQ_TYPE_LEVEL_LOW>;
		dma-requests = <12>;
		clocks = <&pericfg CLK_PERI_AP_DMA>;
		clock-names = "apdma";
		mediatek,dma-33bits;
		#dma-cells = <1>;
	};
