max9867 codec

This device supports I2C mode only.

Required properties:

- compatible : "maxim,max9867"
- reg : The chip select number on the I2C bus

Example:

&i2c {
	max9867: max9867@18 {
		compatible = "maxim,max9867";
		reg = <0x18>;
	};
};
