=============================
Introduction to I2C and SMBus
=============================

I²C (pronounce: I squared C and written I2C in the kernel documentation) is
a protocol developed by Philips. It is a slow two-wire protocol (variable
speed, up to 400 kHz), with a high speed extension (3.4 MHz).  It provides
an inexpensive bus for connecting many types of devices with infrequent or
low bandwidth communications needs.  I2C is widely used with embedded
systems.  Some systems use variants that don't meet branding requirements,
and so are not advertised as being I2C but come under different names,
e.g. TWI (Two Wire Interface), IIC.

The official I2C specification is the `"I2C-bus specification and user
manual" (UM10204) <https://www.nxp.com/docs/en/user-guide/UM10204.pdf>`_
published by NXP Semiconductors.

SMBus (System Management Bus) is based on the I2C protocol, and is mostly
a subset of I2C protocols and signaling.  Many I2C devices will work on an
SMBus, but some SMBus protocols add semantics beyond what is required to
achieve I2C branding.  Modern PC mainboards rely on SMBus.  The most common
devices connected through SMBus are RAM modules configured using I2C EEPROMs,
and hardware monitoring chips.

Because the SMBus is mostly a subset of the generalized I2C bus, we can
use its protocols on many I2C systems.  However, there are systems that don't
meet both SMBus and I2C electrical constraints; and others which can't
implement all the common SMBus protocol semantics or messages.


Terminology
===========

Using the terminology from the official documentation, the I2C bus connects
one or more *master* chips and one or more *slave* chips.

.. kernel-figure::  i2c_bus.svg
   :alt:    Simple I2C bus with one master and 3 slaves

   Simple I2C bus

A **master** chip is a node that starts communications with slaves. In the
Linux kernel implementation it is called an **adapter** or bus. Adapter
drivers are in the ``drivers/i2c/busses/`` subdirectory.

An **algorithm** contains general code that can be used to implement a
whole class of I2C adapters. Each specific adapter driver either depends on
an algorithm driver in the ``drivers/i2c/algos/`` subdirectory, or includes
its own implementation.

A **slave** chip is a node that responds to communications when addressed
by the master. In Linux it is called a **client**. Client drivers are kept
in a directory specific to the feature they provide, for example
``drivers/media/gpio/`` for GPIO expanders and ``drivers/media/i2c/`` for
video-related chips.

For the example configuration in figure, you will need a driver for your
I2C adapter, and drivers for your I2C devices (usually one driver for each
device).
