Device-Tree bindings for hdmiddc driver

Required properties:
- compatible: value should be one of the following
	1) "samsung,exynos5-hdmiddc" <DEPRECATED>
	2) "samsung,exynos4210-hdmiddc"

- reg: I2C address of the hdmiddc device.

Example:

	hdmiddc {
		compatible = "samsung,exynos4210-hdmiddc";
		reg = <0x50>;
	};
