OMAP HS USB OHCI controller (OMAP3 and later)

Required properties:

- compatible: should be "ti,ohci-omap3"
- reg: should contain one register range i.e. start and length
- interrupts: description of the interrupt line

Example for OMAP4:

usbhsohci: ohci@4a064800 {
	compatible = "ti,ohci-omap3";
	reg = <0x4a064800 0x400>;
	interrupts = <0 76 0x4>;
};
