DPAA2 console support

Required properties:

    - compatible
        Value type: <string>
        Definition: Must be "fsl,dpaa2-console".
    - reg
        Value type: <prop-encoded-array>
        Definition: A standard property.  Specifies the region where the MCFBA
                    (MC firmware base address) register can be found.
