What:		/sys/bus/iio/devices/iio:deviceX/out_current_heater_raw
What:		/sys/bus/iio/devices/iio:deviceX/out_current_heater_raw_available
KernelVersion:	4.3
Contact:	linux-iio@vger.kernel.org
Description:
		Controls the heater device within the humidity sensor to get
		rid of excess condensation.

		Valid control values are 0 = OFF, and 1 = ON.
