================
ARM64 ELF hwcaps
================

This document describes the usage and semantics of the arm64 ELF hwcaps.


1. Introduction
---------------

Some hardware or software features are only available on some CPU
implementations, and/or with certain kernel configurations, but have no
architected discovery mechanism available to userspace code at EL0. The
kernel exposes the presence of these features to userspace through a set
of flags called hwcaps, exposed in the auxilliary vector.

Userspace software can test for features by acquiring the AT_HWCAP or
AT_HWCAP2 entry of the auxiliary vector, and testing whether the relevant
flags are set, e.g.::

	bool floating_point_is_present(void)
	{
		unsigned long hwcaps = getauxval(AT_HWCAP);
		if (hwcaps & HWCAP_FP)
			return true;

		return false;
	}

Where software relies on a feature described by a hwcap, it should check
the relevant hwcap flag to verify that the feature is present before
attempting to make use of the feature.

Features cannot be probed reliably through other means. When a feature
is not available, attempting to use it may result in unpredictable
behaviour, and is not guaranteed to result in any reliable indication
that the feature is unavailable, such as a SIGILL.


2. Interpretation of hwcaps
---------------------------

The majority of hwcaps are intended to indicate the presence of features
which are described by architected ID registers inaccessible to
userspace code at EL0. These hwcaps are defined in terms of ID register
fields, and should be interpreted with reference to the definition of
these fields in the ARM Architecture Reference Manual (ARM ARM).

Such hwcaps are described below in the form::

    Functionality implied by idreg.field == val.

Such hwcaps indicate the availability of functionality that the ARM ARM
defines as being present when idreg.field has value val, but do not
indicate that idreg.field is precisely equal to val, nor do they
indicate the absence of functionality implied by other values of
idreg.field.

Other hwcaps may indicate the presence of features which cannot be
described by ID registers alone. These may be described without
reference to ID registers, and may refer to other documentation.


3. The hwcaps exposed in AT_HWCAP
---------------------------------

HWCAP_FP
    Functionality implied by ID_AA64PFR0_EL1.FP == 0b0000.

HWCAP_ASIMD
    Functionality implied by ID_AA64PFR0_EL1.AdvSIMD == 0b0000.

HWCAP_EVTSTRM
    The generic timer is configured to generate events at a frequency of
    approximately 100KHz.

HWCAP_AES
    Functionality implied by ID_AA64ISAR0_EL1.AES == 0b0001.

HWCAP_PMULL
    Functionality implied by ID_AA64ISAR0_EL1.AES == 0b0010.

HWCAP_SHA1
    Functionality implied by ID_AA64ISAR0_EL1.SHA1 == 0b0001.

HWCAP_SHA2
    Functionality implied by ID_AA64ISAR0_EL1.SHA2 == 0b0001.

HWCAP_CRC32
    Functionality implied by ID_AA64ISAR0_EL1.CRC32 == 0b0001.

HWCAP_ATOMICS
    Functionality implied by ID_AA64ISAR0_EL1.Atomic == 0b0010.

HWCAP_FPHP
    Functionality implied by ID_AA64PFR0_EL1.FP == 0b0001.

HWCAP_ASIMDHP
    Functionality implied by ID_AA64PFR0_EL1.AdvSIMD == 0b0001.

HWCAP_CPUID
    EL0 access to certain ID registers is available, to the extent
    described by Documentation/arm64/cpu-feature-registers.rst.

    These ID registers may imply the availability of features.

HWCAP_ASIMDRDM
    Functionality implied by ID_AA64ISAR0_EL1.RDM == 0b0001.

HWCAP_JSCVT
    Functionality implied by ID_AA64ISAR1_EL1.JSCVT == 0b0001.

HWCAP_FCMA
    Functionality implied by ID_AA64ISAR1_EL1.FCMA == 0b0001.

HWCAP_LRCPC
    Functionality implied by ID_AA64ISAR1_EL1.LRCPC == 0b0001.

HWCAP_DCPOP
    Functionality implied by ID_AA64ISAR1_EL1.DPB == 0b0001.

HWCAP_SHA3
    Functionality implied by ID_AA64ISAR0_EL1.SHA3 == 0b0001.

HWCAP_SM3
    Functionality implied by ID_AA64ISAR0_EL1.SM3 == 0b0001.

HWCAP_SM4
    Functionality implied by ID_AA64ISAR0_EL1.SM4 == 0b0001.

HWCAP_ASIMDDP
    Functionality implied by ID_AA64ISAR0_EL1.DP == 0b0001.

HWCAP_SHA512
    Functionality implied by ID_AA64ISAR0_EL1.SHA2 == 0b0010.

HWCAP_SVE
    Functionality implied by ID_AA64PFR0_EL1.SVE == 0b0001.

HWCAP_ASIMDFHM
   Functionality implied by ID_AA64ISAR0_EL1.FHM == 0b0001.

HWCAP_DIT
    Functionality implied by ID_AA64PFR0_EL1.DIT == 0b0001.

HWCAP_USCAT
    Functionality implied by ID_AA64MMFR2_EL1.AT == 0b0001.

HWCAP_ILRCPC
    Functionality implied by ID_AA64ISAR1_EL1.LRCPC == 0b0010.

HWCAP_FLAGM
    Functionality implied by ID_AA64ISAR0_EL1.TS == 0b0001.

HWCAP_SSBS
    Functionality implied by ID_AA64PFR1_EL1.SSBS == 0b0010.

HWCAP_SB
    Functionality implied by ID_AA64ISAR1_EL1.SB == 0b0001.

HWCAP_PACA
    Functionality implied by ID_AA64ISAR1_EL1.APA == 0b0001 or
    ID_AA64ISAR1_EL1.API == 0b0001, as described by
    Documentation/arm64/pointer-authentication.rst.

HWCAP_PACG
    Functionality implied by ID_AA64ISAR1_EL1.GPA == 0b0001 or
    ID_AA64ISAR1_EL1.GPI == 0b0001, as described by
    Documentation/arm64/pointer-authentication.rst.

HWCAP2_DCPODP

    Functionality implied by ID_AA64ISAR1_EL1.DPB == 0b0010.

HWCAP2_SVE2

    Functionality implied by ID_AA64ZFR0_EL1.SVEVer == 0b0001.

HWCAP2_SVEAES

    Functionality implied by ID_AA64ZFR0_EL1.AES == 0b0001.

HWCAP2_SVEPMULL

    Functionality implied by ID_AA64ZFR0_EL1.AES == 0b0010.

HWCAP2_SVEBITPERM

    Functionality implied by ID_AA64ZFR0_EL1.BitPerm == 0b0001.

HWCAP2_SVESHA3

    Functionality implied by ID_AA64ZFR0_EL1.SHA3 == 0b0001.

HWCAP2_SVESM4

    Functionality implied by ID_AA64ZFR0_EL1.SM4 == 0b0001.

HWCAP2_FLAGM2

    Functionality implied by ID_AA64ISAR0_EL1.TS == 0b0010.

HWCAP2_FRINT

    Functionality implied by ID_AA64ISAR1_EL1.FRINTTS == 0b0001.

HWCAP2_SVEI8MM

    Functionality implied by ID_AA64ZFR0_EL1.I8MM == 0b0001.

HWCAP2_SVEF32MM

    Functionality implied by ID_AA64ZFR0_EL1.F32MM == 0b0001.

HWCAP2_SVEF64MM

    Functionality implied by ID_AA64ZFR0_EL1.F64MM == 0b0001.

HWCAP2_SVEBF16

    Functionality implied by ID_AA64ZFR0_EL1.BF16 == 0b0001.

HWCAP2_I8MM

    Functionality implied by ID_AA64ISAR1_EL1.I8MM == 0b0001.

HWCAP2_BF16

    Functionality implied by ID_AA64ISAR1_EL1.BF16 == 0b0001.

HWCAP2_DGH

    Functionality implied by ID_AA64ISAR1_EL1.DGH == 0b0001.

HWCAP2_RNG

    Functionality implied by ID_AA64ISAR0_EL1.RNDR == 0b0001.

HWCAP2_BTI

    Functionality implied by ID_AA64PFR0_EL1.BT == 0b0001.

HWCAP2_MTE

    Functionality implied by ID_AA64PFR1_EL1.MTE == 0b0010, as described
    by Documentation/arm64/memory-tagging-extension.rst.

HWCAP2_ECV

    Functionality implied by ID_AA64MMFR0_EL1.ECV == 0b0001.

HWCAP2_AFP

    Functionality implied by ID_AA64MFR1_EL1.AFP == 0b0001.

HWCAP2_RPRES

    Functionality implied by ID_AA64ISAR2_EL1.RPRES == 0b0001.

4. Unused AT_HWCAP bits
-----------------------

For interoperation with userspace, the kernel guarantees that bits 62
and 63 of AT_HWCAP will always be returned as 0.
