VISHAY VCNL4035 -  Ambient Light and proximity sensor

Link to datasheet: https://www.vishay.com/docs/84251/vcnl4035x01.pdf

Required properties:

	-compatible: should be "vishay,vcnl4035"
	-reg: I2C address of the sensor, should be 0x60
	-interrupts: interrupt mapping for GPIO IRQ (level active low)

Example:

light-sensor@60 {
	compatible = "vishay,vcnl4035";
	reg = <0x60>;
	interrupt-parent = <&gpio4>;
	interrupts = <11 IRQ_TYPE_LEVEL_LOW>;
};
