LEDs connected to Broadcom BCM6358 controller

This controller is present on BCM6358 and BCM6368.
In these SoCs there are Serial LEDs (LEDs connected to a 74x164 controller),
which can either be controlled by software (exporting the 74x164 as spi-gpio.
See Documentation/devicetree/bindings/gpio/gpio-74x164.txt), or
by hardware using this driver.

Required properties:
  - compatible : should be "brcm,bcm6358-leds".
  - #address-cells : must be 1.
  - #size-cells : must be 0.
  - reg : BCM6358 LED controller address and size.

Optional properties:
  - brcm,clk-div : SCK signal divider. Possible values are 1, 2, 4 and 8.
    Default : 1
  - brcm,clk-dat-low : Boolean, makes clock and data signals active low.
    Default : false

Each LED is represented as a sub-node of the brcm,bcm6358-leds device.

LED sub-node required properties:
  - reg : LED pin number (only LEDs 0 to 31 are valid).

LED sub-node optional properties:
  - label : see Documentation/devicetree/bindings/leds/common.txt
  - active-low : Boolean, makes LED active low.
    Default : false
  - default-state : see
    Documentation/devicetree/bindings/leds/common.txt
  - linux,default-trigger : see
    Documentation/devicetree/bindings/leds/common.txt

Examples:
Scenario 1 : BCM6358
	leds0: led-controller@fffe00d0 {
		compatible = "brcm,bcm6358-leds";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0xfffe00d0 0x8>;

		alarm_white {
			reg = <0>;
			active-low;
			label = "white:alarm";
		};
		tv_white {
			reg = <2>;
			active-low;
			label = "white:tv";
		};
		tel_white {
			reg = <3>;
			active-low;
			label = "white:tel";
		};
		adsl_white {
			reg = <4>;
			active-low;
			label = "white:adsl";
		};
	};

Scenario 2 : BCM6368
	leds0: led-controller@100000d0 {
		compatible = "brcm,bcm6358-leds";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x100000d0 0x8>;
		brcm,pol-low;
		brcm,clk-div = <4>;

		power_red {
			reg = <0>;
			active-low;
			label = "red:power";
		};
		power_green {
			reg = <1>;
			active-low;
			label = "green:power";
			default-state = "on";
		};
		power_blue {
			reg = <2>;
			label = "blue:power";
		};
		broadband_red {
			reg = <3>;
			active-low;
			label = "red:broadband";
		};
		broadband_green {
			reg = <4>;
			label = "green:broadband";
		};
		broadband_blue {
			reg = <5>;
			active-low;
			label = "blue:broadband";
		};
		wireless_red {
			reg = <6>;
			active-low;
			label = "red:wireless";
		};
		wireless_green {
			reg = <7>;
			active-low;
			label = "green:wireless";
		};
		wireless_blue {
			reg = <8>;
			label = "blue:wireless";
		};
		phone_red {
			reg = <9>;
			active-low;
			label = "red:phone";
		};
		phone_green {
			reg = <10>;
			active-low;
			label = "green:phone";
		};
		phone_blue {
			reg = <11>;
			label = "blue:phone";
		};
		upgrading_red {
			reg = <12>;
			active-low;
			label = "red:upgrading";
		};
		upgrading_green {
			reg = <13>;
			active-low;
			label = "green:upgrading";
		};
		upgrading_blue {
			reg = <14>;
			label = "blue:upgrading";
		};
	};
