osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Files | Macros | Functions
DKAB bursts
GMR-1 Software Defined Radio library

## Files
file | dkab.h
| Osmocom GMR-1 DKABs bursts header.
file | dkab.c
| Osmocom GMR-1 DKABs bursts implementation.

## Macros
#define | GMR1_DKAB_SYMS (39*3)
#define | DKAB_PWR_RATIO_THRESHOLD 10.0f
| Ratio between peak power and valley power for DKAB detection.

## Functions
int | gmr1_dkab_demod (struct osmo_cxvec *burst_in, int sps, float freq_shift, int p, sbit_t *ebits, float *toa_p)
| All-in-one finding and demodulation of DKAB bursts. More...

## Detailed Description

## Function Documentation

## ◆ gmr1_dkab_demod()

int gmr1_dkab_demod | ( | struct osmo_cxvec * | burst_in,
|  | int | sps,
|  | float | freq_shift,
|  | int | p,
|  | sbit_t * | ebits,
|  | float * | toa_p
| ) |  |

All-in-one finding and demodulation of DKAB bursts.

Parameters

  [in] | burst_in | Complex signal of the burst
  [in] | sps | Oversampling used in the input complex signal
  [in] | freq_shift | Frequency shift to pre-apply to burst_in (rad/sym)
  [in] | p | DKAB position
  [out] | ebits | Encoded soft bits return array
  [out] | toa_p | Pointer to TOA return variable

Returns
  0 for success, 1 if DKAB not found, -errno for fatal errors

burst_in is expected to be longer than necessary. Any extra length will be used as 'search window' to find proper alignement. Good practice is to have a few samples too much in front and a few samples after the expected TOA.

References M_PIf, and osmo_cxvec_sig_normalize().