osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Functions | Variables
pi4cxpsk.c File Reference
GMR-1 Software Defined Radio library » pi2-CBPSK, pi4-CBPSK and pi4-CQPSK modulation

Osmocom GMR-1 pi2-CBPSK, pi4-CBPSK and pi4-CQPSK modulation support implementation. More...

`#include <complex.h>`
`#include <math.h>`
`#include <errno.h>`
`#include <stdint.h>`
`#include <stdlib.h>`
`#include <stdio.h>`
`#include <string.h>`
`#include <osmocom/core/bits.h>`
`#include <osmocom/dsp/cxvec.h>`
`#include <osmocom/dsp/cxvec_math.h>`
`#include <osmocom/gmr1/sdr/defs.h>`
`#include <osmocom/gmr1/sdr/pi4cxpsk.h>`

## Functions
int | gmr1_pi4cxpsk_demod (struct gmr1_pi4cxpsk_burst *burst_type, struct osmo_cxvec *burst_in, int sps, float freq_shift, sbit_t *ebits, int *sync_id_p, float *toa_p, float *freq_err_p)
| All-in-one pi4-CxPSK demodulation method. More...
int | gmr1_pi4cxpsk_detect (struct gmr1_pi4cxpsk_burst **burst_types, float e_toa, struct osmo_cxvec *burst_in, int sps, float freq_shift, int *bt_id_p, int *sync_id_p, float *toa_p)
| Try to identify burst type by matching training sequences. More...
int | gmr1_pi4cxpsk_mod_order (struct osmo_cxvec *burst_in, int sps, float freq_shift)
| Estimates modulation order by comparing power of x^2 vs x^4. More...
int | gmr1_pi4cxpsk_mod (struct gmr1_pi4cxpsk_burst *burst_type, ubit_t *ebits, int sync_id, struct osmo_cxvec *burst_out)
| Modulates (currently at 1 sps) More...

## Variables
struct gmr1_pi4cxpsk_modulation | gmr1_pi2cbpsk
| pi2-CBPSK modulation description More...
struct gmr1_pi4cxpsk_modulation | gmr1_pi4cbpsk
| pi4-CBPSK modulation description More...
struct gmr1_pi4cxpsk_modulation | gmr1_pi4cqpsk
| pi4-CQPSK modulation description More...

## Detailed Description

Osmocom GMR-1 pi2-CBPSK, pi4-CBPSK and pi4-CQPSK modulation support implementation.