osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Files | Macros | Functions
A5 ciphering algorithm
GMR-1 Layer 1 library

## Files
file | a5.h
| Osmocom GMR-1 A5 ciphering algorithm header.
file | a5.c
| Osmocom GMR-1 A5 ciphering algorithm implementation.

## Macros
#define | A51_R1_LEN 19
#define | A51_R2_LEN 22
#define | A51_R3_LEN 23
#define | A51_R4_LEN 17
#define | A51_R1_MASK ((1<<A51_R1_LEN)-1)
#define | A51_R2_MASK ((1<<A51_R2_LEN)-1)
#define | A51_R3_MASK ((1<<A51_R3_LEN)-1)
#define | A51_R4_MASK ((1<<A51_R4_LEN)-1)
#define | A51_R1_TAPS 0x072000 /* x^19 + x^18 + x^17 + x^14 + 1 */
#define | A51_R2_TAPS 0x311000 /* x^22 + x^21 + x^17 + x^13 + 1 */
#define | A51_R3_TAPS 0x660000 /* x^23 + x^22 + x^19 + x^18 + 1 */
#define | A51_R4_TAPS 0x013100 /* x^17 + x^14 + x^13 + x^9 + 1 */
#define | A51_BIT(r, n) (1 << n)

## Functions
void | gmr1_a5 (int n, uint8_t *key, uint32_t fn, int nbits, ubit_t *dl, ubit_t *ul)
| Main method to generate a A5/x cipher stream. More...
void | gmr1_a5_1 (uint8_t *key, uint32_t fn, int nbits, ubit_t *dl, ubit_t *ul)
| Generate a GMR-1 A5/1 cipher stream. More...

## Detailed Description

## Function Documentation

## ◆ gmr1_a5()

void gmr1_a5 | ( | int | n,
|  | uint8_t * | key,
|  | uint32_t | fn,
|  | int | nbits,
|  | ubit_t * | dl,
|  | ubit_t * | ul
| ) |  |

Main method to generate a A5/x cipher stream.

Parameters

  [in] | n | Which A5/x method to use
  [in] | key | 8 byte array for the key (as received from the SIM)
  [in] | fn | Frame number
  [in] | nbits | How many bits to generate
  [out] | dl | Pointer to array of ubits to return Downlink cipher stream
  [out] | ul | Pointer to array of ubits to return Uplink cipher stream

Currently only A5/0 and A5/1. Either (or both) of dl/ul can be NULL if not needed.

References gmr1_a5_1().

## ◆ gmr1_a5_1()

void gmr1_a5_1 | ( | uint8_t * | key,
|  | uint32_t | fn,
|  | int | nbits,
|  | ubit_t * | dl,
|  | ubit_t * | ul
| ) |  |

Generate a GMR-1 A5/1 cipher stream.

Parameters

  [in] | key | 8 byte array for the key (as received from the SIM)
  [in] | fn | Frame number
  [in] | nbits | How many bits to generate
  [out] | dl | Pointer to array of ubits to return Downlink cipher stream
  [out] | ul | Pointer to array of ubits to return Uplink cipher stream

Either (or both) of dl/ul can be NULL if not needed.

Referenced by gmr1_a5().