osmo-gmr 0.2.104-2b98 Osmocom GMR-1

Data Fields
gmr1_pi4cxpsk_burst Struct Reference
GMR-1 Software Defined Radio library » pi2-CBPSK, pi4-CBPSK and pi4-CQPSK modulation

pi4-CxPSK Burst format description More...

`#include <pi4cxpsk.h>`

## Data Fields
struct gmr1_pi4cxpsk_modulation * | mod
| Modulation scheme
int | guard_pre
| Beginning guard period.
int | guard_post
| End guard period
int | len
| Total len with guard.
int | ebits
| Number of encoded bits.
struct gmr1_pi4cxpsk_sync * | sync [GMR1_MAX_SYNC]
| Sync sequences.
struct gmr1_pi4cxpsk_data * | data
| Data chunks.

## Detailed Description

pi4-CxPSK Burst format description

The documentation for this struct was generated from the following file:

- include/osmocom/gmr1/sdr/pi4cxpsk.h